<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0.508" y1="14.224" x2="43.104" y2="14.224" width="0" layer="20"/>
<wire x1="43.104" y1="14.224" x2="43.104" y2="43.424" width="0" layer="20"/>
<wire x1="43.104" y1="43.424" x2="0.508" y2="43.424" width="0" layer="20"/>
<wire x1="0.508" y1="43.424" x2="0.508" y2="14.224" width="0" layer="20"/>
<text>Laser Receiver</text>
<text>FabLAB </text>
<text>Asturias</text>
<text>FabAcademy 2012</text>
</plain>
<libraries>
<library name="avr-7">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
</packages>
</library>
<library name="pinhead-2">
<packages>
<package name="2X03SMD">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 SMD</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="avr-7" package="SOIC14" value="TINY44"/>
<element name="C1" library="rcl" package="C0805K" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="M0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead-2" package="2X03SMD" value="ICSP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIP-LED0805" value="GREEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="M0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LDR" library="SparkFun" package="JST-2-SMD" value=""/>
<element name="R5" library="rcl" package="M0805" value="0"/>
<element name="R3" library="rcl" package="M0805" value="10K"/>
<element name="R4" library="rcl" package="M0805" value="1K"/>
<element name="T1" library="transistor" package="SOT23" value="BC846"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="14"/>
<contactref element="C1" pad="1"/>
<contactref element="JP2" pad="6"/>
<contactref element="R2" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="8"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="9"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="RST">
<contactref element="IC1" pad="4"/>
<contactref element="R1" pad="1"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="7"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="TX">
<contactref element="IC1" pad="13"/>
</signal>
<signal name="RX">
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="11"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="LED1" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R4" pad="2"/>
<contactref element="LDR" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="T1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="LDR" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="T1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
