PCBNEW-BOARD Version 1 date mar 29 may 2012 20:32:14 CEST

# Created by Pcbnew(2011-05-25)-stable

$GENERAL
encoding utf-8
LayerCount 2
Ly 1FFF8001
EnabledLayers 1FFF8001
Links 0
NoConn 0
Di 42915 25515 51651 33541
Ndraw 6
Ntrack 9
Nzone 0
BoardThickness 630
Nmodule 1
Nnets 2
$EndGENERAL

$SHEETDESCR
Sheet A4 11700 8267
Title ""
Date "29 may 2012"
Rev ""
Comp ""
Comment1 ""
Comment2 ""
Comment3 ""
Comment4 ""
$EndSHEETDESCR

$SETUP
InternalUnit 0.000100 INCH
Layers 2
Layer[0] Back signal
Layer[15] Front signal
TrackWidth 787
TrackClearence 100
ZoneClearence 200
TrackMinWidth 80
DrawSegmWidth 150
EdgeSegmWidth 150
ViaSize 350
ViaDrill 250
ViaMinSize 350
ViaMinDrill 200
MicroViaSize 200
MicroViaDrill 50
MicroViasAllowed 0
MicroViaMinSize 200
MicroViaMinDrill 50
TextPcbWidth 120
TextPcbSize 600 800
EdgeModWidth 150
TextModSize 600 600
TextModWidth 120
PadSize 600 600
PadDrill 320
Pad2MaskClearance 100
AuxiliaryAxisOrg 0 0
PcbPlotParams (pcbplotparams (layerselection 32768) (usegerberextensions true) (excludeedgelayer false) (linewidth 60) (plotframeref false) (viasonmask false) (mode 1) (useauxorigin false) (hpglpennumber 1) (hpglpenspeed 20) (hpglpendiameter 15) (hpglpenoverlay 2) (pscolor true) (psnegative false) (psa4output false) (plotreference true) (plotvalue true) (plotothertext true) (plotinvisibletext false) (padsonsilk false) (subtractmaskfromsilk false) (outputformat 2) (mirror false) (drillshape 1) (scaleselection 1) (outputdirectory ""))
$EndSETUP

$EQUIPOT
Na 0 ""
St ~
$EndEQUIPOT
$EQUIPOT
Na 1 "N-000161"
St ~
$EndEQUIPOT
$NCLASS
Name "Default"
Desc "This is the default net class."
Clearance 100
TrackWidth 787
ViaDia 350
ViaDrill 250
uViaDia 200
uViaDrill 50
AddNet ""
AddNet "N-000161"
$EndNCLASS
$MODULE PINTST
Po 47244 29528 0 15 3D649DF9 4FC51570 ~~
Li PINTST
Cd module 1 pin (ou trou mecanique de percage)
Kw DEV
Sc 4FC51570
AR 
Op 0 0 0
T0 0 -499 200 200 0 50 N V 21 N "PINTST"
T1 0 500 200 200 0 50 N I 21 N "Val*"
DC 0 0 -100 -300 50 21
$PAD
Sh "1" C 450 450 0 0 0
Dr 250 0 0
At STD N 00E0FFFF
Ne 1 "N-000161"
Po 0 0
$EndPAD
$SHAPE3D
Na "pin_array/pin_array_1x1.wrl"
Sc 1.000000 1.000000 1.000000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  PINTST
$TEXTPCB
Te "6.75"
Po 44094 30709 600 800 120 900
De 15 1 0 Normal
$EndTEXTPCB
$TEXTPCB
Te "5.85"
Po 50591 30709 600 800 120 900
De 15 1 0 Normal
$EndTEXTPCB
$DRAWSEGMENT
Po 0 43307 33465 43307 25591 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$DRAWSEGMENT
Po 0 51181 33465 43307 33465 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$DRAWSEGMENT
Po 0 51181 25591 51181 33465 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$DRAWSEGMENT
Po 0 43307 25591 51181 25591 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$TRACK
Po 0 46457 28740 48031 28740 787 -1
De 15 0 0 0 0
Po 0 50787 25984 48031 28740 787 -1
De 15 0 0 0 0
Po 0 44094 26378 44094 26377 787 -1
De 15 0 0 0 0
Po 0 46457 28740 44095 26378 787 -1
De 15 0 0 0 0
Po 0 44094 26378 44095 26378 787 -1
De 15 0 0 0 0
Po 0 44094 26377 43701 25984 787 -1
De 15 0 0 0 0
Po 0 46457 30315 48031 30315 787 -1
De 15 0 0 0 0
Po 0 43701 33071 46457 30315 787 -1
De 15 0 0 0 0
Po 0 48031 30315 50787 33071 787 -1
De 15 0 0 0 0
$EndTRACK
$ZONE
$EndZONE
$EndBOARD
