<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="-31" x2="115" y2="-31" width="0" layer="20"/>
<wire x1="115" y1="-31" x2="115" y2="56" width="0" layer="20"/>
<wire x1="115" y1="56" x2="0" y2="56" width="0" layer="20"/>
<wire x1="0" y1="56" x2="0" y2="-31" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="A3216-18">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="1X06-SMD-FEMALE-V2">
<description>Package for 4UCONN part #19686 *UNPROVEN*</description>
</package>
<package name="LED-1206">
</package>
<package name="1X04-SMD">
</package>
</packages>
</library>
<library name="01_attiny24_44_84">
<description>&lt;b&gt;Atmel ATtiny24/44/84: 8-bit AVR microcontroller with 2/4/8 kB in-system programmable flash&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="2X03SMD">
</package>
<package name="CSM-7X-DU">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;&lt;p&gt;
Source: www.ecsxtal.com .. Crystal 3.6864MHz CSM_7X_DU.PDF</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="01_ng" package="A3216-18" value="1 uf"/>
<element name="C2" library="01_SparkFun" package="0805" value="18 uf"/>
<element name="C3" library="01_SparkFun" package="0805" value="18 uf"/>
<element name="IC1" library="01_attiny24_44_84" package="SOIC14" value="ATTINY24/44/84-SSU"/>
<element name="R1" library="01_FAB_Hello" package="1206" value="10 k"/>
<element name="U$1" library="01_FAB_Hello" package="2X03SMD" value="AVRISPSMD"/>
<element name="Q1" library="01_FAB_Hello" package="CSM-7X-DU" value="CSM-7X-DU">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R4" library="01_FAB_Hello" package="1206" value="0 k"/>
<element name="JP2" library="01_SparkFun" package="1X06-SMD-FEMALE-V2" value=""/>
<element name="JP1" library="01_SparkFun" package="1X06-SMD-FEMALE-V2" value=""/>
<element name="JP3" library="01_SparkFun" package="1X06-SMD-FEMALE-V2" value=""/>
<element name="R2" library="01_FAB_Hello" package="1206" value="0 K"/>
<element name="LED2" library="01_SparkFun" package="LED-1206" value=""/>
<element name="R6" library="01_FAB_Hello" package="1206" value="499"/>
<element name="JP4" library="01_SparkFun" package="1X04-SMD" value=""/>
<element name="JP5" library="01_SparkFun" package="1X04-SMD" value=""/>
<element name="JP6" library="01_SparkFun" package="1X04-SMD" value=""/>
<element name="LED1" library="01_SparkFun" package="LED-1206" value=""/>
<element name="R3" library="01_FAB_Hello" package="1206" value="499"/>
<element name="LED3" library="01_SparkFun" package="LED-1206" value=""/>
<element name="R5" library="01_FAB_Hello" package="1206" value="499"/>
<element name="R7" library="01_FAB_Hello" package="1206" value="499"/>
<element name="R8" library="01_FAB_Hello" package="1206" value="499"/>
<element name="R9" library="01_FAB_Hello" package="1206" value="499"/>
<element name="LED4" library="01_SparkFun" package="LED-1206" value=""/>
<element name="LED5" library="01_SparkFun" package="LED-1206" value=""/>
<element name="LED6" library="01_SparkFun" package="LED-1206" value=""/>
<element name="R10" library="01_FAB_Hello" package="1206" value="0 K"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="-"/>
<contactref element="IC1" pad="14"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="JP2" pad="6"/>
<contactref element="R6" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="6"/>
<contactref element="LED3" pad="C"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="LED5" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED6" pad="C"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="JP2" pad="4"/>
<contactref element="C1" pad="+"/>
<contactref element="U$1" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="JP6" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="CTS">
<contactref element="JP2" pad="5"/>
</signal>
<signal name="RX">
<contactref element="IC1" pad="12"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="TX">
<contactref element="IC1" pad="13"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="DTR">
<contactref element="JP2" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="JP1" pad="6"/>
<contactref element="LED1" pad="A"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="3"/>
<contactref element="IC1" pad="9"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="RESET">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="R4" pad="1"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="4"/>
<contactref element="IC1" pad="7"/>
<contactref element="JP3" pad="6"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="C2">
<contactref element="Q1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="C1">
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="5"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="JP3" pad="5"/>
<contactref element="IC1" pad="6"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="3"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="N$1">
<contactref element="JP1" pad="4"/>
<contactref element="IC1" pad="10"/>
<contactref element="R9" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="JP3" pad="4"/>
<contactref element="IC1" pad="5"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="R6" pad="1"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="1"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="R5" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="R9" pad="2"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="LED4" pad="A"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="JP6" pad="3"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R8" pad="2"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="8"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="N$16">
</signal>
<signal name="N$17">
</signal>
</signals>
</board>
</drawing>
</eagle>
