<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="39.04" y2="0" width="0" layer="20"/>
<wire x1="39.04" y1="0" x2="39.04" y2="20.31" width="0" layer="20"/>
<wire x1="39.04" y1="20.31" x2="0" y2="20.31" width="0" layer="20"/>
<wire x1="0" y1="20.31" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab2">
<packages>
<package name="C1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab2" package="C1206FAB" value="CAP-UNPOLARIZEDFAB"/>
<element name="C2" library="fab2" package="C1206FAB" value="CAP-UNPOLARIZEDFAB"/>
<element name="JP1" library="fab2" package="2X03SMD" value=""/>
<element name="JP2" library="fab2" package="2X03SMD" value=""/>
<element name="U$1" library="fab2" package="SOIC8" value="A4953-H-BRIDGE-MOTOR-DRIVER"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="VREF">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="PA2">
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="PA3">
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="VBB">
<contactref element="U$1" pad="5"/>
<contactref element="JP1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="OUT1">
<contactref element="JP2" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="3"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="OUT2">
<contactref element="JP2" pad="5"/>
<contactref element="JP2" pad="6"/>
<contactref element="JP2" pad="4"/>
<contactref element="U$1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
