<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<text>O</text>
<text>C</text>
<wire x1="12" y1="29.6" x2="27.4" y2="28" width="0.254" layer="20" curve="-120.459701"/>
<wire x1="27.4" y1="28" x2="33.8" y2="27.8" width="0.254" layer="20" curve="-77.274958"/>
<wire x1="33.8" y1="27.8" x2="43.2" y2="23" width="0.254" layer="20" curve="-80.253892"/>
<wire x1="43.2" y1="23" x2="41.6" y2="12.8" width="0.254" layer="20" curve="-226.539838"/>
<wire x1="41.6" y1="12.8" x2="28.4" y2="5.6" width="0.254" layer="20" curve="-99.602333"/>
<wire x1="28.4" y1="5.6" x2="17.2" y2="8" width="0.254" layer="20" curve="-69.862263"/>
<wire x1="17.2" y1="8" x2="7" y2="19" width="0.254" layer="20" curve="-124.308407"/>
<wire x1="7" y1="19" x2="12" y2="29.6" width="0.254" layer="20" curve="-115.921607"/>
</plain>
<libraries>
<library name="00fab">
<packages>
<package name="2X03SMD">
</package>
<package name="R1206FAB">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="C1206FAB">
</package>
<package name="1X06SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="00fab" package="R1206FAB" value="10k"/>
<element name="R2" library="00fab" package="R1206FAB" value="10k"/>
<element name="R3" library="00fab" package="R1206FAB" value="10k"/>
<element name="R4" library="00fab" package="R1206FAB" value="10k"/>
<element name="R5" library="00fab" package="R1206FAB" value="10k"/>
<element name="ISPHEADER" library="00fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$2" library="00fab" package="SOIC8" value="ATTINY45SI"/>
<element name="CAP1UF" library="00fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="FTDIHEADER" library="00fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="4"/>
<contactref element="ISPHEADER" pad="6"/>
<contactref element="FTDIHEADER" pad="1"/>
<contactref element="CAP1UF" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="PB2">
<contactref element="U$2" pad="7"/>
<contactref element="ISPHEADER" pad="3"/>
<contactref element="FTDIHEADER" pad="5"/>
</signal>
<signal name="PB1">
<contactref element="U$2" pad="6"/>
<contactref element="ISPHEADER" pad="1"/>
</signal>
<signal name="PB0">
<contactref element="U$2" pad="5"/>
<contactref element="ISPHEADER" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="ISPHEADER" pad="2"/>
<contactref element="U$2" pad="8"/>
<contactref element="CAP1UF" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="FTDIHEADER" pad="3"/>
</signal>
<signal name="RST">
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="1"/>
<contactref element="ISPHEADER" pad="5"/>
</signal>
<signal name="PB4">
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="PB3">
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="U$2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
