(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 24)
    (no_connects 0)
    (area 140.640999 108.636999 197.052001 133.933001)
    (thickness 1.6)
    (drawings 8)
    (tracks 71)
    (zones 0)
    (modules 10)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /RST)
  (net 3 /MOSI)
  (net 4 /RX)
  (net 5 /VCC)
  (net 6 /MISO)
  (net 7 "Net-(M1-Pad2)")
  (net 8 /CTS)
  (net 9 /TX)
  (net 10 /RTS)
  (net 11 /SENSE)
  (net 12 "Net-(R2-Pad1)")
  (net 13 "Net-(U1-PadA)")
  (net 14 "Net-(U1-PadB)")
  (net 15 "Net-(U1-PadE)")
  (net 16 "Net-(U1-PadH)")
  (net 17 "Net-(U1-PadJ)")
  (net 18 "Net-(U1-PadK)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CTS)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RST)
    (add_net /RTS)
    (add_net /RX)
    (add_net /SENSE)
    (add_net /TX)
    (add_net /VCC)
    (add_net GND)
    (add_net "Net-(M1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(U1-PadA)")
    (add_net "Net-(U1-PadB)")
    (add_net "Net-(U1-PadE)")
    (add_net "Net-(U1-PadH)")
    (add_net "Net-(U1-PadJ)")
    (add_net "Net-(U1-PadK)")
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 166.37 122.682)
    (attr smd)
    (fp_text reference JP1 (at -0.635 -4.445) (layer B.SilkS))
    (fp_text value PINHD-2X3-SMD (at 0 4.445) (layer B.SilkS))
    (pad 1 smd rect (at -2.54 -2.54) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.91846 -2.54) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 /RST))
    (pad 3 smd rect (at -2.54 0) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 /MOSI))
    (pad 4 smd rect (at 2.91846 0) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 /RX))
    (pad 5 smd rect (at -2.54 2.54) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 /VCC))
    (pad 6 smd rect (at 2.91846 2.54) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 /MISO))
  )
  (module fab:fab-1X06SMD (layer F.Cu) (tedit 58170E85)
    (at 192.913 122.682)
    (attr smd)
    (fp_text reference M2 (at -2.54 0 90) (layer B.SilkS))
    (fp_text value FTDI-SMD-HEADER (at 2.667 -0.127 90) (layer F.SilkS))
    (pad 1 smd rect (at 0 -6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 /CTS))
    (pad 3 smd rect (at 0 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 /VCC))
    (pad 4 smd rect (at 0 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 /TX))
    (pad 5 smd rect (at 0 3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 /RX))
    (pad 6 smd rect (at 0 6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 /RTS))
  )
  (module Housings_SOIC:SOIJ-8_5.3x5.3mm_Pitch1.27mm (layer F.Cu) (tedit 58170ECD)
    (at 176.911 122.809 270)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference M1 (at -0.254 0 270) (layer F.SilkS))
    (fp_text value ATTINY45SI (at 0 3.68 270) (layer F.Fab))
    (pad 1 smd rect (at -3.65 -1.905 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 /RST))
    (pad 2 smd rect (at -3.65 -0.635 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(M1-Pad2)"))
    (pad 3 smd rect (at -3.65 0.635 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 /SENSE))
    (pad 4 smd rect (at -3.65 1.905 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 3.65 1.905 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 /MOSI))
    (pad 6 smd rect (at 3.65 0.635 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 /MISO))
    (pad 7 smd rect (at 3.65 -0.635 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /RX))
    (pad 8 smd rect (at 3.65 -1.905 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /VCC))
    (model Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58170EB1)
    (at 186.69 122.809 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0.127 0 90) (layer F.SilkS))
    (fp_text value 1u (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58170EAF)
    (at 183.007 122.809 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -0.127 270) (layer F.SilkS))
    (fp_text value 10k (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /RST))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58170EB7)
    (at 157.353 122.301 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -0.127 0 90) (layer F.SilkS))
    (fp_text value 82 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58170EB9)
    (at 153.416 115.443 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0.127 -0.127 180) (layer F.SilkS))
    (fp_text value 1k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /SENSE))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sensors_SMD:MICS-2614 (layer F.Cu) (tedit 58170EA2)
    (at 150.114 123.317 270)
    (fp_text reference U1 (at -3.462 -3.77 270) (layer F.SilkS))
    (fp_text value MICS-2614 (at 3.683 -0.508 270) (layer F.SilkS))
    (pad A smd rect (at 1.25 -2.5 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-PadA)"))
    (pad B smd rect (at 0 -2.5 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-PadB)"))
    (pad C smd rect (at -1.25 -2.5 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R2-Pad1)"))
    (pad D smd rect (at -3.5 -1.27) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 11 /SENSE))
    (pad E smd rect (at -3.5 1.27) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-PadE)"))
    (pad F smd rect (at -1.25 2.5 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 5 /VCC))
    (pad G smd rect (at 0 2.5 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 5 /VCC))
    (pad H smd rect (at 1.25 2.5 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-PadH)"))
    (pad J smd rect (at 3.5 1.27) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-PadJ)"))
    (pad K smd rect (at 3.5 -1.27) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-PadK)"))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 144.907 116.84 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 1u (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 176.149 115.062)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 0 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 140.716 108.712) (end 143.383 108.712) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.716 108.839) (end 140.716 108.712) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.716 133.858) (end 140.716 108.839) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.002 133.858) (end 140.716 133.858) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 196.977 108.712) (end 196.977 133.604) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 196.977 133.858) (end 196.977 133.477) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.002 108.712) (end 196.977 108.712) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.002 133.858) (end 196.977 133.858) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.716 133.731) (xy 140.716 108.712) (xy 196.977 108.712) (xy 196.977 133.858) (xy 140.716 133.858)
      )
    )
  )
)
