<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<library>
<packages>
<package name="PIN6SDL">
</package>
<package name="4SINGLE">
</package>
<package name="4SINGLE_SPLIT">
</package>
<package name="FC_LED_HOLE">
</package>
</packages>
<symbols>
<symbol name="3PD_CCOM">
<pin name="ARED" direction="in"/>
<pin name="AGREEN"/>
<pin name="ABLUE"/>
<pin name="KCOM"/>
</symbol>
<symbol name="3LED_KCOM">
<pin name="A_RED"/>
<pin name="A_GREEN"/>
<pin name="A_BLUE"/>
<pin name="K_COM"/>
</symbol>
<symbol name="3LED_KCOMM">
<pin name="AR"/>
<pin name="AG"/>
<pin name="AB"/>
<pin name="K"/>
</symbol>
<symbol name="FCOL_LED">
<pin name="P$1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RGBSENSOR" prefix="PD">
<description>Photo Diode Array for RGB Sensing.
Hamamatsu S9032-02
https://www.hamamatsu.com/resources/pdf/ssd/s9032-02_kspd1067e.pdf
The S9032-02 is a color sensor molded into a plastic package having a 3-channel (RGB) photodiode sensitive to the blue (λp=460 nm), green (λp=540 nm) and red (λp=620 nm) regions of the spectrum. The S9032-02 has a 3-segment (RGB) circular photosensi-
tive area of 2mm-phi.
R=0.16A/W, G=0.23A/W, B=0.18A/W.</description>
<gates>
<gate name="G$1" symbol="3PD_CCOM"/>
</gates>
<devices>
<device name="" package="PIN6SDL">
<connects>
<connect gate="G$1" pin="ABLUE" pad="P$6"/>
<connect gate="G$1" pin="AGREEN" pad="P$3"/>
<connect gate="G$1" pin="ARED" pad="P$1"/>
<connect gate="G$1" pin="KCOM" pad="P$2 P$5"/>
</connects>
<technologies>
<technology name="S9032-02">
<attribute name="PRODUCER" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STA5131A">
<gates>
<gate name="G$1" symbol="3LED_KCOMM"/>
</gates>
<devices>
<device name="" package="4SINGLE">
<connects>
<connect gate="G$1" pin="AB" pad="P$3"/>
<connect gate="G$1" pin="AG" pad="P$2"/>
<connect gate="G$1" pin="AR" pad="P$5"/>
<connect gate="G$1" pin="K" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="4SINGLE_SPLIT">
<connects>
<connect gate="G$1" pin="AB" pad="P$2"/>
<connect gate="G$1" pin="AG" pad="P$1"/>
<connect gate="G$1" pin="AR" pad="P$4"/>
<connect gate="G$1" pin="K" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NEW_DEV">
<gates>
<gate name="G$1" symbol="3LED_KCOM"/>
</gates>
<devices>
<device name="" package="FC_LED_HOLE">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
