<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="97.46" y2="-1.27" width="0" layer="20"/>
<wire x1="97.46" y1="-1.27" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="E14_Arduino_revB">
<packages>
<package name="ARDUINO_UNO">
<description>Footprint for representing an Arduino Uno board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="2X05SMD">
</package>
<package name="2X02SMD">
</package>
<package name="JACK_.65MM">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD2,54-5,08">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor 223&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 318E-04&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM137M-D.PDF</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PCB1" library="E14_Arduino_revB" package="ARDUINO_UNO" value="ARDUINO_UNO"/>
<element name="U$1" library="fab" package="2X05SMD" value="PINHD-2X5-SMD"/>
<element name="U$3" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="PAD1" library="wirepad" package="SMD2,54-5,08" value=""/>
<element name="IC2" library="v-reg" package="SOT223" value="LD117AS12TR"/>
<element name="U$2" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="J2" library="fab" package="JACK_.65MM" value="JACK.65MM"/>
<element name="IC1" library="v-reg" package="SOT223" value="LD117AS12TR"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="PCB1" pad="5V"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$2" pad="4"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="CS">
<contactref element="U$1" pad="1"/>
<contactref element="PCB1" pad="12"/>
</signal>
<signal name="NC">
<contactref element="U$1" pad="3"/>
</signal>
<signal name="WR">
<contactref element="U$1" pad="5"/>
<contactref element="PCB1" pad="10"/>
</signal>
<signal name="DATA">
<contactref element="U$1" pad="7"/>
<contactref element="PCB1" pad="9"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="9"/>
</signal>
<signal name="CLK">
<contactref element="U$1" pad="2"/>
<contactref element="PCB1" pad="13"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="10"/>
</signal>
<signal name="GND">
<contactref element="U$3" pad="2"/>
<contactref element="U$3" pad="3"/>
<contactref element="U$1" pad="8"/>
<contactref element="PCB1" pad="GND"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$2" pad="2"/>
<contactref element="J2" pad="SHUNT"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="PIN2">
<contactref element="U$3" pad="4"/>
<contactref element="PCB1" pad="2"/>
</signal>
<signal name="12V">
<contactref element="U$3" pad="1"/>
<contactref element="J2" pad="PIN"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="CS2">
<contactref element="PAD1" pad="1"/>
<contactref element="PCB1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
