<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="-2.667" y1="-2.159" x2="59.4616" y2="-2.032" width="0" layer="20"/>
<wire x1="59.4616" y1="-2.032" x2="59.3092" y2="62.601" width="0" layer="20"/>
<wire x1="59.3092" y1="62.601" x2="-2.8702" y2="62.4486" width="0" layer="20"/>
<wire x1="-2.8702" y1="62.4486" x2="-2.667" y2="-2.159" width="0" layer="20"/>
<text>G</text>
<text>V</text>
<text>G</text>
<text>V</text>
<text>DISTANCE SENSOR 
MASTER</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ng">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="atmega8">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="1X06-SMD">
</package>
</packages>
</library>
<library name="wirepad">
<packages>
<package name="2,54/0,9">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="EFOBM">
</package>
</packages>
</library>
<library name="00_fab">
<packages>
<package name="2X02SMD">
</package>
<package name="2X03SMD">
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
<library name="00_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_LOCK_LONGPADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rcl" package="C1206" value=".1uf"/>
<element name="C2" library="ng" package="1206" value="1uf"/>
<element name="C3" library="ng" package="1206" value=".1uf"/>
<element name="C4" library="ng" package="1206" value="10uf"/>
<element name="IC1" library="atmega8" package="TQFP32-08" value="ATMEGA48/88/168-AU"/>
<element name="JP1" library="SparkFun" package="1X06-SMD" value=""/>
<element name="LED" library="ng" package="1206" value=""/>
<element name="PAD2" library="wirepad" package="2,54/0,9" value="WIREPAD2,54/0,9"/>
<element name="R1" library="ng" package="1206" value="10k"/>
<element name="R2" library="ng" package="1206" value="499"/>
<element name="S1" library="ng" package="6MM_SWITCH" value=""/>
<element name="U$2" library="fab" package="EFOBM" value="RESONATOREFOB">
<attribute name="VARIANT" value=""/>
</element>
<element name="U$1" library="00_fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="JP2" library="00_fab" package="2X03SMD" value=""/>
<element name="R3" library="00_fab" package="R1206FAB" value="10k"/>
<element name="R4" library="00_fab" package="R1206FAB" value="10k"/>
<element name="R5" library="00_fab" package="R1206FAB" value="0"/>
<element name="R6" library="00_fab" package="R1206FAB" value="0"/>
<element name="R7" library="00_fab" package="R1206FAB" value="0"/>
<element name="R8" library="00_fab" package="R1206FAB" value="value"/>
<element name="R9" library="00_fab" package="R1206FAB" value="value"/>
<element name="R10" library="00_fab" package="R1206FAB" value="value"/>
<element name="R11" library="00_fab" package="R1206FAB" value="value"/>
<element name="R12" library="00_fab" package="R1206FAB" value="value"/>
<element name="R13" library="00_fab" package="R1206FAB" value="value"/>
<element name="R14" library="00_fab" package="R1206FAB" value="value"/>
<element name="R15" library="00_fab" package="R1206FAB" value="value"/>
<element name="JP3" library="00_SparkFun" package="1X08_LOCK_LONGPADS" value=""/>
<element name="JP4" library="00_SparkFun" package="1X08_LOCK_LONGPADS" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="5"/>
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="IC1" pad="21"/>
<contactref element="IC1" pad="3"/>
<contactref element="LED" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="JP2" pad="5"/>
<contactref element="R7" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="JP3" pad="8"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP4" pad="8"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="R1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="JP3" pad="5"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="5"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="RST">
<contactref element="IC1" pad="29"/>
<contactref element="R1" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="PAD2" pad="1"/>
<contactref element="JP2" pad="6"/>
<contactref element="R5" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="ENT_R11">
<contactref element="IC1" pad="12"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="ENT_R12">
<contactref element="IC1" pad="13"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="ENT_R13">
<contactref element="IC1" pad="14"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="15"/>
<contactref element="JP2" pad="3"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="16"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="17"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$23">
<contactref element="R2" pad="2"/>
<contactref element="LED" pad="1"/>
</signal>
<signal name="DTR">
<contactref element="JP1" pad="6"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="TX">
<contactref element="JP1" pad="5"/>
<contactref element="IC1" pad="31"/>
</signal>
<signal name="RX">
<contactref element="JP1" pad="4"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="8"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="7"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="ENT_R9">
<contactref element="IC1" pad="10"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="ENT_R10">
<contactref element="IC1" pad="11"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="4"/>
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="ENT_R8">
<contactref element="IC1" pad="9"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="EX_R8">
<contactref element="R8" pad="2"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="EX_R9">
<contactref element="R9" pad="2"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="EX_R10">
<contactref element="R10" pad="2"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="EX_R11">
<contactref element="R11" pad="2"/>
<contactref element="JP4" pad="7"/>
</signal>
<signal name="EX_R12">
<contactref element="R12" pad="2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="EX_R13">
<contactref element="R13" pad="2"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="ENT_R15">
<contactref element="R15" pad="1"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="EX_R14">
<contactref element="R14" pad="2"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="EX_R15">
<contactref element="R15" pad="2"/>
<contactref element="JP3" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
