<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="12.192" y1="20.32" x2="44.628" y2="20.32" width="0" layer="20"/>
<wire x1="44.628" y1="20.32" x2="44.628" y2="49.012" width="0" layer="20"/>
<wire x1="44.628" y1="49.012" x2="12.192" y2="49.012" width="0" layer="20"/>
<wire x1="12.192" y1="49.012" x2="12.192" y2="20.32" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
<package name="2X02SMD">
</package>
</packages>
</library>
<library name="Adaftuit_digitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LGA-12">
<description>&lt;h3&gt;LGA-12 2x2x1 mm 12-lead&lt;/h3&gt;
&lt;ul&gt;&lt;li&gt;0.50mm pitch&lt;/li&gt;
&lt;li&gt;Pads are 0.25x0.275 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;h4&gt;Derrived from the following ST PDFs&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00089896.pdf&lt;/li&gt;
&lt;li&gt;http://www.st.com/web/en/resource/technical/document/technical_note/CD00134799.pdf&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="100n"/>
<element name="C3" library="fab" package="C1206FAB" value="100n"/>
<element name="C4" library="fab" package="C1206FAB" value="10u"/>
<element name="C6" library="fab" package="C1206FAB" value="100n"/>
<element name="R1" library="fab" package="R1206FAB" value="4.7k"/>
<element name="R2" library="fab" package="R1206FAB" value="4.7k"/>
<element name="R3" library="fab" package="R1206FAB" value="10k"/>
<element name="R4" library="fab" package="R1206FAB" value="10k"/>
<element name="U1" library="Adaftuit_digitalIC" package="LGA-12" value="LSM303C"/>
<element name="U$1" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="R5" library="fab" package="R1206FAB" value=""/>
<element name="R6" library="fab" package="R1206FAB" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="8"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="C6" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="5"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="2"/>
<contactref element="U1" pad="10"/>
<contactref element="C6" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="9"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="4"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R5" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
