<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="21.6" y2="0" width="0" layer="20"/>
<wire x1="21.6" y1="0" x2="21.6" y2="23.2" width="0" layer="20"/>
<wire x1="21.6" y1="23.2" x2="0" y2="23.2" width="0" layer="20"/>
<wire x1="0" y1="23.2" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
<library name="semicon-smd-ipc">
<description>&lt;b&gt;IPC Standard SMD Semiconductors&lt;/b&gt;&lt;p&gt;
A few devices defined according to the IPC standard.&lt;p&gt;
Based on:&lt;p&gt;
IPC-SM-782&lt;br&gt;
IRevision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT89">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X05-3.5MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="fab" package="SOD123" value="1N4001"/>
<element name="PN2222" library="semicon-smd-ipc" package="SOT89" value=""/>
<element name="R1" library="fab" package="R1206FAB" value="270 Ohm"/>
<element name="J1" library="adafruit" package="1X05-3.5MM" value="1X5"/>
</elements>
<signals>
<signal name="PD5">
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="PN2222" pad="1"/>
</signal>
<signal name="GND">
<contactref element="PN2222" pad="3"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="3"/>
<contactref element="D1" pad="CATHODE"/>
</signal>
<signal name="N$3">
<contactref element="PN2222" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="D1" pad="ANODE"/>
</signal>
<signal name="N$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
