<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="2.5" y1="2" x2="32" y2="2" width="0" layer="20"/>
<wire x1="32" y1="2" x2="32" y2="28.5" width="0" layer="20"/>
<wire x1="32" y1="28.5" x2="2.5" y2="28.5" width="0" layer="20"/>
<wire x1="2.5" y1="28.5" x2="2.5" y2="2" width="0" layer="20"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X4-SMT">
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CN1" library="adafruit" package="1X4-SMT" value="1X4SMT"/>
<element name="CN2" library="adafruit" package="1X4-SMT" value="1X4SMT"/>
<element name="U$2" library="fab" package="SOIC8" value="ATTINY45SI"/>
<element name="U$1" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="C1" library="fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="10K" library="fab" package="R1206FAB" value=""/>
</elements>
<signals>
<signal name="INPUT">
<contactref element="U$2" pad="2"/>
<contactref element="CN1" pad="3"/>
<contactref element="10K" pad="2"/>
</signal>
<signal name="OUTPUT">
<contactref element="U$2" pad="3"/>
<contactref element="CN2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="4"/>
<contactref element="CN1" pad="4"/>
<contactref element="CN2" pad="4"/>
<contactref element="U$1" pad="6"/>
<contactref element="C1" pad="2"/>
<contactref element="10K" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="6"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="U$2" pad="1"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="8"/>
<contactref element="CN1" pad="2"/>
<contactref element="CN1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U$2" pad="7"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="4"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
