<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0.1097" y1="12.10828125" x2="100.261190625" y2="12.209409375" width="0" layer="20"/>
<wire x1="100.261190625" y1="12.209409375" x2="100.158696875" y2="50.131446875" width="0" layer="20"/>
<wire x1="100.158696875" y1="50.131446875" x2="0.158696875" y2="50.131446875" width="0" layer="20"/>
<wire x1="0.158696875" y1="50.131446875" x2="0.1097" y2="12.10828125" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="TQFP32-08THIN">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="R1206FAB">
</package>
<package name="EFOBM">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="2X03SMD">
</package>
<package name="SPDTSWITCH">
</package>
<package name="SJFAB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="fab" package="TQFP32-08THIN" value="ATMEGA88-THIN"/>
<element name="IC2" library="fab" package="SOT23" value=""/>
<element name="R10" library="fab" package="R1206FAB" value=""/>
<element name="R11" library="fab" package="R1206FAB" value=""/>
<element name="R12" library="fab" package="R1206FAB" value=""/>
<element name="R13" library="fab" package="R1206FAB" value=""/>
<element name="R14" library="fab" package="R1206FAB" value=""/>
<element name="R15" library="fab" package="R1206FAB" value=""/>
<element name="R16" library="fab" package="R1206FAB" value=""/>
<element name="R17" library="fab" package="R1206FAB" value=""/>
<element name="R18" library="fab" package="R1206FAB" value=""/>
<element name="R3" library="fab" package="R1206FAB" value=""/>
<element name="R4" library="fab" package="R1206FAB" value=""/>
<element name="R5" library="fab" package="R1206FAB" value=""/>
<element name="R6" library="fab" package="R1206FAB" value=""/>
<element name="R7" library="fab" package="R1206FAB" value=""/>
<element name="R8" library="fab" package="R1206FAB" value=""/>
<element name="R9" library="fab" package="R1206FAB" value=""/>
<element name="U$1" library="fab" package="EFOBM" value="RESONATOR"/>
<element name="U$10" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$11" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$12" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$13" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$14" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$15" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$16" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$17" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$18" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$19" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$2" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$20" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$3" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$4" library="fab" package="SPDTSWITCH" value="SPDTSWITCH"/>
<element name="U$5" library="fab" package="SJFAB" value="SOLDER_JUMPER"/>
<element name="U$6" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$7" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$8" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$9" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="21"/>
<contactref element="U$1" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="U$5" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="U$2" pad="6"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC2" pad="1"/>
<contactref element="U$4" pad="3"/>
<contactref element="U$2" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="AVCC">
<contactref element="IC1" pad="18"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="3"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="15"/>
<contactref element="U$11" pad="1"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="U$2" pad="3"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="N$9">
<contactref element="U$2" pad="5"/>
<contactref element="IC1" pad="29"/>
</signal>
<signal name="N$3">
<contactref element="U$5" pad="2"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="INT">
<contactref element="U$4" pad="2"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="11"/>
<contactref element="U$19" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="10"/>
<contactref element="U$18" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="9"/>
<contactref element="U$17" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="2"/>
<contactref element="U$16" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="1"/>
<contactref element="U$15" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="32"/>
<contactref element="U$14" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="IC1" pad="31"/>
<contactref element="U$13" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="IC1" pad="30"/>
<contactref element="U$12" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="25"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="26"/>
<contactref element="U$7" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="12"/>
<contactref element="U$8" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="13"/>
<contactref element="U$9" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="IC1" pad="14"/>
<contactref element="U$10" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="24"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="23"/>
<contactref element="U$20" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="U$20" pad="2"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="R3" pad="1"/>
<contactref element="U$6" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="U$3" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="U$7" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="U$8" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="U$9" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="U$10" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="U$11" pad="2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="U$12" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="U$13" pad="2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="U$14" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="U$15" pad="2"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="U$16" pad="2"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="U$17" pad="2"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="U$18" pad="2"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="U$19" pad="2"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="16"/>
<contactref element="U$2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
