<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="44.81" y1="37.12" x2="17.74" y2="37.12" width="0.4064" layer="20"/>
<wire x1="17.74" y1="37.12" x2="15.2" y2="34.58" width="0.4064" layer="20" curve="90"/>
<wire x1="15.2" y1="34.58" x2="15.2" y2="7.58" width="0.4064" layer="20"/>
<wire x1="15.2" y1="7.58" x2="18.24" y2="4.54" width="0.4064" layer="20" curve="90"/>
<wire x1="18.24" y1="4.54" x2="45.31" y2="4.54" width="0.4064" layer="20"/>
<wire x1="45.31" y1="4.54" x2="47.85" y2="7.58" width="0.4064" layer="20" curve="90"/>
<wire x1="47.85" y1="7.58" x2="47.85" y2="34.58" width="0.4064" layer="20"/>
<wire x1="47.85" y1="34.58" x2="44.81" y2="37.12" width="0.4064" layer="20" curve="90"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
<library name="murata-filter">
<description>&lt;b&gt;Murata Filters&lt;/b&gt;&lt;p&gt;
Distributor RS Components&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CSTCR6M">
<description>Source: http://search.murata.co.jp/Ceramy/CatalogshowpageAction.do?sDirnm=A07X&amp;sFilnm=81G07006&amp;sType=2&amp;sLang=en&amp;sNHinnm=CSTCR6M00G53Z-R0&amp;sCapt=Standard_Land_Pattern_Dimensions</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="fab" package="SOIC14" value="ATTINY44-SSU"/>
<element name="Q1" library="murata-filter" package="CSTCR6M" value="CSTCR6M00G53Z">
<attribute name="OC_NEWARK" value="25M8759"/>
<attribute name="MPN" value="CSTCR6M00G53-R0"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1170434"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="adafruit" package="1X06" value=""/>
<element name="JP2" library="adafruit" package="1X06" value=""/>
<element name="R1" library="adafruit" package="R1206" value="100"/>
<element name="R2" library="adafruit" package="R1206" value="10K"/>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE_SWITCH_SMD" value="">
<attribute name="PROD_ID" value="SWCH-08247"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_1206" value=""/>
<element name="R3" library="adafruit" package="R1206" value="10K"/>
<element name="R4" library="adafruit" package="R1206" value="0"/>
<element name="R5" library="adafruit" package="R1206" value="0"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP2" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="14"/>
<contactref element="Q1" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="R5" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="7"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="9"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="8"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="XTAL1">
<contactref element="IC1" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="XTAL2">
<contactref element="IC1" pad="3"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="RX">
<contactref element="IC1" pad="13"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="TX">
<contactref element="IC1" pad="12"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="CTS">
<contactref element="JP1" pad="2"/>
</signal>
<signal name="RTS">
<contactref element="JP1" pad="6"/>
</signal>
<signal name="RST">
<contactref element="JP2" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="BUTTON">
<contactref element="S1" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="S1" pad="4"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="LED">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
