<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="51.7" y2="0" width="0" layer="20"/>
<wire x1="51.7" y1="0" x2="51.7" y2="43.4" width="0" layer="20"/>
<wire x1="51.7" y1="43.4" x2="0" y2="43.4" width="0" layer="20"/>
<wire x1="0" y1="43.4" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="2X05SMD">
</package>
<package name="C1206FAB">
</package>
<package name="1X06SMD">
</package>
<package name="2X03SMD">
</package>
<package name="R1206FAB">
</package>
<package name="EFOBM">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BLUETOOTH" library="fab" package="2X05SMD" value="PINHD-2X5-SMD"/>
<element name="C1" library="fab" package="C1206FAB" value="10uF"/>
<element name="C2" library="fab" package="C1206FAB" value="1uF"/>
<element name="C3" library="fab" package="C1206FAB" value="1uF"/>
<element name="FTDI" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="PROGRAMMING" library="fab" package="2X03SMD" value=""/>
<element name="R1" library="fab" package="R1206FAB" value="10k"/>
<element name="R2" library="fab" package="R1206FAB" value="1k"/>
<element name="R3" library="fab" package="R1206FAB" value="2k"/>
<element name="U$3" library="fab" package="EFOBM" value="RESONATOR 16MHz"/>
<element name="STEPPEROUT" library="fab" package="2X05SMD" value="PINHD-2X5-SMD"/>
<element name="HYPPY" library="fab" package="R1206FAB" value=""/>
<element name="U1" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P">
<attribute name="PROD_ID" value="IC-09069"/>
</element>
<element name="HYPPY2" library="fab" package="R1206FAB" value=""/>
</elements>
<signals>
<signal name="N$4">
<contactref element="U$3" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="PROGRAMMING" pad="5"/>
<contactref element="BLUETOOTH" pad="8"/>
<contactref element="STEPPEROUT" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="PROGRAMMING" pad="2"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="N$2">
<contactref element="U$3" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="U$3" pad="3"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="GND">
<contactref element="FTDI" pad="1"/>
<contactref element="BLUETOOTH" pad="6"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="PROGRAMMING" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="STEPPEROUT" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="N$5">
<contactref element="FTDI" pad="5"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="31"/>
</signal>
<signal name="N$7">
<contactref element="BLUETOOTH" pad="4"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="N$8">
<contactref element="PROGRAMMING" pad="4"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="N$9">
<contactref element="PROGRAMMING" pad="6"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="N$11">
<contactref element="PROGRAMMING" pad="3"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$10">
<contactref element="STEPPEROUT" pad="4"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="N$12">
<contactref element="STEPPEROUT" pad="6"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="N$13">
<contactref element="STEPPEROUT" pad="5"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="N$14">
<contactref element="STEPPEROUT" pad="3"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="N$16">
<contactref element="STEPPEROUT" pad="7"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="N$17">
<contactref element="STEPPEROUT" pad="8"/>
<contactref element="HYPPY" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="HYPPY" pad="1"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="N$19">
</signal>
<signal name="N$20">
</signal>
<signal name="N$6">
<contactref element="BLUETOOTH" pad="2"/>
<contactref element="HYPPY2" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="HYPPY2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
