<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.1">
<drawing>
<board>
<plain>
<wire x1="-3.664" y1="-6.16" x2="49.424" y2="-6.064" width="0" layer="20"/>
<wire x1="49.424" y1="-6.064" x2="49.36" y2="24.336" width="0" layer="20"/>
<wire x1="49.36" y1="24.336" x2="-3.664" y2="24.192" width="0" layer="20"/>
<wire x1="-3.664" y1="24.192" x2="-3.664" y2="-6.16" width="0" layer="20"/>
<text>D1B SLV TX</text>
<text>EQB
2017</text>
</plain>
<libraries>
<library name="00fab">
<packages>
<package name="C1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="00fab" package="C1206FAB" value="1uF"/>
<element name="JP1" library="00fab" package="2X03SMD" value=""/>
<element name="R1" library="00fab" package="R1206FAB" value="10k"/>
<element name="U2" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="Tiny85-20-SMT">
<attribute name="PROD_ID" value="IC-09092"/>
</element>
<element name="LED2" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="R2" library="00fab" package="R1206FAB" value="220ohm"/>
<element name="R3" library="00fab" package="R1206FAB" value="220ohm"/>
<element name="LED1" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="FROM_MASTER" library="pinhead" package="1X04" value=""/>
<element name="TX433MHZ" library="pinhead" package="1X03" value=""/>
<element name="R4" library="00fab" package="R1206FAB" value="0ohm"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U2" pad="8"/>
<contactref element="JP1" pad="5"/>
<contactref element="R3" pad="2"/>
<contactref element="FROM_MASTER" pad="1"/>
<contactref element="TX433MHZ" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U2" pad="4"/>
<contactref element="C2" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="LED2" pad="2"/>
<contactref element="LED1" pad="2"/>
<contactref element="FROM_MASTER" pad="4"/>
<contactref element="TX433MHZ" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U2" pad="5"/>
<contactref element="JP1" pad="3"/>
<contactref element="FROM_MASTER" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="U2" pad="6"/>
<contactref element="JP1" pad="6"/>
<contactref element="TX433MHZ" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="U2" pad="7"/>
<contactref element="JP1" pad="4"/>
<contactref element="FROM_MASTER" pad="2"/>
</signal>
<signal name="RST">
<contactref element="U2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="1"/>
</signal>
<signal name="PB4">
<contactref element="U2" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="PB3">
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="1"/>
<contactref element="LED1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
