<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
<wire x1="55.88" y1="22.86" x2="93.96" y2="22.86" width="0" layer="20"/>
<wire x1="93.96" y1="22.86" x2="93.96" y2="64.44" width="0" layer="20"/>
<wire x1="93.96" y1="64.44" x2="55.88" y2="64.44" width="0" layer="20"/>
<wire x1="55.88" y1="64.44" x2="55.88" y2="22.86" width="0" layer="20"/>
<text>EDesign</text>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="2X03SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="GREEN" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="R1" library="fab" package="R1206FAB" value="499"/>
<element name="R2" library="fab" package="R1206FAB" value="1K"/>
<element name="R3" library="fab" package="R1206FAB" value="10K"/>
<element name="RED" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="S1" library="fab" package="6MM_SWITCH" value=""/>
<element name="U$1" library="fab" package="SOIC8" value="ATTINY45SI"/>
<element name="U$2" library="fab" package="2X03SMD" value="AVRISPSMD"/>
</elements>
<signals>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="GREEN" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="RED" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="4"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="1"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="SCK">
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="7"/>
<contactref element="S1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="RST">
<contactref element="U$2" pad="5"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="U$1" pad="8"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="LED2">
<contactref element="RED" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="U$2" pad="6"/>
<contactref element="R3" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="LED1">
<contactref element="GREEN" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
