<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="24.13" x2="45.7" y2="24.13" width="0" layer="20"/>
<wire x1="45.7" y1="24.13" x2="45.7" y2="64.44" width="0" layer="20"/>
<wire x1="45.7" y1="64.44" x2="0" y2="64.44" width="0" layer="20"/>
<wire x1="0" y1="64.44" x2="0" y2="24.13" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="R1206FAB">
</package>
<package name="1X06SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="fab" package="SOIC14" value="ATTINY44-SSU"/>
<element name="ISP" library="fab" package="2X03SMD" value=""/>
<element name="LED01" library="fab" package="LED1206FAB" value="Blue"/>
<element name="LED02" library="fab" package="LED1206FAB" value="Blue"/>
<element name="LED03" library="fab" package="LED1206FAB" value="Blue"/>
<element name="LED04" library="fab" package="LED1206FAB" value="Blue"/>
<element name="POT" library="fab" package="2X03SMD" value=""/>
<element name="R1" library="fab" package="R1206FAB" value="220"/>
<element name="R2" library="fab" package="R1206FAB" value=""/>
<element name="R3" library="fab" package="R1206FAB" value=""/>
<element name="R4" library="fab" package="R1206FAB" value=""/>
<element name="U$5" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
</elements>
<signals>
<signal name="POT">
<contactref element="IC1" pad="13"/>
<contactref element="POT" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="POT" pad="1"/>
<contactref element="U$5" pad="3"/>
<contactref element="ISP" pad="6"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="14"/>
<contactref element="POT" pad="5"/>
<contactref element="ISP" pad="2"/>
<contactref element="U$5" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="RST">
<contactref element="ISP" pad="1"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="SCK">
<contactref element="ISP" pad="3"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="MISO">
<contactref element="ISP" pad="5"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="MOSI">
<contactref element="ISP" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="CTS">
<contactref element="U$5" pad="2"/>
</signal>
<signal name="TXD">
<contactref element="U$5" pad="4"/>
</signal>
<signal name="RXD">
<contactref element="U$5" pad="5"/>
</signal>
<signal name="RTS">
<contactref element="U$5" pad="6"/>
</signal>
<signal name="LED01">
<contactref element="IC1" pad="11"/>
<contactref element="LED01" pad="1"/>
</signal>
<signal name="LED02">
<contactref element="IC1" pad="10"/>
<contactref element="LED02" pad="1"/>
</signal>
<signal name="LED03">
<contactref element="IC1" pad="6"/>
<contactref element="LED03" pad="1"/>
</signal>
<signal name="LED04">
<contactref element="IC1" pad="3"/>
<contactref element="LED04" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="LED01" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LED02" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="LED03" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="2"/>
<contactref element="LED04" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
