<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="44.12" y2="0" width="0" layer="20"/>
<wire x1="44.12" y1="0" x2="44.12" y2="30.47" width="0" layer="20"/>
<wire x1="44.12" y1="30.47" x2="0" y2="30.47" width="0" layer="20"/>
<wire x1="0" y1="30.47" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="01fab">
<packages>
<package name="C1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="R1206FAB">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="1X06SMD">
</package>
<package name="2X02SMD">
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="01fab" package="C1206FAB" value="1uF"/>
<element name="JP1" library="01fab" package="2X03SMD" value=""/>
<element name="R1" library="01fab" package="R1206FAB" value="1K"/>
<element name="R2" library="01fab" package="R1206FAB" value="10K"/>
<element name="U$1" library="01fab" package="SOIC8" value="ATTINY45SI"/>
<element name="U$2" library="01fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="U$4" library="01fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="WHITE" library="01fab" package="LED1206" value="LED"/>
</elements>
<signals>
<signal name="RST">
<contactref element="JP1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="A">
<contactref element="R1" pad="1"/>
<contactref element="WHITE" pad="1"/>
</signal>
<signal name="C">
<contactref element="WHITE" pad="2"/>
<contactref element="U$1" pad="5"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$4" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="V">
<contactref element="U$2" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="JP1" pad="5"/>
<contactref element="R1" pad="2"/>
<contactref element="U$4" pad="3"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="TX">
<contactref element="U$2" pad="4"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$4" pad="2"/>
</signal>
<signal name="RX">
<contactref element="U$2" pad="5"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$4" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
