<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.3">
<drawing>
<board>
<plain>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="2X05SMD">
</package>
<package name="TQFP32-08THIN">
</package>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="bt_con-jst-xh">
<description>&lt;b&gt;J.S.T. Connectors XH Family&lt;/b&gt;
&lt;p&gt;Created by Michael Shimniok &lt;a href="http://www.bot-thoughts.com/"&gt;www.bot-thoughts.com&lt;/a&gt;&lt;/b&gt;</description>
<packages>
<package name="B3B-XH">
<description>&lt;b&gt;JST XH Connector&lt;/b&gt;

&lt;p&gt;JST 2.54mm connector. Folded beam contact, box-shaped shrouded header, header with a boss, interchangeability, conformance to the HA terminal&lt;/p&gt;

&lt;p&gt;Datasheet: &lt;a href="http://www.jst-mfg.com/product/pdf/eng/eXH.pdf"&gt; eXH.pdf&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="B4B-XH">
<description>&lt;b&gt;JST XH Connector&lt;/b&gt;

&lt;p&gt;JST 2.54mm connector. Folded beam contact, box-shaped shrouded header, header with a boss, interchangeability, conformance to the HA terminal&lt;/p&gt;

&lt;p&gt;Datasheet: &lt;a href="http://www.jst-mfg.com/product/pdf/eng/eXH.pdf"&gt; eXH.pdf&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="B2B-XH">
<description>&lt;b&gt;JST XH Connector&lt;/b&gt;

&lt;p&gt;JST 2.54mm connector. Folded beam contact, box-shaped shrouded header, header with a boss, interchangeability, conformance to the HA terminal&lt;/p&gt;

&lt;p&gt;Datasheet: &lt;a href="http://www.jst-mfg.com/product/pdf/eng/eXH.pdf"&gt; eXH.pdf&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="con-wago-508">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.08 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-132">
<description>&lt;b&gt;WAGO SREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49UP">
<description>&lt;h3&gt;HC-49/UP 11.4x4.8mm SMD Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.standardcrystalcorp.com/pdf%5Cc-3.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="power_led">
<packages>
<package name="SIMPLEHOLE1MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="fab" package="SOT223" value="REGULATOR_SOT223"/>
<element name="T1" library="fab" package="TO252" value=""/>
<element name="C1" library="fab" package="C1206FAB" value="22pF"/>
<element name="C2" library="fab" package="C1206FAB" value="22pF"/>
<element name="C3" library="fab" package="C1206FAB" value="10uF"/>
<element name="C4" library="fab" package="C1206FAB" value="1uF"/>
<element name="C5" library="fab" package="C1206FAB" value="100nF"/>
<element name="C6" library="fab" package="C1206FAB" value="100nF"/>
<element name="C7" library="fab" package="C1206FAB" value="10uF"/>
<element name="C8" library="fab" package="C1206FAB" value="10uF"/>
<element name="C9" library="fab" package="C1206FAB" value="100uF"/>
<element name="R1" library="fab" package="R1206FAB" value="10K"/>
<element name="R2" library="fab" package="R1206FAB" value="499"/>
<element name="R3" library="fab" package="R1206FAB" value="499"/>
<element name="R4" library="fab" package="R1206FAB" value="10K"/>
<element name="D1" library="fab" package="SOD123" value=""/>
<element name="S1" library="fab" package="6MM_SWITCH" value=""/>
<element name="U$1" library="fab" package="LED1206FAB" value="YELLOW"/>
<element name="U$2" library="fab" package="LED1206FAB" value="GREEN"/>
<element name="U$4" library="bt_con-jst-xh" package="B3B-XH" value="RCWL"/>
<element name="U$5" library="bt_con-jst-xh" package="B3B-XH" value="SERVO"/>
<element name="X1" library="bt_con-jst-xh" package="B4B-XH" value="VL53LOX"/>
<element name="X2" library="con-wago-508" package="W237-132" value=""/>
<element name="X3" library="con-wago-508" package="W237-132" value=""/>
<element name="U$6" library="fab" package="2X05SMD" value="PINHD-2X5-SMD"/>
<element name="R5" library="fab" package="R1206FAB" value="4.99K"/>
<element name="R6" library="fab" package="R1206FAB" value="4.99K"/>
<element name="16MHZ" library="SparkFun-Clocks" package="HC49UP" value=""/>
<element name="IC1" library="fab" package="TQFP32-08THIN" value="ATMEGA88-THIN"/>
<element name="RST" library="power_led" package="SIMPLEHOLE1MM" value="SIMPLEHOLE1MM"/>
<element name="GND" library="power_led" package="SIMPLEHOLE1MM" value="SIMPLEHOLE1MM"/>
<element name="5V" library="power_led" package="SIMPLEHOLE1MM" value="SIMPLEHOLE1MM"/>
<element name="MOSI" library="power_led" package="SIMPLEHOLE1MM" value="SIMPLEHOLE1MM"/>
<element name="MISO" library="power_led" package="SIMPLEHOLE1MM" value="SIMPLEHOLE1MM"/>
<element name="SCK" library="power_led" package="SIMPLEHOLE1MM" value="SIMPLEHOLE1MM"/>
<element name="RX" library="power_led" package="SIMPLEHOLE1MM" value="SIMPLEHOLE1MM"/>
<element name="TX" library="power_led" package="SIMPLEHOLE1MM" value="SIMPLEHOLE1MM"/>
<element name="ADJ" library="bt_con-jst-xh" package="B2B-XH" value="02-JST"/>
<element name="D2" library="fab" package="SOD123" value=""/>
<element name="D3" library="fab" package="SOD123" value=""/>
</elements>
<signals>
<signal name="5V">
<contactref element="U$4" pad="P$2"/>
<contactref element="U$5" pad="P$2"/>
<contactref element="X1" pad="P$3"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U$2" pad="1"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="20"/>
<contactref element="R1" pad="1"/>
<contactref element="5V" pad="HOLE"/>
<contactref element="D1" pad="ANODE"/>
</signal>
<signal name="YELLOW">
<contactref element="U$1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="R4" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="U$4" pad="P$3"/>
<contactref element="U$5" pad="P$3"/>
<contactref element="X2" pad="2"/>
<contactref element="X1" pad="P$4"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="IC1" pad="21"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="GND" pad="HOLE"/>
<contactref element="U1" pad="1"/>
<contactref element="T1" pad="2"/>
</signal>
<signal name="GREEN">
<contactref element="R3" pad="2"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="IC1" pad="29"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="XTAL1">
<contactref element="IC1" pad="7"/>
<contactref element="16MHZ" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="XTAL2">
<contactref element="IC1" pad="8"/>
<contactref element="16MHZ" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="CA1">
<contactref element="IC1" pad="23"/>
<contactref element="U$6" pad="9"/>
</signal>
<signal name="CA2">
<contactref element="IC1" pad="24"/>
<contactref element="U$6" pad="7"/>
</signal>
<signal name="CA3">
<contactref element="IC1" pad="25"/>
<contactref element="U$6" pad="5"/>
</signal>
<signal name="CA4">
<contactref element="IC1" pad="26"/>
<contactref element="U$6" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="27"/>
<contactref element="R5" pad="1"/>
<contactref element="X1" pad="P$2"/>
</signal>
<signal name="SCL">
<contactref element="IC1" pad="28"/>
<contactref element="R6" pad="1"/>
<contactref element="X1" pad="P$1"/>
</signal>
<signal name="N$78">
<contactref element="IC1" pad="19"/>
</signal>
<signal name="N$79">
<contactref element="IC1" pad="22"/>
</signal>
<signal name="N$80">
<contactref element="IC1" pad="30"/>
<contactref element="RX" pad="HOLE"/>
</signal>
<signal name="N$81">
<contactref element="IC1" pad="31"/>
<contactref element="TX" pad="HOLE"/>
</signal>
<signal name="RCWL">
<contactref element="IC1" pad="32"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="SERVO">
<contactref element="IC1" pad="1"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="SW">
<contactref element="IC1" pad="2"/>
<contactref element="T1" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="ADJ1">
<contactref element="IC1" pad="9"/>
<contactref element="D2" pad="ANODE"/>
</signal>
<signal name="ADJ2">
<contactref element="IC1" pad="10"/>
<contactref element="D3" pad="ANODE"/>
</signal>
<signal name="N$87">
<contactref element="IC1" pad="11"/>
</signal>
<signal name="AN1">
<contactref element="IC1" pad="12"/>
<contactref element="U$6" pad="2"/>
</signal>
<signal name="AN2">
<contactref element="IC1" pad="13"/>
<contactref element="U$6" pad="4"/>
</signal>
<signal name="AN3">
<contactref element="IC1" pad="14"/>
<contactref element="U$6" pad="6"/>
</signal>
<signal name="AN4">
<contactref element="IC1" pad="15"/>
<contactref element="U$6" pad="8"/>
<contactref element="MOSI" pad="HOLE"/>
</signal>
<signal name="AN5">
<contactref element="IC1" pad="16"/>
<contactref element="U$6" pad="10"/>
<contactref element="MISO" pad="HOLE"/>
</signal>
<signal name="CA5">
<contactref element="IC1" pad="17"/>
<contactref element="U$1" pad="1"/>
<contactref element="SCK" pad="HOLE"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="X2" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="X3" pad="1"/>
<contactref element="D1" pad="CATHODE"/>
</signal>
<signal name="RESET_PIN">
<contactref element="C6" pad="1"/>
<contactref element="RST" pad="HOLE"/>
</signal>
<signal name="DRAIN">
<contactref element="X3" pad="2"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="D3" pad="CATHODE"/>
<contactref element="ADJ" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="CATHODE"/>
<contactref element="ADJ" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
