<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.3">
<drawing>
<schematic>
<libraries>
<library name="fab">
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="C1206FAB">
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
<package name="2X05SMD">
</package>
<package name="TQFP32-08THIN">
</package>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="REGULATOR_SOT223">
<pin name="IN"/>
<pin name="GND"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
</symbol>
<symbol name="N_MOSFET">
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="C-US">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="TS2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
<symbol name="LED">
<description>LED</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="PINH2X5">
<pin name="1" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="23-I/O">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="D">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="REGULATOR_SOT223" prefix="U">
<gates>
<gate name="G$1" symbol="REGULATOR_SOT223"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NMOSFET" prefix="T" uservalue="yes">
<description>&lt;b&gt;MOS FET&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="N_MOSFET"/>
</gates>
<devices>
<device name="SOT23" package="SOT-23">
<connects>
<connect gate="A" pin="D" pad="1"/>
<connect gate="A" pin="G" pad="3"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO252" package="TO252">
<connects>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-US" prefix="C">
<gates>
<gate name="G$1" symbol="C-US"/>
</gates>
<devices>
<device name="1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206K" package="C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="C1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6MM_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
<gates>
<gate name="2" symbol="TS2"/>
</gates>
<devices>
<device name="6MM_SWITCH" package="6MM_SWITCH">
<connects>
<connect gate="2" pin="P" pad="1"/>
<connect gate="2" pin="P1" pad="2"/>
<connect gate="2" pin="S" pad="3"/>
<connect gate="2" pin="S1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB1206" package="LED1206FAB">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X5-SMD">
<gates>
<gate name="G$1" symbol="PINH2X5"/>
</gates>
<devices>
<device name="" package="2X05SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA88-THIN" prefix="IC">
<gates>
<gate name="G$1" symbol="23-I/O"/>
</gates>
<devices>
<device name="" package="TQFP32-08THIN">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE" prefix="D" uservalue="yes">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
high speed (Philips)</description>
<gates>
<gate name="G$1" symbol="D"/>
</gates>
<devices>
<device name="SOD123" package="SOD123">
<connects>
<connect gate="G$1" pin="A" pad="ANODE"/>
<connect gate="G$1" pin="C" pad="CATHODE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="bt_con-jst-xh">
<description>&lt;b&gt;J.S.T. Connectors XH Family&lt;/b&gt;
&lt;p&gt;Created by Michael Shimniok &lt;a href="http://www.bot-thoughts.com/"&gt;www.bot-thoughts.com&lt;/a&gt;&lt;/b&gt;</description>
<packages>
<package name="B3B-XH">
<description>&lt;b&gt;JST XH Connector&lt;/b&gt;

&lt;p&gt;JST 2.54mm connector. Folded beam contact, box-shaped shrouded header, header with a boss, interchangeability, conformance to the HA terminal&lt;/p&gt;

&lt;p&gt;Datasheet: &lt;a href="http://www.jst-mfg.com/product/pdf/eng/eXH.pdf"&gt; eXH.pdf&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="B4B-XH">
<description>&lt;b&gt;JST XH Connector&lt;/b&gt;

&lt;p&gt;JST 2.54mm connector. Folded beam contact, box-shaped shrouded header, header with a boss, interchangeability, conformance to the HA terminal&lt;/p&gt;

&lt;p&gt;Datasheet: &lt;a href="http://www.jst-mfg.com/product/pdf/eng/eXH.pdf"&gt; eXH.pdf&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="B2B-XH">
<description>&lt;b&gt;JST XH Connector&lt;/b&gt;

&lt;p&gt;JST 2.54mm connector. Folded beam contact, box-shaped shrouded header, header with a boss, interchangeability, conformance to the HA terminal&lt;/p&gt;

&lt;p&gt;Datasheet: &lt;a href="http://www.jst-mfg.com/product/pdf/eng/eXH.pdf"&gt; eXH.pdf&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="P-VN">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="P-N">
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="03-JST">
<description>&lt;B&gt;JST CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="-1" symbol="P-VN"/>
<gate name="-2" symbol="P-N"/>
<gate name="-3" symbol="P-N"/>
</gates>
<devices>
<device name="-B3B-XH-A" package="B3B-XH">
<connects>
<connect gate="-1" pin="1" pad="P$1"/>
<connect gate="-2" pin="1" pad="P$2"/>
<connect gate="-3" pin="1" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="04-JST" prefix="X">
<description>&lt;b&gt;JST CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="-1" symbol="P-VN"/>
<gate name="-2" symbol="P-N"/>
<gate name="-3" symbol="P-N"/>
<gate name="-4" symbol="P-N"/>
</gates>
<devices>
<device name="-B4B-XH-A" package="B4B-XH">
<connects>
<connect gate="-1" pin="1" pad="P$1"/>
<connect gate="-2" pin="1" pad="P$2"/>
<connect gate="-3" pin="1" pad="P$3"/>
<connect gate="-4" pin="1" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="02-JST">
<description>&lt;B&gt;JST CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="-1" symbol="P-VN"/>
<gate name="-2" symbol="P-N"/>
</gates>
<devices>
<device name="" package="B2B-XH">
<connects>
<connect gate="-1" pin="1" pad="P$1"/>
<connect gate="-2" pin="1" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="con-wago-508">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.08 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-132">
<description>&lt;b&gt;WAGO SREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="KL">
<pin name="KL" direction="pas"/>
</symbol>
<symbol name="KL+V">
<pin name="KL" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="W237-02P" prefix="X" uservalue="yes">
<description>&lt;b&gt;WAGO SREW CLAMP&lt;/b&gt;</description>
<gates>
<gate name="-1" symbol="KL"/>
<gate name="-2" symbol="KL+V"/>
</gates>
<devices>
<device name="" package="W237-132">
<connects>
<connect gate="-1" pin="KL" pad="1"/>
<connect gate="-2" pin="KL" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49U">
<description>&lt;h3&gt;HC49/U 11.6x4.6mm PTH Crystal (13.46mm height)&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.digikey.com/Web%20Export/Supplier%20Content/Citizen_300/PDF/Citizen_HC49US.pdf?redirected=1"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="CRYSTAL-PTH-3X8-CYL">
<description>&lt;h3&gt;3x8mm Cylindrical Can (Radial) PTH Crystal&lt;/h3&gt;

This is the "KIT" version, which has limited top masking for improved ease of assembly.

&lt;p&gt;Example product: &lt;a href="https://www.sparkfun.com/products/540"&gt;32kHz crystal&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.ecsxtal.com/store/pdf/ECS-3x8.pdf"&gt;Example datasheet&lt;/a&gt; (ECS-3X8)&lt;/p&gt;</description>
</package>
<package name="CRYSTAL-PTH-2X6-CYL">
<description>&lt;h3&gt;2x6mm Cylindrical Can (Radial) PTH Crystal&lt;/h3&gt;

&lt;p&gt;Example product: &lt;a href="https://www.sparkfun.com/products/540"&gt;32kHz crystal&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.ecsxtal.com/store/pdf/ECS-3x8.pdf"&gt;Example datasheet&lt;/a&gt; (ECS-2X6)&lt;/p&gt;</description>
</package>
<package name="HC49UP">
<description>&lt;h3&gt;HC-49/UP 11.4x4.8mm SMD Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.standardcrystalcorp.com/pdf%5Cc-3.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="HC49US">
<description>&lt;h3&gt;HC49/US 11.6x4.6mm PTH Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.digikey.com/Web%20Export/Supplier%20Content/Citizen_300/PDF/Citizen_HC49US.pdf?redirected=1"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="CRYSTAL-SMD-2X6-CYL">
<description>&lt;h3&gt;6.0x2.0mm Cylindrical Can (Radial) SMD Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://cfm.citizen.co.jp/english/product/pdf/CMR200T.pdf"&gt;Example&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="CRYSTAL-SMD-5X3.2-4PAD">
<description>&lt;h3&gt;5x3.2mm SMD Crystal&lt;/h3&gt;
&lt;p&gt;Example: &lt;a href="https://www.sparkfun.com/products/94"&gt;16MHz SMD Crystal&lt;/a&gt; (&lt;a href="https://www.sparkfun.com/datasheets/Components/SPK-5032-16MHZ.pdf"&gt;Datasheet&lt;/a&gt;)&lt;/p&gt;</description>
</package>
<package name="CRYSTAL-SMD-MC-146">
<description>&lt;h3&gt;7x1.5mm MC-146 Flat Lead SMD Crystal&lt;/h3&gt;

&lt;p&gt;&lt;a href="https://support.epson.biz/td/api/doc_check.php?dl=brief_MC-156_en.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="CRYSTAL-PTH-2X6-CYL-KIT">
<description>&lt;h3&gt;2x6mm Cylindrical Can (Radial) PTH Crystal&lt;/h3&gt;

This is the "KIT" version, which has limited top masking for improved ease of assembly.

&lt;p&gt;Example product: &lt;a href="https://www.sparkfun.com/products/540"&gt;32kHz crystal&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.ecsxtal.com/store/pdf/ECS-3x8.pdf"&gt;Example datasheet&lt;/a&gt; (ECS-2X6)&lt;/p&gt;</description>
</package>
<package name="CRYSTAL-SMD-5X3.2-2PAD">
<description>&lt;h3&gt;5x3.2mm 2-pad SMD Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.txccrystal.com/images/pdf/7a.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="CRYSTAL-SMD-3.2X1.5MM">
<description>&lt;h3&gt;3.2 x 1.5mm SMD Crystal Package&lt;/h3&gt;
&lt;p&gt;Example: &lt;a href="http://www.sii.co.jp/en/quartz/files/2013/03/file_PRODUCT_MASTER_50812_GRAPHIC03.pdf"&gt;SX-32S&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="CRYSTAL-SMD-3.2X2.5MM">
<description>&lt;h3&gt;3.2 x 2.5mm SMD Crystal Package&lt;/h3&gt;
&lt;p&gt;Example: &lt;a href="http://www.digikey.com/product-search/en?keywords=SER3627TR-ND"&gt;SX-32S&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="CRYSTAL">
<description>&lt;h3&gt;Crystal (no ground pin)&lt;/h3&gt;</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CRYSTAL" prefix="Y" uservalue="yes">
<description>&lt;h3&gt;Crystals (Generic)&lt;/h3&gt;
&lt;p&gt;These are &lt;b&gt;passive&lt;/b&gt; quartz crystals, which can be used as a clock source for a microcontroller.&lt;/p&gt;
&lt;p&gt;Crystal's are two-terminal devices. They require external "load" capacitors to generate an oscillating signal.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="PTH-HC49UV" package="HC49U">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-3X8" package="CRYSTAL-PTH-3X8-CYL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-2X6" package="CRYSTAL-PTH-2X6-CYL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-HC49UP" package="HC49UP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-HC49US" package="HC49US">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-2X6" package="CRYSTAL-SMD-2X6-CYL">
<connects>
<connect gate="G$1" pin="1" pad="X1"/>
<connect gate="G$1" pin="2" pad="X2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-5X3.2-4PAD" package="CRYSTAL-SMD-5X3.2-4PAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-MC146" package="CRYSTAL-SMD-MC-146">
<connects>
<connect gate="G$1" pin="1" pad="P$2"/>
<connect gate="G$1" pin="2" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-2X6-KIT" package="CRYSTAL-PTH-2X6-CYL-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-5X3.2-2PAD" package="CRYSTAL-SMD-5X3.2-2PAD">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-3.2X1.5" package="CRYSTAL-SMD-3.2X1.5MM">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-3.2X2.5" package="CRYSTAL-SMD-3.2X2.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="HelloKamakura">
<description>Generated from &lt;b&gt;HelloKamakura.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
</packages>
<symbols>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="power_led">
<packages>
<package name="SIMPLEHOLE1MM">
</package>
</packages>
<symbols>
<symbol name="SIMPLEHOLE1MM">
<pin name="P$1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SIMPLEHOLE1MM">
<gates>
<gate name="G$1" symbol="SIMPLEHOLE1MM"/>
</gates>
<devices>
<device name="" package="SIMPLEHOLE1MM">
<connects>
<connect gate="G$1" pin="P$1" pad="HOLE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="U1" library="fab" deviceset="REGULATOR_SOT223" device=""/>
<part name="T1" library="fab" deviceset="NMOSFET" device="TO252"/>
<part name="C1" library="fab" deviceset="CAP-US" device="1206FAB" value="22pF"/>
<part name="C2" library="fab" deviceset="CAP-US" device="1206FAB" value="22pF"/>
<part name="C3" library="fab" deviceset="CAP-US" device="1206FAB" value="10uF"/>
<part name="C4" library="fab" deviceset="CAP-US" device="1206FAB" value="1uF"/>
<part name="C5" library="fab" deviceset="CAP-US" device="1206FAB" value="100nF"/>
<part name="C6" library="fab" deviceset="CAP-US" device="1206FAB" value="100nF"/>
<part name="C7" library="fab" deviceset="CAP-US" device="1206FAB" value="10uF"/>
<part name="C8" library="fab" deviceset="CAP-US" device="1206FAB" value="10uF"/>
<part name="C9" library="fab" deviceset="CAP-US" device="1206FAB" value="100uF"/>
<part name="R1" library="fab" deviceset="RES-US" device="1206FAB" value="10K"/>
<part name="R2" library="fab" deviceset="RES-US" device="1206FAB" value="499"/>
<part name="R3" library="fab" deviceset="RES-US" device="1206FAB" value="499"/>
<part name="R4" library="fab" deviceset="RES-US" device="1206FAB" value="10K"/>
<part name="D1" library="fab" deviceset="DIODE" device="SOD123"/>
<part name="S1" library="fab" deviceset="6MM_SWITCH" device="6MM_SWITCH"/>
<part name="U$1" library="fab" deviceset="LED" device="FAB1206" value="YELLOW"/>
<part name="U$2" library="fab" deviceset="LED" device="FAB1206" value="GREEN"/>
<part name="U$4" library="bt_con-jst-xh" deviceset="03-JST" device="-B3B-XH-A" value="RCWL"/>
<part name="U$5" library="bt_con-jst-xh" deviceset="03-JST" device="-B3B-XH-A" value="SERVO"/>
<part name="X1" library="bt_con-jst-xh" deviceset="04-JST" device="-B4B-XH-A" value="VL53LOX"/>
<part name="X2" library="con-wago-508" deviceset="W237-02P" device=""/>
<part name="X3" library="con-wago-508" deviceset="W237-02P" device=""/>
<part name="U$6" library="fab" deviceset="PINHD-2X5-SMD" device=""/>
<part name="R5" library="fab" deviceset="RES-US" device="1206FAB" value="4.99K"/>
<part name="R6" library="fab" deviceset="RES-US" device="1206FAB" value="4.99K"/>
<part name="16MHZ" library="SparkFun-Clocks" deviceset="CRYSTAL" device="SMD-HC49UP"/>
<part name="GND1" library="HelloKamakura" deviceset="GND" device=""/>
<part name="IC1" library="fab" deviceset="ATMEGA88-THIN" device=""/>
<part name="GND2" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND3" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND4" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND5" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND6" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND7" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND8" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND9" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND11" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND12" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND13" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND14" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND15" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND16" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND17" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND18" library="HelloKamakura" deviceset="GND" device=""/>
<part name="RST" library="power_led" deviceset="SIMPLEHOLE1MM" device=""/>
<part name="GND" library="power_led" deviceset="SIMPLEHOLE1MM" device=""/>
<part name="5V" library="power_led" deviceset="SIMPLEHOLE1MM" device=""/>
<part name="MOSI" library="power_led" deviceset="SIMPLEHOLE1MM" device=""/>
<part name="MISO" library="power_led" deviceset="SIMPLEHOLE1MM" device=""/>
<part name="SCK" library="power_led" deviceset="SIMPLEHOLE1MM" device=""/>
<part name="RX" library="power_led" deviceset="SIMPLEHOLE1MM" device=""/>
<part name="TX" library="power_led" deviceset="SIMPLEHOLE1MM" device=""/>
<part name="GND19" library="HelloKamakura" deviceset="GND" device=""/>
<part name="ADJ" library="bt_con-jst-xh" deviceset="02-JST" device=""/>
<part name="GND20" library="HelloKamakura" deviceset="GND" device=""/>
<part name="GND10" library="HelloKamakura" deviceset="GND" device=""/>
<part name="D2" library="fab" deviceset="DIODE" device="SOD123"/>
<part name="D3" library="fab" deviceset="DIODE" device="SOD123"/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="5V">
<segment>
<pinref part="U$4" gate="-2" pin="1"/>
</segment>
<segment>
<pinref part="U$5" gate="-2" pin="1"/>
</segment>
<segment>
<pinref part="X1" gate="-3" pin="1"/>
</segment>
<segment>
<pinref part="R5" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="R6" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C8" gate="G$1" pin="2"/>
<pinref part="U1" gate="G$1" pin="OUT1"/>
<pinref part="C9" gate="G$1" pin="2"/>
<pinref part="D1" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="C5" gate="G$1" pin="2"/>
<pinref part="C4" gate="G$1" pin="2"/>
<pinref part="C3" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="AVCC"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="VCC@1"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="VCC@2"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="AREF"/>
</segment>
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="5V" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="YELLOW">
<segment>
<pinref part="U$1" gate="G$1" pin="C"/>
<pinref part="R2" gate="G$1" pin="2"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="R4" gate="G$1" pin="1"/>
<pinref part="GND1" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C1" gate="G$1" pin="2"/>
<pinref part="GND2" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C2" gate="G$1" pin="2"/>
<pinref part="GND3" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C9" gate="G$1" pin="1"/>
<pinref part="GND4" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C8" gate="G$1" pin="1"/>
<pinref part="GND5" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C7" gate="G$1" pin="1"/>
<pinref part="GND6" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="U$4" gate="-3" pin="1"/>
<pinref part="GND8" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="U$5" gate="-3" pin="1"/>
<pinref part="GND7" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="X2" gate="-2" pin="KL"/>
<pinref part="GND9" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="X1" gate="-4" pin="1"/>
<pinref part="GND11" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C5" gate="G$1" pin="1"/>
<pinref part="C4" gate="G$1" pin="1"/>
<pinref part="C3" gate="G$1" pin="1"/>
<pinref part="GND12" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="GND13" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="R3" gate="G$1" pin="1"/>
<pinref part="GND14" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="S1" gate="2" pin="S"/>
<pinref part="S1" gate="2" pin="S1"/>
<pinref part="GND15" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="GND"/>
<pinref part="GND16" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="GND@1"/>
<pinref part="GND17" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="GND@2"/>
<pinref part="GND18" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND" gate="G$1" pin="P$1"/>
<pinref part="GND19" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="U1" gate="G$1" pin="GND"/>
<pinref part="GND20" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="T1" gate="A" pin="S"/>
<pinref part="GND10" gate="1" pin="GND"/>
</segment>
</net>
<net name="GREEN">
<segment>
<pinref part="R3" gate="G$1" pin="2"/>
<pinref part="U$2" gate="G$1" pin="C"/>
</segment>
</net>
<net name="RESET">
<segment>
<pinref part="S1" gate="2" pin="P"/>
<pinref part="S1" gate="2" pin="P1"/>
<pinref part="IC1" gate="G$1" pin="PC6(/RESET)"/>
<pinref part="R1" gate="G$1" pin="2"/>
<pinref part="C6" gate="G$1" pin="2"/>
</segment>
</net>
<net name="XTAL1">
<segment>
<pinref part="IC1" gate="G$1" pin="PB6(XTAL1/TOSC1)"/>
</segment>
<segment>
<pinref part="C1" gate="G$1" pin="1"/>
<pinref part="16MHZ" gate="G$1" pin="1"/>
</segment>
</net>
<net name="XTAL2">
<segment>
<pinref part="IC1" gate="G$1" pin="PB7(XTAL2/TOSC2)"/>
</segment>
<segment>
<pinref part="C2" gate="G$1" pin="1"/>
<pinref part="16MHZ" gate="G$1" pin="2"/>
</segment>
</net>
<net name="CA1">
<segment>
<pinref part="IC1" gate="G$1" pin="PC0(ADC0)"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="9"/>
</segment>
</net>
<net name="CA2">
<segment>
<pinref part="IC1" gate="G$1" pin="PC1(ADC1)"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="7"/>
</segment>
</net>
<net name="CA3">
<segment>
<pinref part="IC1" gate="G$1" pin="PC2(ADC2)"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="5"/>
</segment>
</net>
<net name="CA4">
<segment>
<pinref part="IC1" gate="G$1" pin="PC3(ADC3)"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="3"/>
</segment>
</net>
<net name="SDA">
<segment>
<pinref part="IC1" gate="G$1" pin="PC4(ADC4/SDA)"/>
</segment>
<segment>
<pinref part="R5" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="X1" gate="-2" pin="1"/>
</segment>
</net>
<net name="SCL">
<segment>
<pinref part="IC1" gate="G$1" pin="PC5(ADC5/SCL)"/>
</segment>
<segment>
<pinref part="R6" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="X1" gate="-1" pin="1"/>
</segment>
</net>
<net name="N$78">
<segment>
<pinref part="IC1" gate="G$1" pin="ADC6"/>
</segment>
</net>
<net name="N$79">
<segment>
<pinref part="IC1" gate="G$1" pin="ADC7"/>
</segment>
</net>
<net name="N$80">
<segment>
<pinref part="IC1" gate="G$1" pin="PD0(RXD)"/>
<pinref part="RX" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="N$81">
<segment>
<pinref part="IC1" gate="G$1" pin="PD1(TXD)"/>
<pinref part="TX" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="RCWL">
<segment>
<pinref part="IC1" gate="G$1" pin="PD2(INT0)"/>
</segment>
<segment>
<pinref part="U$4" gate="-1" pin="1"/>
</segment>
</net>
<net name="SERVO">
<segment>
<pinref part="IC1" gate="G$1" pin="PD3(INT1)"/>
</segment>
<segment>
<pinref part="U$5" gate="-1" pin="1"/>
</segment>
</net>
<net name="SW">
<segment>
<pinref part="IC1" gate="G$1" pin="PD4(XCK/T0)"/>
</segment>
<segment>
<pinref part="T1" gate="A" pin="G"/>
<pinref part="R4" gate="G$1" pin="2"/>
</segment>
</net>
<net name="ADJ1">
<segment>
<pinref part="IC1" gate="G$1" pin="PD5(T1)"/>
</segment>
<segment>
<pinref part="D2" gate="G$1" pin="A"/>
</segment>
</net>
<net name="ADJ2">
<segment>
<pinref part="IC1" gate="G$1" pin="PD6(AIN0)"/>
</segment>
<segment>
<pinref part="D3" gate="G$1" pin="A"/>
</segment>
</net>
<net name="N$87">
<segment>
<pinref part="IC1" gate="G$1" pin="PD7(AIN1)"/>
</segment>
</net>
<net name="AN1">
<segment>
<pinref part="IC1" gate="G$1" pin="PB0(ICP)"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="2"/>
</segment>
</net>
<net name="AN2">
<segment>
<pinref part="IC1" gate="G$1" pin="PB1(OC1A)"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="4"/>
</segment>
</net>
<net name="AN3">
<segment>
<pinref part="IC1" gate="G$1" pin="PB2(SS/OC1B)"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="6"/>
</segment>
</net>
<net name="AN4">
<segment>
<pinref part="IC1" gate="G$1" pin="PB3(MOSI/OC2)"/>
<pinref part="MOSI" gate="G$1" pin="P$1"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="8"/>
</segment>
</net>
<net name="AN5">
<segment>
<pinref part="IC1" gate="G$1" pin="PB4(MISO)"/>
<pinref part="MISO" gate="G$1" pin="P$1"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="10"/>
</segment>
</net>
<net name="CA5">
<segment>
<pinref part="IC1" gate="G$1" pin="PB5(SCK)"/>
<pinref part="SCK" gate="G$1" pin="P$1"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="1"/>
</segment>
</net>
<net name="VCC">
<segment>
<pinref part="X2" gate="-1" pin="KL"/>
</segment>
<segment>
<pinref part="C7" gate="G$1" pin="2"/>
<pinref part="U1" gate="G$1" pin="IN"/>
<pinref part="D1" gate="G$1" pin="C"/>
</segment>
<segment>
<pinref part="X3" gate="-1" pin="KL"/>
</segment>
</net>
<net name="RESET_PIN">
<segment>
<pinref part="C6" gate="G$1" pin="1"/>
<pinref part="RST" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="DRAIN">
<segment>
<pinref part="X3" gate="-2" pin="KL"/>
</segment>
<segment>
<pinref part="T1" gate="A" pin="D"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="D3" gate="G$1" pin="C"/>
<pinref part="ADJ" gate="-2" pin="1"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="D2" gate="G$1" pin="C"/>
<pinref part="ADJ" gate="-1" pin="1"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
