<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.0">
<drawing>
<schematic>
<libraries>
<library name="atmega8">
<packages>
<package name="MLF32">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
<symbols>
<symbol name="ATMEGA48/88/168-TQFP/QFN32">
<pin name="PB5(SCK/PCINT5)"/>
<pin name="PB7(XTAL2/TOSC2/PCINT7)"/>
<pin name="PB6(XTAL1/TOSC1/PCINT6)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pas"/>
<pin name="PB4(MISO/PCINT4)"/>
<pin name="PB3(MOSI/OC2A/PCINT3)"/>
<pin name="PB2(SS/OC1B/PCINT2)"/>
<pin name="PB1(OC1A/PCINT1)"/>
<pin name="PB0(ICP1/CLKO/PCINT0)"/>
<pin name="PD7(AIN1/PCINT23)"/>
<pin name="PD6(AIN0/OC0A/PCINT22)"/>
<pin name="PD5(T1/OC0B/PCINT21)"/>
<pin name="PD4(T0/XCK/PCINT20)"/>
<pin name="PD3(INT1/OC2B/PCINT19)"/>
<pin name="PD2(INT0/PCINT18)"/>
<pin name="PD1(TXD/PCINT17)"/>
<pin name="PD0(RXD/PCINT16)"/>
<pin name="PC5(ADC5/SCL/PCINT13)"/>
<pin name="PC4(ADC4/SDA/PCINT12)"/>
<pin name="PC3(ADC3/PCINT11)"/>
<pin name="PC2(ADC2/PCINT10)"/>
<pin name="PC1(ADC1/PCINT9)"/>
<pin name="PC0(ADC0/PCINT8)"/>
<pin name="PC6(/RESET/PCINT14)"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="ADC7" direction="pas"/>
<pin name="ADC6" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATMEGA48/88/168" prefix="IC">
<gates>
<gate name="1" symbol="ATMEGA48/88/168-TQFP/QFN32"/>
</gates>
<devices>
<device name="-MU" package="MLF32">
<connects>
<connect gate="1" pin="ADC6" pad="19"/>
<connect gate="1" pin="ADC7" pad="22"/>
<connect gate="1" pin="AGND" pad="21"/>
<connect gate="1" pin="AREF" pad="20"/>
<connect gate="1" pin="AVCC" pad="18"/>
<connect gate="1" pin="GND@1" pad="3"/>
<connect gate="1" pin="GND@2" pad="5"/>
<connect gate="1" pin="PB0(ICP1/CLKO/PCINT0)" pad="12"/>
<connect gate="1" pin="PB1(OC1A/PCINT1)" pad="13"/>
<connect gate="1" pin="PB2(SS/OC1B/PCINT2)" pad="14"/>
<connect gate="1" pin="PB3(MOSI/OC2A/PCINT3)" pad="15"/>
<connect gate="1" pin="PB4(MISO/PCINT4)" pad="16"/>
<connect gate="1" pin="PB5(SCK/PCINT5)" pad="17"/>
<connect gate="1" pin="PB6(XTAL1/TOSC1/PCINT6)" pad="7"/>
<connect gate="1" pin="PB7(XTAL2/TOSC2/PCINT7)" pad="8"/>
<connect gate="1" pin="PC0(ADC0/PCINT8)" pad="23"/>
<connect gate="1" pin="PC1(ADC1/PCINT9)" pad="24"/>
<connect gate="1" pin="PC2(ADC2/PCINT10)" pad="25"/>
<connect gate="1" pin="PC3(ADC3/PCINT11)" pad="26"/>
<connect gate="1" pin="PC4(ADC4/SDA/PCINT12)" pad="27"/>
<connect gate="1" pin="PC5(ADC5/SCL/PCINT13)" pad="28"/>
<connect gate="1" pin="PC6(/RESET/PCINT14)" pad="29"/>
<connect gate="1" pin="PD0(RXD/PCINT16)" pad="30"/>
<connect gate="1" pin="PD1(TXD/PCINT17)" pad="31"/>
<connect gate="1" pin="PD2(INT0/PCINT18)" pad="32"/>
<connect gate="1" pin="PD3(INT1/OC2B/PCINT19)" pad="1"/>
<connect gate="1" pin="PD4(T0/XCK/PCINT20)" pad="2"/>
<connect gate="1" pin="PD5(T1/OC0B/PCINT21)" pad="9"/>
<connect gate="1" pin="PD6(AIN0/OC0A/PCINT22)" pad="10"/>
<connect gate="1" pin="PD7(AIN1/PCINT23)" pad="11"/>
<connect gate="1" pin="VCC@1" pad="4"/>
<connect gate="1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AU" package="TQFP32-08">
<connects>
<connect gate="1" pin="ADC6" pad="19"/>
<connect gate="1" pin="ADC7" pad="22"/>
<connect gate="1" pin="AGND" pad="21"/>
<connect gate="1" pin="AREF" pad="20"/>
<connect gate="1" pin="AVCC" pad="18"/>
<connect gate="1" pin="GND@1" pad="3"/>
<connect gate="1" pin="GND@2" pad="5"/>
<connect gate="1" pin="PB0(ICP1/CLKO/PCINT0)" pad="12"/>
<connect gate="1" pin="PB1(OC1A/PCINT1)" pad="13"/>
<connect gate="1" pin="PB2(SS/OC1B/PCINT2)" pad="14"/>
<connect gate="1" pin="PB3(MOSI/OC2A/PCINT3)" pad="15"/>
<connect gate="1" pin="PB4(MISO/PCINT4)" pad="16"/>
<connect gate="1" pin="PB5(SCK/PCINT5)" pad="17"/>
<connect gate="1" pin="PB6(XTAL1/TOSC1/PCINT6)" pad="7"/>
<connect gate="1" pin="PB7(XTAL2/TOSC2/PCINT7)" pad="8"/>
<connect gate="1" pin="PC0(ADC0/PCINT8)" pad="23"/>
<connect gate="1" pin="PC1(ADC1/PCINT9)" pad="24"/>
<connect gate="1" pin="PC2(ADC2/PCINT10)" pad="25"/>
<connect gate="1" pin="PC3(ADC3/PCINT11)" pad="26"/>
<connect gate="1" pin="PC4(ADC4/SDA/PCINT12)" pad="27"/>
<connect gate="1" pin="PC5(ADC5/SCL/PCINT13)" pad="28"/>
<connect gate="1" pin="PC6(/RESET/PCINT14)" pad="29"/>
<connect gate="1" pin="PD0(RXD/PCINT16)" pad="30"/>
<connect gate="1" pin="PD1(TXD/PCINT17)" pad="31"/>
<connect gate="1" pin="PD2(INT0/PCINT18)" pad="32"/>
<connect gate="1" pin="PD3(INT1/OC2B/PCINT19)" pad="1"/>
<connect gate="1" pin="PD4(T0/XCK/PCINT20)" pad="2"/>
<connect gate="1" pin="PD5(T1/OC0B/PCINT21)" pad="9"/>
<connect gate="1" pin="PD6(AIN0/OC0A/PCINT22)" pad="10"/>
<connect gate="1" pin="PD7(AIN1/PCINT23)" pad="11"/>
<connect gate="1" pin="VCC@1" pad="4"/>
<connect gate="1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="CSM-7X-DU">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;&lt;p&gt;
Source: www.ecsxtal.com .. Crystal 3.6864MHz CSM_7X_DU.PDF</description>
</package>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="5MM">
<description>5 mm, round</description>
</package>
<package name="0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="Q">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CSM-7X-DU" prefix="Q">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;&lt;p&gt;
Source: www.ecsxtal.com .. Crystal 3.6864MHz CSM_7X_DU.PDF</description>
<gates>
<gate name="P" symbol="Q"/>
</gates>
<devices>
<device name="" package="CSM-7X-DU">
<connects>
<connect gate="P" pin="1" pad="1"/>
<connect gate="P" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" uservalue="yes">
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="0402">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="AVX_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/04/2012 16:26:10</description>
<packages>
<package name="CAPC3216X178N">
</package>
</packages>
<symbols>
<symbol name="CAPH">
<pin name="C2" direction="pas"/>
<pin name="C1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="0612ZC225MAT2A" prefix="C">
<description>Capacitor 1206</description>
<gates>
<gate name="A" symbol="CAPH"/>
</gates>
<devices>
<device name="" package="CAPC3216X178N">
<connects>
<connect gate="A" pin="C1" pad="1"/>
<connect gate="A" pin="C2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="0612ZC225MAT2A"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="12N3209"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±20%"/>
<attribute name="VALUE" value="2.2µF"/>
<attribute name="VOLTAGERATING" value="10V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="AXIAL-0.3">
</package>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0805">
</package>
<package name="0603-RES">
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1/6W-RES">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
<package name="R2512">
</package>
<package name="CAP-PTH-SMALL">
</package>
<package name="CAP-PTH-SMALL2">
</package>
<package name="CAP-PTH-LARGE">
</package>
<package name="GRM43D">
</package>
<package name="0603-CAP">
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CAP-PTH-5MM">
</package>
<package name="AXIAL-5MM">
</package>
<package name="1210">
</package>
</packages>
<symbols>
<symbol name="RESISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor&lt;/b&gt;
Basic schematic elements and footprints for 0603, 1206, and PTH 1/10th watt (small) resistors.</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="AXIAL-0.3">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2010" package="R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603-RES" package="0603-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402-RES" package="0402-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1/6W" package="1/6W-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2512" package="R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP" prefix="C" uservalue="yes">
<description>&lt;b&gt;Capacitor&lt;/b&gt;
Standard 0603 ceramic capacitor, and 0.1" leaded capacitor.</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="PTH" package="CAP-PTH-SMALL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="CAP-PTH-SMALL2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="CAP-PTH-LARGE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="GRM43D">
<connects>
<connect gate="G$1" pin="1" pad="A"/>
<connect gate="G$1" pin="2" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603-CAP" package="0603-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402-CAP" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="CAP-PTH-5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="AXIAL-5MM">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="02P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="03P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="06P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="M02">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="M03">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="M06">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="M02" prefix="SL" uservalue="yes">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="M02"/>
</gates>
<devices>
<device name="" package="02P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M03" prefix="SL" uservalue="yes">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="M03"/>
</gates>
<devices>
<device name="" package="03P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M06" prefix="SL" uservalue="yes">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="M06"/>
</gates>
<devices>
<device name="" package="06P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO016">
</package>
</packages>
<symbols>
<symbol name="CH340G">
<pin name="GND"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="V3"/>
<pin name="UD+"/>
<pin name="UD-"/>
<pin name="XI"/>
<pin name="XO"/>
<pin name="!CTS"/>
<pin name="!DSR"/>
<pin name="!RI"/>
<pin name="!DCD"/>
<pin name="!DTR"/>
<pin name="!RTS"/>
<pin name="R232"/>
<pin name="VCC"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CH340G" prefix="U">
<description>A simple USB 2.0 to Serial IC.</description>
<gates>
<gate name="U1" symbol="CH340G"/>
</gates>
<devices>
<device name="SMD" package="SO016">
<connects>
<connect gate="U1" pin="!CTS" pad="9"/>
<connect gate="U1" pin="!DCD" pad="12"/>
<connect gate="U1" pin="!DSR" pad="10"/>
<connect gate="U1" pin="!DTR" pad="13"/>
<connect gate="U1" pin="!RI" pad="11"/>
<connect gate="U1" pin="!RTS" pad="14"/>
<connect gate="U1" pin="GND" pad="1"/>
<connect gate="U1" pin="R232" pad="15"/>
<connect gate="U1" pin="RXD" pad="3"/>
<connect gate="U1" pin="TXD" pad="2"/>
<connect gate="U1" pin="UD+" pad="5"/>
<connect gate="U1" pin="UD-" pad="6"/>
<connect gate="U1" pin="V3" pad="4"/>
<connect gate="U1" pin="VCC" pad="16"/>
<connect gate="U1" pin="XI" pad="7"/>
<connect gate="U1" pin="XO" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13498"/>
<attribute name="VALUE" value="CH340G"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun">
<packages>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="USB-5PIN">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
<pin name="ID"/>
<pin name="MTN1"/>
<pin name="MTN2"/>
<pin name="MTN3"/>
<pin name="MTN4"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="USB-MINIB">
<gates>
<gate name="G$1" symbol="USB-5PIN"/>
</gates>
<devices>
<device name="-5PIN" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="ID" pad="ID"/>
<connect gate="G$1" pin="MTN1" pad="MTN3"/>
<connect gate="G$1" pin="MTN2" pad="MTN1"/>
<connect gate="G$1" pin="MTN3" pad="MTN2"/>
<connect gate="G$1" pin="MTN4" pad="MTN4"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="flight_controller.lbr01_FAB_Hello">
<packages>
<package name="CSM-7X-DU">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;&lt;p&gt;
Source: www.ecsxtal.com .. Crystal 3.6864MHz CSM_7X_DU.PDF</description>
</package>
</packages>
<symbols>
<symbol name="Q">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CSM-7X-DU" prefix="Q">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;&lt;p&gt;
Source: www.ecsxtal.com .. Crystal 3.6864MHz CSM_7X_DU.PDF</description>
<gates>
<gate name="P" symbol="Q"/>
</gates>
<devices>
<device name="" package="CSM-7X-DU">
<connects>
<connect gate="P" pin="1" pad="1"/>
<connect gate="P" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="fab">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
</packages>
<symbols>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="LED">
<description>LED</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB1206" package="LED1206FAB">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="IC">
<packages>
<package name="A4988_STEP">
</package>
</packages>
<symbols>
<symbol name="A4988_STEP">
<pin name="/EN"/>
<pin name="MS1"/>
<pin name="MS2"/>
<pin name="MS3"/>
<pin name="/RST"/>
<pin name="/SLP"/>
<pin name="STEP"/>
<pin name="DIR"/>
<pin name="VMOT"/>
<pin name="GND"/>
<pin name="2B"/>
<pin name="2A"/>
<pin name="1A"/>
<pin name="1B"/>
<pin name="VDD"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="A4988_STEP">
<gates>
<gate name="G$1" symbol="A4988_STEP"/>
</gates>
<devices>
<device name="" package="A4988_STEP">
<connects>
<connect gate="G$1" pin="/EN" pad="/EN"/>
<connect gate="G$1" pin="/RST" pad="/RST"/>
<connect gate="G$1" pin="/SLP" pad="/SLP"/>
<connect gate="G$1" pin="1A" pad="1A"/>
<connect gate="G$1" pin="1B" pad="1B"/>
<connect gate="G$1" pin="2A" pad="2A"/>
<connect gate="G$1" pin="2B" pad="2B"/>
<connect gate="G$1" pin="DIR" pad="DIR"/>
<connect gate="G$1" pin="GND" pad="GND GND2"/>
<connect gate="G$1" pin="MS1" pad="MS1"/>
<connect gate="G$1" pin="MS2" pad="MS2"/>
<connect gate="G$1" pin="MS3" pad="MS3"/>
<connect gate="G$1" pin="STEP" pad="STEP"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
<connect gate="G$1" pin="VMOT" pad="VMOT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA07-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA06-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="MA07-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="MA06-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MA07-1" prefix="SV" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="MA07-1"/>
</gates>
<devices>
<device name="" package="MA07-1">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="5" pad="5"/>
<connect gate="1" pin="6" pad="6"/>
<connect gate="1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MA06-1" prefix="SV" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="MA06-1"/>
</gates>
<devices>
<device name="" package="MA06-1">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="5" pad="5"/>
<connect gate="1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="1X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X03/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="328-1" library="atmega8" deviceset="ATMEGA48/88/168" device="-AU" value="ATMEGA328P-AU"/>
<part name="CRYSTAL1" library="01_FAB_Hello" deviceset="CSM-7X-DU" device="" value="16Mhz"/>
<part name="C1" library="AVX_By_element14_Batch_1" deviceset="0612ZC225MAT2A" device="" value="18pF"/>
<part name="C2" library="AVX_By_element14_Batch_1" deviceset="0612ZC225MAT2A" device="" value="18pF"/>
<part name="R1" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="10k"/>
<part name="LED_GREEN" library="01_FAB_Hello" deviceset="LED" device="1206"/>
<part name="R2" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="499"/>
<part name="C3" library="01_SparkFun" deviceset="CAP" device="1206" value="10uF"/>
<part name="C4" library="01_SparkFun" deviceset="CAP" device="1206" value="1uF"/>
<part name="C5" library="01_SparkFun" deviceset="CAP" device="1206" value="100nF"/>
<part name="C6" library="01_SparkFun" deviceset="CAP" device="1206" value="100nF"/>
<part name="RESETS" library="con-amp-quick" deviceset="M02" device=""/>
<part name="U2" library="SparkFun-DigitalIC" deviceset="CH340G" device="SMD" value="CH340G"/>
<part name="U$7" library="SparkFun" deviceset="USB-MINIB" device="-5PIN"/>
<part name="CRYSTAL" library="flight_controller.lbr01_FAB_Hello" deviceset="CSM-7X-DU" device="" value="12MHZ"/>
<part name="C10" library="01_SparkFun" deviceset="CAP" device="1206" value="18pF"/>
<part name="C11" library="01_SparkFun" deviceset="CAP" device="1206" value="18pF"/>
<part name="C13" library="01_SparkFun" deviceset="CAP" device="1206" value="10nF"/>
<part name="R6" library="fab" deviceset="RES-US" device="1206" value="2K7"/>
<part name="R7" library="fab" deviceset="RES-US" device="1206" value="2K7"/>
<part name="R8" library="fab" deviceset="RES-US" device="1206" value="1K"/>
<part name="R9" library="fab" deviceset="RES-US" device="1206" value="1K"/>
<part name="LED_RX" library="fab" deviceset="LED" device="" value="YELLOW"/>
<part name="LED_TX" library="fab" deviceset="LED" device="" value="YELLOW"/>
<part name="5V2" library="con-amp-quick" deviceset="M03" device=""/>
<part name="5V1" library="con-amp-quick" deviceset="M03" device=""/>
<part name="GND1" library="con-amp-quick" deviceset="M03" device=""/>
<part name="GND3" library="con-amp-quick" deviceset="M03" device=""/>
<part name="SERIAL" library="con-amp-quick" deviceset="M02" device=""/>
<part name="R3" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="100k"/>
<part name="U$1" library="IC" deviceset="A4988_STEP" device=""/>
<part name="13DEC" library="con-lstb" deviceset="MA07-1" device=""/>
<part name="SV2" library="con-lstb" deviceset="MA06-1" device=""/>
<part name="LED_GREEN1" library="01_FAB_Hello" deviceset="LED" device="1206"/>
<part name="R4" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="499"/>
<part name="PD" library="pinhead" deviceset="PINHD-1X3" device=""/>
<part name="SL2" library="con-amp-quick" deviceset="M06" device=""/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="5V">
<segment>
<pinref part="328-1" gate="1" pin="VCC@1"/>
</segment>
<segment>
<pinref part="328-1" gate="1" pin="VCC@2"/>
</segment>
<segment>
<pinref part="328-1" gate="1" pin="AVCC"/>
</segment>
<segment>
<pinref part="328-1" gate="1" pin="AREF"/>
</segment>
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="LED_GREEN" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="C4" gate="G$1" pin="1"/>
<pinref part="C5" gate="G$1" pin="1"/>
<pinref part="C3" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="5V2" gate="G$1" pin="1"/>
<pinref part="5V2" gate="G$1" pin="2"/>
<pinref part="5V2" gate="G$1" pin="3"/>
<pinref part="5V1" gate="G$1" pin="1"/>
<pinref part="5V1" gate="G$1" pin="2"/>
<pinref part="5V1" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="U$7" gate="G$1" pin="VBUS"/>
</segment>
<segment>
<pinref part="U2" gate="U1" pin="VCC"/>
</segment>
<segment>
<pinref part="R6" gate="G$1" pin="2"/>
<pinref part="R7" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="R3" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="MS1"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="328-1" gate="1" pin="PB6(XTAL1/TOSC1/PCINT6)"/>
<pinref part="CRYSTAL1" gate="P" pin="2"/>
<pinref part="C1" gate="A" pin="C2"/>
</segment>
</net>
<net name="N$9">
<segment>
<pinref part="328-1" gate="1" pin="PB7(XTAL2/TOSC2/PCINT7)"/>
<pinref part="CRYSTAL1" gate="P" pin="1"/>
<pinref part="C2" gate="A" pin="C2"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="328-1" gate="1" pin="GND@1"/>
</segment>
<segment>
<pinref part="328-1" gate="1" pin="GND@2"/>
</segment>
<segment>
<pinref part="C1" gate="A" pin="C1"/>
</segment>
<segment>
<pinref part="C2" gate="A" pin="C1"/>
</segment>
<segment>
<pinref part="328-1" gate="1" pin="AGND"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="U$7" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U2" gate="U1" pin="GND"/>
</segment>
<segment>
<pinref part="C10" gate="G$1" pin="2"/>
<pinref part="C11" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C13" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND1" gate="G$1" pin="1"/>
<pinref part="GND1" gate="G$1" pin="2"/>
<pinref part="GND1" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="C4" gate="G$1" pin="2"/>
<pinref part="C5" gate="G$1" pin="2"/>
<pinref part="C3" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND3" gate="G$1" pin="1"/>
<pinref part="GND3" gate="G$1" pin="2"/>
<pinref part="GND3" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="/EN"/>
</segment>
<segment>
<pinref part="R4" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$26">
<segment>
<pinref part="LED_GREEN" gate="G$1" pin="C"/>
<pinref part="R2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="RST-FTDI">
<segment>
<pinref part="C6" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="RESETS" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="U2" gate="U1" pin="!DTR"/>
</segment>
</net>
<net name="RST">
<segment>
<pinref part="R1" gate="G$1" pin="2"/>
<pinref part="328-1" gate="1" pin="PC6(/RESET/PCINT14)"/>
<pinref part="C6" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="RESETS" gate="G$1" pin="1"/>
</segment>
</net>
<net name="TX-340">
<segment>
<pinref part="328-1" gate="1" pin="PD0(RXD/PCINT16)"/>
</segment>
<segment>
<pinref part="R8" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="SERIAL" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="U$7" gate="G$1" pin="D+"/>
<pinref part="U2" gate="U1" pin="UD+"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="U$7" gate="G$1" pin="D-"/>
<pinref part="U2" gate="U1" pin="UD-"/>
</segment>
</net>
<net name="OSC_IN">
<segment>
<pinref part="CRYSTAL" gate="P" pin="2"/>
<pinref part="C10" gate="G$1" pin="1"/>
<pinref part="U2" gate="U1" pin="XO"/>
</segment>
</net>
<net name="OSC_OUT">
<segment>
<pinref part="CRYSTAL" gate="P" pin="1"/>
<pinref part="C11" gate="G$1" pin="1"/>
<pinref part="U2" gate="U1" pin="XI"/>
</segment>
</net>
<net name="V3">
<segment>
<pinref part="U2" gate="U1" pin="V3"/>
</segment>
<segment>
<pinref part="C13" gate="G$1" pin="1"/>
</segment>
</net>
<net name="TXD">
<segment>
<pinref part="U2" gate="U1" pin="TXD"/>
</segment>
<segment>
<pinref part="LED_TX" gate="G$1" pin="C"/>
</segment>
<segment>
<pinref part="R8" gate="G$1" pin="1"/>
</segment>
</net>
<net name="RXD">
<segment>
<pinref part="U2" gate="U1" pin="RXD"/>
</segment>
<segment>
<pinref part="LED_RX" gate="G$1" pin="C"/>
</segment>
<segment>
<pinref part="R9" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$7">
<segment>
<pinref part="R6" gate="G$1" pin="1"/>
<pinref part="LED_RX" gate="G$1" pin="A"/>
</segment>
</net>
<net name="N$8">
<segment>
<pinref part="R7" gate="G$1" pin="1"/>
<pinref part="LED_TX" gate="G$1" pin="A"/>
</segment>
</net>
<net name="RX-340">
<segment>
<pinref part="R9" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="328-1" gate="1" pin="PD1(TXD/PCINT17)"/>
</segment>
<segment>
<pinref part="SERIAL" gate="G$1" pin="2"/>
</segment>
</net>
<net name="SCK">
<segment>
<pinref part="328-1" gate="1" pin="PB5(SCK/PCINT5)"/>
<pinref part="LED_GREEN1" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="13DEC" gate="1" pin="7"/>
</segment>
</net>
<net name="MISO">
<segment>
<pinref part="328-1" gate="1" pin="PB4(MISO/PCINT4)"/>
</segment>
<segment>
<pinref part="13DEC" gate="1" pin="6"/>
</segment>
</net>
<net name="MOSI">
<segment>
<pinref part="328-1" gate="1" pin="PB3(MOSI/OC2A/PCINT3)"/>
</segment>
<segment>
<pinref part="13DEC" gate="1" pin="5"/>
</segment>
</net>
<net name="PB0">
<segment>
<pinref part="328-1" gate="1" pin="PB0(ICP1/CLKO/PCINT0)"/>
</segment>
<segment>
<pinref part="13DEC" gate="1" pin="2"/>
</segment>
</net>
<net name="PB1">
<segment>
<pinref part="328-1" gate="1" pin="PB1(OC1A/PCINT1)"/>
</segment>
<segment>
<pinref part="13DEC" gate="1" pin="3"/>
</segment>
</net>
<net name="PB2">
<segment>
<pinref part="328-1" gate="1" pin="PB2(SS/OC1B/PCINT2)"/>
</segment>
<segment>
<pinref part="13DEC" gate="1" pin="4"/>
</segment>
</net>
<net name="PD7">
<segment>
<pinref part="328-1" gate="1" pin="PD7(AIN1/PCINT23)"/>
</segment>
<segment>
<pinref part="13DEC" gate="1" pin="1"/>
</segment>
</net>
<net name="PD6">
<segment>
<pinref part="328-1" gate="1" pin="PD6(AIN0/OC0A/PCINT22)"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="GND"/>
</segment>
</net>
<net name="PD5">
<segment>
<pinref part="328-1" gate="1" pin="PD5(T1/OC0B/PCINT21)"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="VMOT"/>
</segment>
</net>
<net name="PD4">
<segment>
<pinref part="328-1" gate="1" pin="PD4(T0/XCK/PCINT20)"/>
</segment>
<segment>
<pinref part="PD" gate="A" pin="3"/>
</segment>
</net>
<net name="PD3">
<segment>
<pinref part="328-1" gate="1" pin="PD3(INT1/OC2B/PCINT19)"/>
</segment>
<segment>
<pinref part="PD" gate="A" pin="2"/>
</segment>
</net>
<net name="PD2">
<segment>
<pinref part="328-1" gate="1" pin="PD2(INT0/PCINT18)"/>
</segment>
<segment>
<pinref part="PD" gate="A" pin="1"/>
</segment>
</net>
<net name="ADC7">
<segment>
<pinref part="328-1" gate="1" pin="ADC7"/>
</segment>
</net>
<net name="ADC6">
<segment>
<pinref part="328-1" gate="1" pin="ADC6"/>
</segment>
</net>
<net name="PC5">
<segment>
<pinref part="328-1" gate="1" pin="PC5(ADC5/SCL/PCINT13)"/>
</segment>
<segment>
<pinref part="SL2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="PC4">
<segment>
<pinref part="328-1" gate="1" pin="PC4(ADC4/SDA/PCINT12)"/>
</segment>
<segment>
<pinref part="SL2" gate="G$1" pin="2"/>
</segment>
</net>
<net name="PC3">
<segment>
<pinref part="328-1" gate="1" pin="PC3(ADC3/PCINT11)"/>
</segment>
<segment>
<pinref part="SL2" gate="G$1" pin="3"/>
</segment>
</net>
<net name="PC2">
<segment>
<pinref part="328-1" gate="1" pin="PC2(ADC2/PCINT10)"/>
</segment>
<segment>
<pinref part="SL2" gate="G$1" pin="4"/>
</segment>
</net>
<net name="PC1">
<segment>
<pinref part="328-1" gate="1" pin="PC1(ADC1/PCINT9)"/>
</segment>
<segment>
<pinref part="SL2" gate="G$1" pin="5"/>
</segment>
</net>
<net name="PC0">
<segment>
<pinref part="328-1" gate="1" pin="PC0(ADC0/PCINT8)"/>
<pinref part="R3" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SL2" gate="G$1" pin="6"/>
</segment>
</net>
<net name="GNDM">
<segment>
<pinref part="U$1" gate="G$1" pin="STEP"/>
</segment>
<segment>
<pinref part="SV2" gate="1" pin="2"/>
</segment>
</net>
<net name="VCCM">
<segment>
<pinref part="U$1" gate="G$1" pin="DIR"/>
</segment>
<segment>
<pinref part="SV2" gate="1" pin="1"/>
</segment>
</net>
<net name="MP1">
<segment>
<pinref part="U$1" gate="G$1" pin="MS2"/>
</segment>
<segment>
<pinref part="SV2" gate="1" pin="6"/>
</segment>
</net>
<net name="MP2">
<segment>
<pinref part="U$1" gate="G$1" pin="MS3"/>
</segment>
<segment>
<pinref part="SV2" gate="1" pin="5"/>
</segment>
</net>
<net name="MP3">
<segment>
<pinref part="U$1" gate="G$1" pin="/RST"/>
</segment>
<segment>
<pinref part="SV2" gate="1" pin="4"/>
</segment>
</net>
<net name="MP4">
<segment>
<pinref part="U$1" gate="G$1" pin="/SLP"/>
</segment>
<segment>
<pinref part="SV2" gate="1" pin="3"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="LED_GREEN1" gate="G$1" pin="C"/>
<pinref part="R4" gate="G$1" pin="1"/>
</segment>
</net>
</nets>
</sheet>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
