<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<library>
<packages>
<package name="2X03SMD">
</package>
<package name="ELECTRET_2742PBJ-A">
</package>
<package name="USB_MINIB">
</package>
<package name="SJFAB">
</package>
<package name="OP1206">
</package>
<package name="2X02SMD">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="EFOBM">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="QFN/MLF20">
<description>&lt;b&gt;HP-VFQFP-N20&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="DO41Z10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="P-LCC-4-3">
<description>&lt;b&gt;Hyper TOPLED® &lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/</description>
</package>
<package name="P-LCC-4">
<description>&lt;b&gt;Power TOPLED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LA_LY E67B.pdf</description>
</package>
<package name="TQFP32-08THIN">
</package>
<package name="JACK_2.1MM">
</package>
<package name="JACK_.65MM">
</package>
<package name="2-SMD-5X3MM">
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="R1206FAB">
</package>
<package name="C1206FAB">
</package>
<package name="1X06SMD">
</package>
<package name="MSOP">
</package>
<package name="SOIC16">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;, 5 lead</description>
</package>
<package name="S008">
<description>Small outline package</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="8-LCC">
</package>
<package name="2X05SMD">
</package>
<package name="SPDTSWITCH">
</package>
<package name="LCC16">
<description>&lt;b&gt;LCC16&lt;/b&gt; Package&lt;p&gt;
Source: http://www.memsic.com/data/products/MXR9500G&amp;M/MXR9500G&amp;M.pdf</description>
</package>
<package name="SMD_COIL">
<description>ELL-CTV series SMD choke coils
:
Panasonic Electronic Components ELL-CTV choke coils, 1.2-100uH, surface mount</description>
</package>
<package name="CSP-4PIN">
<description>Knowles SPU0414HR5H-SB

MEMS microphone, SiSonic series</description>
</package>
<package name="MIC_BOTTOM_PORT">
<description>Knowles SPH0645LM4H-B

I2S Output Digital Microphone, 18-bit precision</description>
</package>
<package name="MIC_MEMS_ANALOG_SPU0414HR5H">
<description>http://www.digikey.com/product-search/en?keywords=423-1134-1-ND%09</description>
</package>
<package name="2X04_THRU">
<description>2x4 header.  

Meant for nRF24L01+, but could be used for any header or 2x4 part.

Extra-wide pads for greater durability in soldering.</description>
</package>
<package name="ELLCTV">
</package>
<package name="PJ-002AH-SMT">
</package>
<package name="DX4R005HJ5_100">
</package>
<package name="DX4R005HJ5">
</package>
<package name="DX4R005HJ5_64">
</package>
<package name="AYZ0102AGRLC">
</package>
<package name="3.5MMTERM">
</package>
<package name="ED555DS-2DS">
</package>
<package name="ED555DS-3DS">
</package>
<package name="MINI-SMA">
<description>mini-SMA diode</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="SOIC8_PAD">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="TQFP44-13THIN">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
<package name="QFN-44-7X7">
<description>&lt;b&gt;QFN-44&lt;/b&gt; (7x7x1.8mm)&lt;p&gt;
Source: http://www.st.com/stonline/products/literature/ds/11020.pdf</description>
</package>
<package name="LQFP48">
<description>&lt;b&gt;48-pin plastic LQFP (FPT-48P-M26)&lt;/b&gt;&lt;p&gt;
www.fma.fujitsu.com/pdf/e713717.pdf</description>
</package>
<package name="TQFP100-14X14">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt; 14x14 mm&lt;p&gt;</description>
</package>
<package name="MSOP8">
<description>&lt;b&gt;8M, 8-Lead, 0.118" Wide, Miniature Small Outline Package&lt;/b&gt;&lt;p&gt;
MSOP&lt;br&gt;
8M-Package doc1097.pdf</description>
</package>
<package name="2X3-SHROUDED">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3_SMT_POSTS">
<description>&lt;h3&gt;Surface Mount - 2x3 Male Header with Keying Posts&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/15881.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3_POGO">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Pogo Pins&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3-NS">
<description>&lt;h3&gt;Plated Through Hole - 2x3 No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3_SMD">
<description>&lt;h3&gt;Surface Mount - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:2.54mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X4">
<description>&lt;h3&gt;Plated Through Hole - 2x4&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X4-SHROUDED">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PMA-B">
<description>&lt;b&gt;SMD SHUNT RESISTOR&lt;/b&gt;</description>
</package>
<package name="WSL2726">
<description>&lt;b&gt;SMD SHUNT RESISTOR&lt;/b&gt;</description>
</package>
<package name="HTSSOP-56">
</package>
<package name="BFC">
</package>
<package name="PWRPAD_4MM">
</package>
<package name="PWRPAD_2-5MM">
</package>
<package name="C2220">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="CBA-SILK-LOGO">
</package>
<package name="MK-LOGO-SILK">
</package>
<package name="TSSOP20-08THIN">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 20&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="2X4-SHROUDED-SQUISH">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5_1.27MM_SMD">
</package>
<package name="2X5_1.27MM_PTH">
</package>
<package name="TC2050-IDC">
</package>
<package name="2X5">
<description>&lt;h3&gt;Plated Through Hole - 2x5&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-RA">
<description>&lt;h3&gt;Plated Through Hole - 2x5 Right Angle Male Headers&lt;/h3&gt;
tDocu shows pin location. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-RAF">
<description>&lt;h3&gt;Plated Through Hole - 2x5 Right Angle Female Header&lt;/h3&gt;
Silk outline of pins
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-SHROUDED">
<description>&lt;h3&gt;Plated Through Hole - 2x5 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-SHROUDED_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 2x5 Shrouded Header Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-SHROUDED_SMD">
<description>&lt;h3&gt;Surface Mount - 2x5 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5_NOSILK">
<description>&lt;h3&gt;Plated Through Hole - 2x5 No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5_PTH_SILK_.05">
<description>&lt;h3&gt;Plated Through Hole - 2x5&lt;/h3&gt;
Holes are 0.05". 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-SHROUDED-NS">
<description>&lt;h3&gt;Plated Through Hole - 2x5 Shrouded Header No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MSOP8-8MILPADS">
<description>&lt;b&gt;8M, 8-Lead, 0.118" Wide, Miniature Small Outline Package&lt;/b&gt;&lt;p&gt;
MSOP&lt;br&gt;
8M-Package doc1097.pdf</description>
</package>
<package name="QFN-16-3X3">
<description>&lt;b&gt;16-Lead Plastic QFN (3mm × 3mm)&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 44&lt;/i&gt;&lt;br&gt;
&lt;br&gt;
Source: http://cds.linear.com/docs/en/datasheet/3645f.pdf&lt;br&gt;</description>
</package>
<package name="QFN-16-3X3-1-100">
<description>&lt;b&gt;16-Lead Plastic QFN (3mm × 3mm)&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 44&lt;/i&gt;&lt;br&gt;
&lt;br&gt;
Source: http://cds.linear.com/docs/en/datasheet/3645f.pdf&lt;br&gt;</description>
</package>
<package name="TQFP64_14X14MM-013THIN">
<description>64-Lead TQFP Plastic Thin Quad Flatpack - 14x14x1mm Body</description>
</package>
</packages>
<symbols>
<symbol name="ELECTRET">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="SJFAB">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="PHOTOTRANSISTOR">
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PINH2X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="AVRISP">
<pin name="MISO" direction="pas" function="dot"/>
<pin name="VCC" direction="pas" function="dot"/>
<pin name="SCK" direction="pas" function="dot"/>
<pin name="MOSI" direction="pas" function="dot"/>
<pin name="RST" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
</symbol>
<symbol name="TS2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
<symbol name="ATTINY45">
<pin name="GND"/>
<pin name="PB5/PCINT5/-RESET/ADC0/DW"/>
<pin name="PB3/PCINT3/XTAL1/CLKI/-OC1B/ADC3"/>
<pin name="PB4/PCINT4/XTAL2/CLKO/OC1B/ADC2"/>
<pin name="VCC"/>
<pin name="SCK/USCK/SCL/ADC1/T0/INT0/PCINT2/PB2"/>
<pin name="MISO/DO/AIN1/OC0B/OC1A/PCINT1/PB1"/>
<pin name="MOSI/DI/SDA/AIN0/OC0A/-OC1A/AREF/PCINT0/PB0"/>
</symbol>
<symbol name="N_MOSFET">
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="D">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="REGULATOR">
<pin name="IN"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="CERAMIC_RESONATOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="ATTINY24/44/84">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="(PCINT7/ICP/OC0B/ADC7)PA7"/>
<pin name="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6"/>
<pin name="(PCINT5/OC1B/MISO/DO/ADC5)PA5"/>
<pin name="(PCINT4/T1/SCL/USCK/ADC4)PA4"/>
<pin name="(PCINT3/T0/ADC3)PA3"/>
<pin name="(PCINT2/AIN1/ADC2)PA2"/>
<pin name="(PCINT1/AIN0/ADC1)PA1"/>
<pin name="(PCINT0/AREF/ADC0)PA0"/>
<pin name="(PCINT11/RESET/DW)PB3"/>
<pin name="(PCINT10/INT0/OC0A/CKOUT)PB2"/>
<pin name="(PCINT9/XTAL2)PB1"/>
<pin name="(PCINT8/XTAL1/CLKI)PB0"/>
</symbol>
<symbol name="P_MOSFET">
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="ZENER">
<pin name="ANODE" direction="pas"/>
<pin name="CATHODE" direction="pas"/>
</symbol>
<symbol name="LED-RGB">
<pin name="CGREEN" direction="pas"/>
<pin name="CBLUE" direction="pas"/>
<pin name="CRED" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="23-I/O">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="JACK">
<pin name="PIN"/>
<pin name="CONTACT"/>
<pin name="SHUNT"/>
</symbol>
<symbol name="CRYSTAL">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="C-US">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="FTDI">
<pin name="GND"/>
<pin name="CTS"/>
<pin name="VCC"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="RTS"/>
</symbol>
<symbol name="A4953-H-BRIDGE-MOTOR-DRIVER">
<pin name="GND"/>
<pin name="IN2"/>
<pin name="IN1"/>
<pin name="VREF"/>
<pin name="VBB"/>
<pin name="OUT1"/>
<pin name="LSS"/>
<pin name="OUT2"/>
</symbol>
<symbol name="12-BIT_ADC">
<pin name="CS"/>
<pin name="CH0"/>
<pin name="CH1"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="CLK"/>
<pin name="DOUT"/>
<pin name="DIN"/>
</symbol>
<symbol name="12-BIT_ADC_8CH">
<pin name="CH0"/>
<pin name="CH1"/>
<pin name="CH2"/>
<pin name="CH3"/>
<pin name="CH4"/>
<pin name="CH5"/>
<pin name="CH6"/>
<pin name="CH7"/>
<pin name="VDD"/>
<pin name="VREF"/>
<pin name="AGND"/>
<pin name="CLK"/>
<pin name="DOUT"/>
<pin name="DIN"/>
<pin name="CS"/>
<pin name="DGND"/>
</symbol>
<symbol name="LED">
<description>LED</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="CAP-NONPOLARIZED">
<description>non-polarized capacitor</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="OPAMP">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MXD6235M">
<pin name="PD"/>
<pin name="TP"/>
<pin name="GND" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="Y_OUT"/>
<pin name="X_OUT"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PINH2X5">
<pin name="1" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="SPDTSWITCH">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="ACCEL_MXR9150MZ">
<description>Three-axis surface-mount 3.3V accelerometer</description>
<pin name="DI1"/>
<pin name="VDD1"/>
<pin name="VSA2"/>
<pin name="DI2"/>
<pin name="SCK2"/>
<pin name="ZOUT"/>
<pin name="VDD3"/>
<pin name="XOUT"/>
<pin name="YOUT"/>
<pin name="VDD2"/>
<pin name="VSA1"/>
<pin name="SCK1"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="MEMS_MIC_ANALOG">
<description>Knowles SPU0414HR5H-SB

Amplified SiSonic (TM) Microphone</description>
<pin name="OUT"/>
<pin name="GND"/>
<pin name="GAIN"/>
<pin name="VDD"/>
</symbol>
<symbol name="MEMS_MIC_I2S">
<pin name="VDD"/>
<pin name="WS"/>
<pin name="CLK"/>
<pin name="DATA"/>
<pin name="SEL"/>
<pin name="GND"/>
</symbol>
<symbol name="MIC_MEMS_ANALOG_SPU0414HR5H">
<description>http://www.digikey.com/product-search/en?keywords=423-1134-1-ND%09</description>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="GAIN"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="ATMEGA16U2">
<description>ATmega8U2/16U2/32U2 USB microcontroller</description>
<pin name="UCAP"/>
<pin name="UGND"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="UVCC"/>
<pin name="AVCC"/>
<pin name="XTAL1"/>
<pin name="(PC0)XTAL2"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="(PCINT10)PC4"/>
<pin name="(PCINT9/OC.1B)PC5"/>
<pin name="(PC1/DW)!RESET"/>
<pin name="(OC.1A/PCINT8)PC6"/>
<pin name="(INT4/ICP1/CLKO)PC7"/>
<pin name="(PCINT7/OC.0A/OC.1C)PB7"/>
<pin name="(PCINT6)PB6"/>
<pin name="(PCINT5)PB5"/>
<pin name="(T1/PCINT4)PB4"/>
<pin name="(PDO/MISO/PCINT3)PB3"/>
<pin name="(PDI/MOSI/PCINT2)PB2"/>
<pin name="(SCLK/PCINT1)PB1"/>
<pin name="(!SS!/PCINT0)PB0"/>
<pin name="(!CTS!/!HWB!/AIN6/T0/INT7)PD7"/>
<pin name="(!RTS!/AIN5/INT6)PD6"/>
<pin name="(XCK/AIN4/PCINT12)PD5"/>
<pin name="(PCINT11/AIN2)PC2"/>
<pin name="(OC.0B/INT0)PD0"/>
<pin name="(AIN0/INT1)PD1"/>
<pin name="(RXD1/AIN1/INT2)PD2"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(INT5/AIN3)PD4"/>
</symbol>
<symbol name="NRF24L01+">
<description>nRF24L01+ 2.4GHz Wireless transceiver module</description>
<pin name="GND"/>
<pin name="CE"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="VCC"/>
<pin name="CSN"/>
<pin name="MOSI"/>
<pin name="IRQ"/>
</symbol>
<symbol name="COIL">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="DC-POWER-JACK">
<pin name="PIN1" direction="pwr"/>
<pin name="SHUNT" direction="pwr"/>
<pin name="CONTACT" direction="pwr"/>
<pin name="PIN2" direction="pwr"/>
</symbol>
<symbol name="USB-1">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
</symbol>
<symbol name="SWITCH-SPDT">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
</symbol>
<symbol name="1X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="1X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="DIODE">
<pin name="KATHODE"/>
<pin name="ANODE"/>
</symbol>
<symbol name="78ADJ">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OUT@1" direction="out"/>
</symbol>
<symbol name="ATXMEGA_A4U">
<pin name="PE0/SDA"/>
<pin name="PE1/XCK0/SCL"/>
<pin name="PE2/RXD0"/>
<pin name="PE3/TXD0"/>
<pin name="PD7/TXD1/SCK/DP"/>
<pin name="PD6/RXD1/MISO/DM"/>
<pin name="PD5/XCK1/MOSI"/>
<pin name="PD4/CS"/>
<pin name="PD3/TXD0"/>
<pin name="PD2/RXD0"/>
<pin name="PD1/XCK0"/>
<pin name="PD0"/>
<pin name="PC7/TXD1/SCK"/>
<pin name="PC6/RXD1/MISO"/>
<pin name="PC5/XCK1/MOSI"/>
<pin name="PC4/CS"/>
<pin name="PC3/TXD0"/>
<pin name="PC2/RXD0"/>
<pin name="PC1/SCL/XCK0"/>
<pin name="PC0/SDA"/>
<pin name="PB3"/>
<pin name="PB2"/>
<pin name="PB1"/>
<pin name="PB0"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="PR0(XT2)"/>
<pin name="PR1(XT1)"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PDI_DATA"/>
<pin name="GND2" direction="pwr"/>
<pin name="!RESET!/PDI_CLK"/>
</symbol>
<symbol name="ATSAM4N8A">
<pin name="ADVREFP"/>
<pin name="GND_1"/>
<pin name="PB0/AD4"/>
<pin name="PB1/AD5"/>
<pin name="PB2/AD6"/>
<pin name="PB3/AD7"/>
<pin name="VDDIN"/>
<pin name="VDDOUT"/>
<pin name="PA17/PGMD5/AD0"/>
<pin name="PA18/PGMD6/AD1"/>
<pin name="PA19/PGMD7/AD2"/>
<pin name="PA20/AD3"/>
<pin name="VDDIO_1"/>
<pin name="PA16/PGMD4"/>
<pin name="PA15/PGMD3"/>
<pin name="PA14/PGMD2"/>
<pin name="PA13/PGMD1"/>
<pin name="VDDCORE_1"/>
<pin name="PA12/PGMD0"/>
<pin name="PA11/PGMM3"/>
<pin name="PA10/PGMM2"/>
<pin name="PA9/PGMM1"/>
<pin name="PA8/XOUT32/PGMM0"/>
<pin name="PA7/XIN32/PGMNVALID"/>
<pin name="TDI/PB4"/>
<pin name="PA6/PGMNOE"/>
<pin name="PA5/PGMRDY"/>
<pin name="PA5/PGMNCMD"/>
<pin name="NRST"/>
<pin name="TST"/>
<pin name="PA3"/>
<pin name="PA2/PGMEN2"/>
<pin name="VDDIO_2"/>
<pin name="GND_2"/>
<pin name="PA1/PGMEN1"/>
<pin name="PA0/PGMEN0"/>
<pin name="TDO/TRACESWO/PB5"/>
<pin name="JTAGSEL"/>
<pin name="TMS/SWDIO/PB6"/>
<pin name="TCK/SWCLK/PB7"/>
<pin name="VDDCORE_2"/>
<pin name="ERASE/PB12"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="XOUT/PB8"/>
<pin name="XIN/P/PB9/GMCK"/>
<pin name="VDDIO_3"/>
<pin name="VDDPLL"/>
</symbol>
<symbol name="ATSAMS70N">
<pin name="PA0/I2SC0_MCK"/>
<pin name="PA1/I2SC0_CK"/>
<pin name="PA2"/>
<pin name="PA3/TWD0"/>
<pin name="PA4/UTXD1/TWCK0"/>
<pin name="PA5/URXD1"/>
<pin name="PA7/XIN32"/>
<pin name="PA8/XOUT32"/>
<pin name="PA9/URXD0"/>
<pin name="PA10/UTXD0"/>
<pin name="PA11/PWMC0_PWMH0"/>
<pin name="PA12/PWMC0_PWMH1"/>
<pin name="PA13/PWMC0_PWMH2"/>
<pin name="PA14/WMC0_PWMH3"/>
<pin name="PA15/PWMC0_PWML3"/>
<pin name="PA16/PWMC0_PWML2"/>
<pin name="PA17/AFE0_AD6"/>
<pin name="PA18/AFE0_AD7"/>
<pin name="PA19/PWMC0_PWML0/AFE0_AD8"/>
<pin name="PA20/PWMC0_PWML1/AFE0_AD9"/>
<pin name="PA21/AFE0_AD1"/>
<pin name="PA22"/>
<pin name="PA23"/>
<pin name="PA24"/>
<pin name="PA25"/>
<pin name="PA26"/>
<pin name="PA27"/>
<pin name="PA28"/>
<pin name="PA30"/>
<pin name="PA31/SPI0_NPCS1"/>
<pin name="PB0/RXD0"/>
<pin name="PB1/TXD0"/>
<pin name="PB2/SPI0_NPCS0/CTS0"/>
<pin name="PB3/RTS0"/>
<pin name="PB4/TDI/TWD1"/>
<pin name="PB5/TDO/TWCK1"/>
<pin name="PB6/SWDIO/TMS"/>
<pin name="PB7/SWCLK/TCK"/>
<pin name="PB8/XOUT"/>
<pin name="PB9/XIN"/>
<pin name="PB12/ERASE"/>
<pin name="PB13/DAC0/SCK0"/>
<pin name="PD1/PWMC1_PWMH0"/>
<pin name="PD2/PWMC1_PWML1"/>
<pin name="PD3/PWMC1_PWMH1"/>
<pin name="PD4/PWMC1_PWML2"/>
<pin name="PD5/PWMC1_PWMH2"/>
<pin name="PD6/PWMC1_PWML3"/>
<pin name="PD7/PWMC1_PWMH3"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="PD10/PWMC0_PWML0"/>
<pin name="PD11/PWMC0_PWMH0"/>
<pin name="PD12/SPI0_NPCS2"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PD16"/>
<pin name="PD17"/>
<pin name="PD18/URXD4"/>
<pin name="PD19/UTXD4"/>
<pin name="PD20/SPI0_MISO"/>
<pin name="PD21/SPI0_MOSI"/>
<pin name="PD22_SPI0_SPCK"/>
<pin name="PD24"/>
<pin name="PD25/URXD2"/>
<pin name="PD26/UTXD2"/>
<pin name="PD27/SPI0_NPCS3/TWD2"/>
<pin name="PD28/URXD3/TWCK2"/>
<pin name="PD30/UTXD3"/>
<pin name="PD31"/>
<pin name="PD0/DAC1/PWMC1_PWML0"/>
<pin name="VDDIO1"/>
<pin name="VDDIO2"/>
<pin name="VDDIO3"/>
<pin name="VDDIO4"/>
<pin name="JTAGSEL"/>
<pin name="TST"/>
<pin name="VREFP"/>
<pin name="NRST"/>
<pin name="VDDOUT"/>
<pin name="VDDIN"/>
<pin name="VREFN"/>
<pin name="USB_DP"/>
<pin name="USB_DM"/>
<pin name="VDDPLL"/>
<pin name="VDDUTMII"/>
<pin name="VDDUTMIC"/>
<pin name="VBG"/>
<pin name="GND6"/>
<pin name="GND5"/>
<pin name="VDDCORE1"/>
<pin name="VDDCORE2"/>
<pin name="VDDCORE3"/>
<pin name="VDDCORE4"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="VDDPLLUSB"/>
</symbol>
<symbol name="ISL3177E">
<pin name="VCC"/>
<pin name="RO"/>
<pin name="DI"/>
<pin name="GND"/>
<pin name="A"/>
<pin name="B"/>
<pin name="Z"/>
<pin name="Y"/>
</symbol>
<symbol name="REGULATOR_SOT223">
<pin name="IN"/>
<pin name="GND"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
</symbol>
<symbol name="CONN_03X2">
<description>&lt;h3&gt;6 Pin Connection&lt;/h3&gt;
3x2 pin layout</description>
<pin name="1"/>
<pin name="3"/>
<pin name="5"/>
<pin name="6"/>
<pin name="4"/>
<pin name="2"/>
</symbol>
<symbol name="CONN_04X2">
<description>&lt;h3&gt;8 Pin Connection&lt;/h3&gt;
4x2 pin layout</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="R-4">
<pin name="SB" direction="pas"/>
<pin name="SA" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="WSL2726">
<pin name="SB" direction="pas"/>
<pin name="SA" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="DRV8302">
<pin name="RT_CLK"/>
<pin name="COMP"/>
<pin name="VSENSE"/>
<pin name="PWRGND"/>
<pin name="NOCTW"/>
<pin name="NFAULT"/>
<pin name="DTC"/>
<pin name="M_PWM"/>
<pin name="M_OC"/>
<pin name="GAIN"/>
<pin name="OC_ADJ"/>
<pin name="DC_CAL"/>
<pin name="GVDD"/>
<pin name="CP1"/>
<pin name="CP2"/>
<pin name="EN_GATE"/>
<pin name="INH_A"/>
<pin name="INL_A"/>
<pin name="INH_B"/>
<pin name="INL_B"/>
<pin name="INH_C"/>
<pin name="INL_C"/>
<pin name="DVDD"/>
<pin name="REF"/>
<pin name="SO1"/>
<pin name="SO2"/>
<pin name="AVDD"/>
<pin name="AGND"/>
<pin name="PVDD1"/>
<pin name="SP2"/>
<pin name="SN2"/>
<pin name="SP1"/>
<pin name="SN1"/>
<pin name="SL_C"/>
<pin name="GL_C"/>
<pin name="SH_C"/>
<pin name="GH_C"/>
<pin name="BST_C"/>
<pin name="SL_B"/>
<pin name="GL_B"/>
<pin name="SH_B"/>
<pin name="GH_B"/>
<pin name="BST_B"/>
<pin name="SL_A"/>
<pin name="GL_A"/>
<pin name="SH_A"/>
<pin name="GH_A"/>
<pin name="BST_A"/>
<pin name="BIAS"/>
<pin name="PH1"/>
<pin name="PH2"/>
<pin name="BST_BK"/>
<pin name="PVDD2-1"/>
<pin name="PVDD2-2"/>
<pin name="EN_BUCK"/>
<pin name="SS_TR"/>
<pin name="GNDPAD"/>
</symbol>
<symbol name="PWRPAD">
<pin name="PWRPAD"/>
</symbol>
<symbol name="AS5304-6">
<pin name="VSS"/>
<pin name="A"/>
<pin name="VDDP"/>
<pin name="B"/>
<pin name="TEST1"/>
<pin name="AO"/>
<pin name="VDD"/>
<pin name="INDEX"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="TEST2"/>
<pin name="TEST3"/>
<pin name="TEST4"/>
<pin name="TEST_GND"/>
<pin name="VDDA"/>
<pin name="TEST5"/>
<pin name="TEST6"/>
<pin name="TEST7"/>
<pin name="ZPZ"/>
</symbol>
<symbol name="ARM_SWD_10">
<pin name="VCC"/>
<pin name="GND@3"/>
<pin name="GND@5"/>
<pin name="GND@7"/>
<pin name="GND@9"/>
<pin name="NRESET"/>
<pin name="NC/TDI"/>
<pin name="SWO/TDO"/>
<pin name="SWDCLK/TCK"/>
<pin name="SWDIO/TMS"/>
</symbol>
<symbol name="CONN_05X2">
<description>&lt;h3&gt;10 Pin Connection&lt;/h3&gt;
5x2 pin layout</description>
<pin name="10" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="XR21V410-USB-UART">
<pin name="GND1"/>
<pin name="LOWPOWER"/>
<pin name="GPIO5"/>
<pin name="GPIO4"/>
<pin name="GPIO3"/>
<pin name="GPIO2"/>
<pin name="GPIO1"/>
<pin name="GPIO0"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GND2"/>
<pin name="USBD-"/>
<pin name="USBD+"/>
<pin name="VCC"/>
<pin name="GND_PAD"/>
</symbol>
<symbol name="ATXMEGA_A3U">
<pin name="RESET/PDI_CLK"/>
<pin name="PDI_DATA"/>
<pin name="AVCC"/>
<pin name="VCC@1"/>
<pin name="VCC@2"/>
<pin name="VCC@3"/>
<pin name="VCC@4"/>
<pin name="VCC@5"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="PR0/XTAL2"/>
<pin name="PR1/XTAL1"/>
<pin name="PA0/AREF"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0/AREF"/>
<pin name="PB1"/>
<pin name="PB2/DAC0"/>
<pin name="PB3/DAC1"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PC0/SDA"/>
<pin name="PC1/SCL/XCK0"/>
<pin name="PC2/RXD0"/>
<pin name="PC3/TXD0"/>
<pin name="PC4/SS"/>
<pin name="PC5/XCK1/MOSI"/>
<pin name="PC6/RXD1/MISO"/>
<pin name="PC7/TXD1/SCK"/>
<pin name="PD0"/>
<pin name="PD1/XCK0"/>
<pin name="PD2/RXD0"/>
<pin name="PD3/TXD0"/>
<pin name="PD4/SS"/>
<pin name="PD5/XCK/MOSI"/>
<pin name="PD6/RXD1/MISO/D-"/>
<pin name="PD7/TXD1/SCK/D+"/>
<pin name="PE0/SDA"/>
<pin name="PE1/SCL/XCK0"/>
<pin name="PE2/RXD0"/>
<pin name="PE3/TXD0"/>
<pin name="PE4/SS"/>
<pin name="PE5/XCK1/MOSI"/>
<pin name="PE6/RXD1/MISO"/>
<pin name="PE7/TXD1/SCK"/>
<pin name="PF0"/>
<pin name="PF1/XCK0"/>
<pin name="PF2/RXD0"/>
<pin name="PF3/TXD0"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ELECTRET">
<gates>
<gate name="G$1" symbol="ELECTRET"/>
</gates>
<devices>
<device name="" package="ELECTRET_2742PBJ-A">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_MINIB">
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="" package="USB_MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SHIELD" pad="SHIELD@1 SHIELD@2 SHIELD@3 SHIELD@4"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDER_JUMPER">
<gates>
<gate name="G$1" symbol="SJFAB"/>
</gates>
<devices>
<device name="" package="SJFAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PHOTOTRANSISTOR-NPN">
<gates>
<gate name="G$1" symbol="PHOTOTRANSISTOR"/>
</gates>
<devices>
<device name="1206" package="OP1206">
<connects>
<connect gate="G$1" pin="C" pad="COLLECTOR"/>
<connect gate="G$1" pin="E" pad="EMITTER"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X2-SMD">
<gates>
<gate name="G$1" symbol="PINH2X2"/>
</gates>
<devices>
<device name="" package="2X02SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X3-SMD" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X3"/>
</gates>
<devices>
<device name="" package="2X03SMD">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVRISP">
<gates>
<gate name="G$1" symbol="AVRISP"/>
</gates>
<devices>
<device name="SMD" package="2X03SMD">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="2X03">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6MM_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
<gates>
<gate name="2" symbol="TS2"/>
</gates>
<devices>
<device name="6MM_SWITCH" package="6MM_SWITCH">
<connects>
<connect gate="2" pin="P" pad="1"/>
<connect gate="2" pin="P1" pad="2"/>
<connect gate="2" pin="S" pad="3"/>
<connect gate="2" pin="S1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY45">
<gates>
<gate name="G$1" symbol="ATTINY45"/>
</gates>
<devices>
<device name="SI" package="SOIC8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="MISO/DO/AIN1/OC0B/OC1A/PCINT1/PB1" pad="6"/>
<connect gate="G$1" pin="MOSI/DI/SDA/AIN0/OC0A/-OC1A/AREF/PCINT0/PB0" pad="5"/>
<connect gate="G$1" pin="PB3/PCINT3/XTAL1/CLKI/-OC1B/ADC3" pad="2"/>
<connect gate="G$1" pin="PB4/PCINT4/XTAL2/CLKO/OC1B/ADC2" pad="3"/>
<connect gate="G$1" pin="PB5/PCINT5/-RESET/ADC0/DW" pad="1"/>
<connect gate="G$1" pin="SCK/USCK/SCL/ADC1/T0/INT0/PCINT2/PB2" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NMOSFET" prefix="T" uservalue="yes">
<description>&lt;b&gt;MOS FET&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="N_MOSFET"/>
</gates>
<devices>
<device name="SOT23" package="SOT-23">
<connects>
<connect gate="A" pin="D" pad="1"/>
<connect gate="A" pin="G" pad="3"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO252" package="TO252">
<connects>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE" prefix="D" uservalue="yes">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
high speed (Philips)</description>
<gates>
<gate name="G$1" symbol="D"/>
</gates>
<devices>
<device name="SOD123" package="SOD123">
<connects>
<connect gate="G$1" pin="A" pad="ANODE"/>
<connect gate="G$1" pin="C" pad="CATHODE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REGULATOR" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="REGULATOR"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR">
<gates>
<gate name="G$1" symbol="CERAMIC_RESONATOR"/>
</gates>
<devices>
<device name="" package="EFOBM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY44" prefix="IC">
<gates>
<gate name="1" symbol="ATTINY24/44/84"/>
</gates>
<devices>
<device name="-SSU" package="SOIC14">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="4"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="1" pin="GND" pad="14"/>
<connect gate="1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PU" package="DIL14">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="4"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="1" pin="GND" pad="14"/>
<connect gate="1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MU" package="QFN/MLF20">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="5"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="4"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="14"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="13"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="3"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="2"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="1"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="20"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="16"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="15"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="11"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="12"/>
<connect gate="1" pin="GND" pad="8"/>
<connect gate="1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMOSFET" prefix="T" uservalue="yes">
<description>&lt;b&gt;MOS FET&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="P_MOSFET"/>
</gates>
<devices>
<device name="SOT23" package="SOT-23">
<connects>
<connect gate="A" pin="D" pad="1"/>
<connect gate="A" pin="G" pad="3"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZENER_DIODE" prefix="D" uservalue="yes">
<description>zener diode</description>
<gates>
<gate name="1" symbol="ZENER"/>
</gates>
<devices>
<device name="DO41Z10" package="DO41Z10">
<connects>
<connect gate="1" pin="ANODE" pad="A"/>
<connect gate="1" pin="CATHODE" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD123" package="SOD123">
<connects>
<connect gate="1" pin="ANODE" pad="ANODE"/>
<connect gate="1" pin="CATHODE" pad="CATHODE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LEDRGBOLD" prefix="LED" uservalue="yes">
<description>&lt;b&gt;OSRAM&lt;/b&gt;&lt;p&gt;
&lt;u&gt;Hyper Multi TOPLED® Hyper-Bright LED&lt;/u&gt;&lt;br&gt;
LATB T686&lt;br&gt;

&lt;p&gt;
Source: http://www.osram.convergy.de/</description>
<gates>
<gate name="G$1" symbol="LED-RGB"/>
</gates>
<devices>
<device name="" package="P-LCC-4-3">
<connects>
<connect gate="G$1" pin="A2" pad="A"/>
<connect gate="G$1" pin="CBLUE" pad="B"/>
<connect gate="G$1" pin="CGREEN" pad="G"/>
<connect gate="G$1" pin="CRED" pad="R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LEDRGBNEW" prefix="D">
<gates>
<gate name="G$1" symbol="LED-RGB"/>
</gates>
<devices>
<device name="" package="P-LCC-4">
<connects>
<connect gate="G$1" pin="A2" pad="A"/>
<connect gate="G$1" pin="CBLUE" pad="B"/>
<connect gate="G$1" pin="CGREEN" pad="G"/>
<connect gate="G$1" pin="CRED" pad="R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA88-THIN" prefix="IC">
<gates>
<gate name="G$1" symbol="23-I/O"/>
</gates>
<devices>
<device name="" package="TQFP32-08THIN">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JACK" prefix="J">
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="2.1MM" package="JACK_2.1MM">
<connects>
<connect gate="G$1" pin="CONTACT" pad="CONTACT"/>
<connect gate="G$1" pin="PIN" pad="PIN"/>
<connect gate="G$1" pin="SHUNT" pad="SHUNT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=".65MM" package="JACK_.65MM">
<connects>
<connect gate="G$1" pin="CONTACT" pad="SHUNT"/>
<connect gate="G$1" pin="PIN" pad="PIN"/>
<connect gate="G$1" pin="SHUNT" pad="CONTACT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL">
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="2-SMD-5X3MM">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-US" prefix="C">
<gates>
<gate name="G$1" symbol="C-US"/>
</gates>
<devices>
<device name="1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206K" package="C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="C1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTDI-SMD-HEADER">
<gates>
<gate name="G$1" symbol="FTDI"/>
</gates>
<devices>
<device name="" package="1X06SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RTS" pad="6"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TXD" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A4953-H-BRIDGE-MOTOR-DRIVER">
<gates>
<gate name="G$1" symbol="A4953-H-BRIDGE-MOTOR-DRIVER"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="IN2" pad="2"/>
<connect gate="G$1" pin="LSS" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT2" pad="8"/>
<connect gate="G$1" pin="VBB" pad="5"/>
<connect gate="G$1" pin="VREF" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12-BIT_DUAL_ADC_MSOP">
<gates>
<gate name="G$1" symbol="12-BIT_ADC"/>
</gates>
<devices>
<device name="" package="MSOP">
<connects>
<connect gate="G$1" pin="CH0" pad="P$2"/>
<connect gate="G$1" pin="CH1" pad="P$3"/>
<connect gate="G$1" pin="CLK" pad="P$7"/>
<connect gate="G$1" pin="CS" pad="P$1"/>
<connect gate="G$1" pin="DIN" pad="P$5"/>
<connect gate="G$1" pin="DOUT" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$8"/>
<connect gate="G$1" pin="VSS" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12-BIT_ADC_8CH_SOIC">
<gates>
<gate name="G$1" symbol="12-BIT_ADC_8CH"/>
</gates>
<devices>
<device name="" package="SOIC16">
<connects>
<connect gate="G$1" pin="AGND" pad="14"/>
<connect gate="G$1" pin="CH0" pad="1"/>
<connect gate="G$1" pin="CH1" pad="2"/>
<connect gate="G$1" pin="CH2" pad="3"/>
<connect gate="G$1" pin="CH3" pad="4"/>
<connect gate="G$1" pin="CH4" pad="5"/>
<connect gate="G$1" pin="CH5" pad="6"/>
<connect gate="G$1" pin="CH6" pad="7"/>
<connect gate="G$1" pin="CH7" pad="8"/>
<connect gate="G$1" pin="CLK" pad="13"/>
<connect gate="G$1" pin="CS" pad="10"/>
<connect gate="G$1" pin="DGND" pad="9"/>
<connect gate="G$1" pin="DIN" pad="11"/>
<connect gate="G$1" pin="DOUT" pad="12"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREF" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB1206" package="LED1206FAB">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-UNPOLARIZED" prefix="C" uservalue="yes">
<gates>
<gate name="&gt;NAME" symbol="CAP-NONPOLARIZED"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB" package="C1206FAB">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2220" package="C2220">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPAMP" prefix="IC">
<description>&lt;b&gt;Rail-to-Rail Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Single-Supply, MicroAmplifier(TM) Series</description>
<gates>
<gate name="G$1" symbol="OPAMP"/>
</gates>
<devices>
<device name="SOT23-5" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO08" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MXD6235M">
<gates>
<gate name="G$1" symbol="MXD6235M"/>
</gates>
<devices>
<device name="-SMD" package="8-LCC">
<connects>
<connect gate="G$1" pin="GND" pad="P$3"/>
<connect gate="G$1" pin="NC" pad="P$4"/>
<connect gate="G$1" pin="NC2" pad="P$5"/>
<connect gate="G$1" pin="PD" pad="P$1"/>
<connect gate="G$1" pin="TP" pad="P$2"/>
<connect gate="G$1" pin="VDD" pad="P$8"/>
<connect gate="G$1" pin="X_OUT" pad="P$7"/>
<connect gate="G$1" pin="Y_OUT" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X5-SMD">
<gates>
<gate name="G$1" symbol="PINH2X5"/>
</gates>
<devices>
<device name="" package="2X05SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPDTSWITCH">
<gates>
<gate name="G$1" symbol="SPDTSWITCH"/>
</gates>
<devices>
<device name="" package="SPDTSWITCH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACCEL_MXR9150MZ">
<description>3-axis 3.3V accelerometer</description>
<gates>
<gate name="G$1" symbol="ACCEL_MXR9150MZ"/>
</gates>
<devices>
<device name="" package="LCC16">
<connects>
<connect gate="G$1" pin="DI1" pad="5"/>
<connect gate="G$1" pin="DI2" pad="16"/>
<connect gate="G$1" pin="SCK1" pad="6"/>
<connect gate="G$1" pin="SCK2" pad="15"/>
<connect gate="G$1" pin="VDD1" pad="4"/>
<connect gate="G$1" pin="VDD2" pad="11"/>
<connect gate="G$1" pin="VDD3" pad="14"/>
<connect gate="G$1" pin="VSA1" pad="8"/>
<connect gate="G$1" pin="VSA2" pad="3"/>
<connect gate="G$1" pin="XOUT" pad="13"/>
<connect gate="G$1" pin="YOUT" pad="12"/>
<connect gate="G$1" pin="ZOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR" prefix="L" uservalue="yes">
<description>&lt;b&gt;Inductors&lt;/b&gt;&lt;p&gt;
Basic Inductor/Choke - 0603 and 1206. Footprints are not proven and vary greatly between part numbers.&lt;br&gt;
INDUCTOR POWER 3.3UH 4.0A SMD&lt;br&gt;
0.197" L x 0.197" W x 0.177" H (5.00mm x 5.00mm x 4.50mm)</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="" package="SMD_COIL">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEMS_MIC_SPU0414HR5H-SB">
<gates>
<gate name="G$1" symbol="MEMS_MIC_ANALOG"/>
</gates>
<devices>
<device name="" package="CSP-4PIN">
<connects>
<connect gate="G$1" pin="GAIN" pad="P$3"/>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="OUT" pad="P$4"/>
<connect gate="G$1" pin="VDD" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEMS_MIC_SPH0645LM4H-B">
<gates>
<gate name="G$1" symbol="MEMS_MIC_I2S"/>
</gates>
<devices>
<device name="I2S" package="MIC_BOTTOM_PORT">
<connects>
<connect gate="G$1" pin="CLK" pad="4"/>
<connect gate="G$1" pin="DATA" pad="6"/>
<connect gate="G$1" pin="GND" pad="3 P$1"/>
<connect gate="G$1" pin="SEL" pad="2"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="WS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC_MEMS_ANALOG_SPU0414HR5H">
<gates>
<gate name="G$1" symbol="MIC_MEMS_ANALOG_SPU0414HR5H"/>
</gates>
<devices>
<device name="" package="MIC_MEMS_ANALOG_SPU0414HR5H">
<connects>
<connect gate="G$1" pin="GAIN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA16U2">
<gates>
<gate name="G$1" symbol="ATMEGA16U2"/>
</gates>
<devices>
<device name="-TQ" package="TQFP32-08THIN">
<connects>
<connect gate="G$1" pin="(!CTS!/!HWB!/AIN6/T0/INT7)PD7" pad="13"/>
<connect gate="G$1" pin="(!RTS!/AIN5/INT6)PD6" pad="12"/>
<connect gate="G$1" pin="(!SS!/PCINT0)PB0" pad="14"/>
<connect gate="G$1" pin="(AIN0/INT1)PD1" pad="7"/>
<connect gate="G$1" pin="(INT4/ICP1/CLKO)PC7" pad="22"/>
<connect gate="G$1" pin="(INT5/AIN3)PD4" pad="10"/>
<connect gate="G$1" pin="(OC.0B/INT0)PD0" pad="6"/>
<connect gate="G$1" pin="(OC.1A/PCINT8)PC6" pad="23"/>
<connect gate="G$1" pin="(PC0)XTAL2" pad="2"/>
<connect gate="G$1" pin="(PC1/DW)!RESET" pad="24"/>
<connect gate="G$1" pin="(PCINT10)PC4" pad="26"/>
<connect gate="G$1" pin="(PCINT11/AIN2)PC2" pad="5"/>
<connect gate="G$1" pin="(PCINT5)PB5" pad="19"/>
<connect gate="G$1" pin="(PCINT6)PB6" pad="20"/>
<connect gate="G$1" pin="(PCINT7/OC.0A/OC.1C)PB7" pad="21"/>
<connect gate="G$1" pin="(PCINT9/OC.1B)PC5" pad="25"/>
<connect gate="G$1" pin="(PDI/MOSI/PCINT2)PB2" pad="16"/>
<connect gate="G$1" pin="(PDO/MISO/PCINT3)PB3" pad="17"/>
<connect gate="G$1" pin="(RXD1/AIN1/INT2)PD2" pad="8"/>
<connect gate="G$1" pin="(SCLK/PCINT1)PB1" pad="15"/>
<connect gate="G$1" pin="(T1/PCINT4)PB4" pad="18"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="9"/>
<connect gate="G$1" pin="(XCK/AIN4/PCINT12)PD5" pad="11"/>
<connect gate="G$1" pin="AVCC" pad="32"/>
<connect gate="G$1" pin="D+" pad="29"/>
<connect gate="G$1" pin="D-" pad="30"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="UCAP" pad="27"/>
<connect gate="G$1" pin="UGND" pad="28"/>
<connect gate="G$1" pin="UVCC" pad="31"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24L01+">
<description>nRF24L01+ 2.4GHz Wireless Transceiver module</description>
<gates>
<gate name="G$1" symbol="NRF24L01+"/>
</gates>
<devices>
<device name="" package="2X04_THRU">
<connects>
<connect gate="G$1" pin="CE" pad="2"/>
<connect gate="G$1" pin="CSN" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IRQ" pad="5"/>
<connect gate="G$1" pin="MISO" pad="4"/>
<connect gate="G$1" pin="MOSI" pad="6"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHOKE" prefix="L">
<description>SMD choke (inductor/coil) ELL-CTV000M as found in the fablab inventory.

&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="U1" symbol="COIL"/>
</gates>
<devices>
<device name="SMD" package="ELLCTV">
<connects>
<connect gate="U1" pin="P$1" pad="1"/>
<connect gate="U1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JACK-2.1MM" prefix="J">
<description>SMD DC power jack PJ-002AH-SMT As found in the fablab inventory.

&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="G$1" symbol="DC-POWER-JACK"/>
</gates>
<devices>
<device name="" package="PJ-002AH-SMT">
<connects>
<connect gate="G$1" pin="CONTACT" pad="CONTACT"/>
<connect gate="G$1" pin="PIN1" pad="PIN1"/>
<connect gate="G$1" pin="PIN2" pad="PIN2"/>
<connect gate="G$1" pin="SHUNT" pad="SHUNT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICRO-USB" prefix="X">
<description>SMD micro USB connector as found in the fablab inventory. 
Three footprint variants included: 
&lt;ol&gt;
&lt;li&gt; original, as described by manufacturer's datasheet
&lt;li&gt; for milling with the 1/100" bit
&lt;li&gt; for milling with the 1/64" bit
&lt;/ol&gt;
&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="G$1" symbol="USB-1"/>
</gates>
<devices>
<device name="_1/100" package="DX4R005HJ5_100">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_ORIG" package="DX4R005HJ5">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1/64" package="DX4R005HJ5_64">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SLIDE-SWITCH" prefix="S">
<description>SMD slide-switch AYZ0102AGRLC as found in the fablab inventory.  Includes the mounting holes.

&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="G$1" symbol="SWITCH-SPDT"/>
</gates>
<devices>
<device name="" package="AYZ0102AGRLC">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TERM-1X02" prefix="J">
<description>3.5mm terminal block, 2 positions ED555-2DS as found in the fablab inventory. 
&lt;p&gt;Stolen from &lt;a href="http://www.ladyada.net/library/pcb/eaglelibrary.html"&gt;Adafruit&lt;/a&gt;, adapted by Zaerc.</description>
<gates>
<gate name="G$1" symbol="1X2"/>
</gates>
<devices>
<device name="-ADAFRUIT" package="3.5MMTERM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-FABLAB" package="ED555DS-2DS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TERM-1X03">
<description>3.5mm terminal block, 3 positions ED555-3DS as found in the fablab inventory.
&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="G$1" symbol="1X3"/>
</gates>
<devices>
<device name="'-FABLAB'" package="ED555DS-3DS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CDBM1100-G" prefix="D">
<description>Diode schottky 100V 1A mini-SMA as found in the fablab inventory
&lt;ul&gt;
&lt;li&gt;Reverse Voltage: 100 Volts
&lt;li&gt;Forward Current: 1.0 Amp
&lt;li&gt;Maximum forward voltage: 0.85 Volts
&lt;/ul&gt;
&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="MINI-SMA">
<connects>
<connect gate="G$1" pin="ANODE" pad="ANODE"/>
<connect gate="G$1" pin="KATHODE" pad="KATHODE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_LM1117" prefix="U" uservalue="yes">
<description>&lt;b&gt;Voltage Regulator LM1117&lt;/b&gt;
Standard adjustable voltage regulator but in SMD form. Spark Fun Electronics SKU : COM-00595</description>
<gates>
<gate name="G$1" symbol="78ADJ"/>
</gates>
<devices>
<device name="SOT223" package="SOT223">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="OUT@1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="VREG-08170"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A4953-H-BRIDGE-MOTOR-DRIVER-PAD">
<gates>
<gate name="G$1" symbol="A4953-H-BRIDGE-MOTOR-DRIVER"/>
</gates>
<devices>
<device name="" package="SOIC8_PAD">
<connects>
<connect gate="G$1" pin="GND" pad="1 GND"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="IN2" pad="2"/>
<connect gate="G$1" pin="LSS" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT2" pad="8"/>
<connect gate="G$1" pin="VBB" pad="5"/>
<connect gate="G$1" pin="VREF" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA_A4U">
<gates>
<gate name="G$1" symbol="ATXMEGA_A4U"/>
</gates>
<devices>
<device name="TQFP-44-1-64" package="TQFP44-13THIN">
<connects>
<connect gate="G$1" pin="!RESET!/PDI_CLK" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="30"/>
<connect gate="G$1" pin="GND3" pad="38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0/SDA" pad="10"/>
<connect gate="G$1" pin="PC1/SCL/XCK0" pad="11"/>
<connect gate="G$1" pin="PC2/RXD0" pad="12"/>
<connect gate="G$1" pin="PC3/TXD0" pad="13"/>
<connect gate="G$1" pin="PC4/CS" pad="14"/>
<connect gate="G$1" pin="PC5/XCK1/MOSI" pad="15"/>
<connect gate="G$1" pin="PC6/RXD1/MISO" pad="16"/>
<connect gate="G$1" pin="PC7/TXD1/SCK" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1/XCK0" pad="21"/>
<connect gate="G$1" pin="PD2/RXD0" pad="22"/>
<connect gate="G$1" pin="PD3/TXD0" pad="23"/>
<connect gate="G$1" pin="PD4/CS" pad="24"/>
<connect gate="G$1" pin="PD5/XCK1/MOSI" pad="25"/>
<connect gate="G$1" pin="PD6/RXD1/MISO/DM" pad="26"/>
<connect gate="G$1" pin="PD7/TXD1/SCK/DP" pad="27"/>
<connect gate="G$1" pin="PDI_DATA" pad="34"/>
<connect gate="G$1" pin="PE0/SDA" pad="28"/>
<connect gate="G$1" pin="PE1/XCK0/SCL" pad="29"/>
<connect gate="G$1" pin="PE2/RXD0" pad="32"/>
<connect gate="G$1" pin="PE3/TXD0" pad="33"/>
<connect gate="G$1" pin="PR0(XT2)" pad="36"/>
<connect gate="G$1" pin="PR1(XT1)" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VCC1" pad="19"/>
<connect gate="G$1" pin="VCC2" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VFQFN-44" package="QFN-44-7X7">
<connects>
<connect gate="G$1" pin="!RESET!/PDI_CLK" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8 TH"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="30"/>
<connect gate="G$1" pin="GND3" pad="38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0/SDA" pad="10"/>
<connect gate="G$1" pin="PC1/SCL/XCK0" pad="11"/>
<connect gate="G$1" pin="PC2/RXD0" pad="12"/>
<connect gate="G$1" pin="PC3/TXD0" pad="13"/>
<connect gate="G$1" pin="PC4/CS" pad="14"/>
<connect gate="G$1" pin="PC5/XCK1/MOSI" pad="15"/>
<connect gate="G$1" pin="PC6/RXD1/MISO" pad="16"/>
<connect gate="G$1" pin="PC7/TXD1/SCK" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1/XCK0" pad="21"/>
<connect gate="G$1" pin="PD2/RXD0" pad="22"/>
<connect gate="G$1" pin="PD3/TXD0" pad="23"/>
<connect gate="G$1" pin="PD4/CS" pad="24"/>
<connect gate="G$1" pin="PD5/XCK1/MOSI" pad="25"/>
<connect gate="G$1" pin="PD6/RXD1/MISO/DM" pad="26"/>
<connect gate="G$1" pin="PD7/TXD1/SCK/DP" pad="27"/>
<connect gate="G$1" pin="PDI_DATA" pad="34"/>
<connect gate="G$1" pin="PE0/SDA" pad="28"/>
<connect gate="G$1" pin="PE1/XCK0/SCL" pad="29"/>
<connect gate="G$1" pin="PE2/RXD0" pad="32"/>
<connect gate="G$1" pin="PE3/TXD0" pad="33"/>
<connect gate="G$1" pin="PR0(XT2)" pad="36"/>
<connect gate="G$1" pin="PR1(XT1)" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VCC1" pad="19"/>
<connect gate="G$1" pin="VCC2" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATSAM4N8A" prefix="U">
<gates>
<gate name="G$1" symbol="ATSAM4N8A"/>
</gates>
<devices>
<device name="ATSAM4N8A" package="LQFP48">
<connects>
<connect gate="G$1" pin="ADVREFP" pad="1"/>
<connect gate="G$1" pin="ERASE/PB12" pad="42"/>
<connect gate="G$1" pin="GND_1" pad="2"/>
<connect gate="G$1" pin="GND_2" pad="34"/>
<connect gate="G$1" pin="JTAGSEL" pad="38"/>
<connect gate="G$1" pin="NRST" pad="29"/>
<connect gate="G$1" pin="PA0/PGMEN0" pad="36"/>
<connect gate="G$1" pin="PA1/PGMEN1" pad="35"/>
<connect gate="G$1" pin="PA10/PGMM2" pad="21"/>
<connect gate="G$1" pin="PA11/PGMM3" pad="20"/>
<connect gate="G$1" pin="PA12/PGMD0" pad="19"/>
<connect gate="G$1" pin="PA13/PGMD1" pad="17"/>
<connect gate="G$1" pin="PA14/PGMD2" pad="16"/>
<connect gate="G$1" pin="PA15/PGMD3" pad="15"/>
<connect gate="G$1" pin="PA16/PGMD4" pad="14"/>
<connect gate="G$1" pin="PA17/PGMD5/AD0" pad="9"/>
<connect gate="G$1" pin="PA18/PGMD6/AD1" pad="10"/>
<connect gate="G$1" pin="PA19/PGMD7/AD2" pad="11"/>
<connect gate="G$1" pin="PA2/PGMEN2" pad="32"/>
<connect gate="G$1" pin="PA20/AD3" pad="12"/>
<connect gate="G$1" pin="PA3" pad="31"/>
<connect gate="G$1" pin="PA5/PGMNCMD" pad="28"/>
<connect gate="G$1" pin="PA5/PGMRDY" pad="27"/>
<connect gate="G$1" pin="PA6/PGMNOE" pad="26"/>
<connect gate="G$1" pin="PA7/XIN32/PGMNVALID" pad="24"/>
<connect gate="G$1" pin="PA8/XOUT32/PGMM0" pad="23"/>
<connect gate="G$1" pin="PA9/PGMM1" pad="22"/>
<connect gate="G$1" pin="PB0/AD4" pad="3"/>
<connect gate="G$1" pin="PB1/AD5" pad="4"/>
<connect gate="G$1" pin="PB10" pad="43"/>
<connect gate="G$1" pin="PB11" pad="44"/>
<connect gate="G$1" pin="PB2/AD6" pad="5"/>
<connect gate="G$1" pin="PB3/AD7" pad="6"/>
<connect gate="G$1" pin="TCK/SWCLK/PB7" pad="40"/>
<connect gate="G$1" pin="TDI/PB4" pad="25"/>
<connect gate="G$1" pin="TDO/TRACESWO/PB5" pad="37"/>
<connect gate="G$1" pin="TMS/SWDIO/PB6" pad="39"/>
<connect gate="G$1" pin="TST" pad="30"/>
<connect gate="G$1" pin="VDDCORE_1" pad="18"/>
<connect gate="G$1" pin="VDDCORE_2" pad="41"/>
<connect gate="G$1" pin="VDDIN" pad="7"/>
<connect gate="G$1" pin="VDDIO_1" pad="13"/>
<connect gate="G$1" pin="VDDIO_2" pad="33"/>
<connect gate="G$1" pin="VDDIO_3" pad="47"/>
<connect gate="G$1" pin="VDDOUT" pad="8"/>
<connect gate="G$1" pin="VDDPLL" pad="48"/>
<connect gate="G$1" pin="XIN/P/PB9/GMCK" pad="46"/>
<connect gate="G$1" pin="XOUT/PB8" pad="45"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATSAMS70N-TQFP100" prefix="U">
<gates>
<gate name="G$1" symbol="ATSAMS70N"/>
</gates>
<devices>
<device name="" package="TQFP100-14X14">
<connects>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$1" pin="GND3" pad="8"/>
<connect gate="G$1" pin="GND4" pad="10"/>
<connect gate="G$1" pin="GND5" pad="29"/>
<connect gate="G$1" pin="GND6" pad="67"/>
<connect gate="G$1" pin="JTAGSEL" pad="73"/>
<connect gate="G$1" pin="NRST" pad="58"/>
<connect gate="G$1" pin="PA0/I2SC0_MCK" pad="72"/>
<connect gate="G$1" pin="PA1/I2SC0_CK" pad="70"/>
<connect gate="G$1" pin="PA10/UTXD0" pad="46"/>
<connect gate="G$1" pin="PA11/PWMC0_PWMH0" pad="44"/>
<connect gate="G$1" pin="PA12/PWMC0_PWMH1" pad="48"/>
<connect gate="G$1" pin="PA13/PWMC0_PWMH2" pad="27"/>
<connect gate="G$1" pin="PA14/WMC0_PWMH3" pad="34"/>
<connect gate="G$1" pin="PA15/PWMC0_PWML3" pad="33"/>
<connect gate="G$1" pin="PA16/PWMC0_PWML2" pad="30"/>
<connect gate="G$1" pin="PA17/AFE0_AD6" pad="16"/>
<connect gate="G$1" pin="PA18/AFE0_AD7" pad="15"/>
<connect gate="G$1" pin="PA19/PWMC0_PWML0/AFE0_AD8" pad="14"/>
<connect gate="G$1" pin="PA2" pad="66"/>
<connect gate="G$1" pin="PA20/PWMC0_PWML1/AFE0_AD9" pad="13"/>
<connect gate="G$1" pin="PA21/AFE0_AD1" pad="21"/>
<connect gate="G$1" pin="PA22" pad="26"/>
<connect gate="G$1" pin="PA23" pad="31"/>
<connect gate="G$1" pin="PA24" pad="38"/>
<connect gate="G$1" pin="PA25" pad="40"/>
<connect gate="G$1" pin="PA26" pad="42"/>
<connect gate="G$1" pin="PA27" pad="50"/>
<connect gate="G$1" pin="PA28" pad="79"/>
<connect gate="G$1" pin="PA3/TWD0" pad="64"/>
<connect gate="G$1" pin="PA30" pad="82"/>
<connect gate="G$1" pin="PA31/SPI0_NPCS1" pad="83"/>
<connect gate="G$1" pin="PA4/UTXD1/TWCK0" pad="55"/>
<connect gate="G$1" pin="PA5/URXD1" pad="52"/>
<connect gate="G$1" pin="PA7/XIN32" pad="24"/>
<connect gate="G$1" pin="PA8/XOUT32" pad="25"/>
<connect gate="G$1" pin="PA9/URXD0" pad="54"/>
<connect gate="G$1" pin="PB0/RXD0" pad="12"/>
<connect gate="G$1" pin="PB1/TXD0" pad="11"/>
<connect gate="G$1" pin="PB12/ERASE" pad="61"/>
<connect gate="G$1" pin="PB13/DAC0/SCK0" pad="100"/>
<connect gate="G$1" pin="PB2/SPI0_NPCS0/CTS0" pad="17"/>
<connect gate="G$1" pin="PB3/RTS0" pad="20"/>
<connect gate="G$1" pin="PB4/TDI/TWD1" pad="74"/>
<connect gate="G$1" pin="PB5/TDO/TWCK1" pad="77"/>
<connect gate="G$1" pin="PB6/SWDIO/TMS" pad="57"/>
<connect gate="G$1" pin="PB7/SWCLK/TCK" pad="63"/>
<connect gate="G$1" pin="PB8/XOUT" pad="98"/>
<connect gate="G$1" pin="PB9/XIN" pad="99"/>
<connect gate="G$1" pin="PD0/DAC1/PWMC1_PWML0" pad="1"/>
<connect gate="G$1" pin="PD1/PWMC1_PWMH0" pad="92"/>
<connect gate="G$1" pin="PD10/PWMC0_PWML0" pad="71"/>
<connect gate="G$1" pin="PD11/PWMC0_PWMH0" pad="69"/>
<connect gate="G$1" pin="PD12/SPI0_NPCS2" pad="65"/>
<connect gate="G$1" pin="PD13" pad="62"/>
<connect gate="G$1" pin="PD14" pad="59"/>
<connect gate="G$1" pin="PD15" pad="75"/>
<connect gate="G$1" pin="PD16" pad="56"/>
<connect gate="G$1" pin="PD17" pad="53"/>
<connect gate="G$1" pin="PD18/URXD4" pad="49"/>
<connect gate="G$1" pin="PD19/UTXD4" pad="47"/>
<connect gate="G$1" pin="PD2/PWMC1_PWML1" pad="91"/>
<connect gate="G$1" pin="PD20/SPI0_MISO" pad="45"/>
<connect gate="G$1" pin="PD21/SPI0_MOSI" pad="43"/>
<connect gate="G$1" pin="PD22_SPI0_SPCK" pad="41"/>
<connect gate="G$1" pin="PD24" pad="37"/>
<connect gate="G$1" pin="PD25/URXD2" pad="35"/>
<connect gate="G$1" pin="PD26/UTXD2" pad="36"/>
<connect gate="G$1" pin="PD27/SPI0_NPCS3/TWD2" pad="32"/>
<connect gate="G$1" pin="PD28/URXD3/TWCK2" pad="51"/>
<connect gate="G$1" pin="PD3/PWMC1_PWMH1" pad="89"/>
<connect gate="G$1" pin="PD30/UTXD3" pad="23"/>
<connect gate="G$1" pin="PD31" pad="2"/>
<connect gate="G$1" pin="PD4/PWMC1_PWML2" pad="88"/>
<connect gate="G$1" pin="PD5/PWMC1_PWMH2" pad="87"/>
<connect gate="G$1" pin="PD6/PWMC1_PWML3" pad="85"/>
<connect gate="G$1" pin="PD7/PWMC1_PWMH3" pad="84"/>
<connect gate="G$1" pin="PD8" pad="80"/>
<connect gate="G$1" pin="PD9" pad="78"/>
<connect gate="G$1" pin="TST" pad="60"/>
<connect gate="G$1" pin="USB_DM" pad="94"/>
<connect gate="G$1" pin="USB_DP" pad="95"/>
<connect gate="G$1" pin="VBG" pad="97"/>
<connect gate="G$1" pin="VDDCORE1" pad="18"/>
<connect gate="G$1" pin="VDDCORE2" pad="22"/>
<connect gate="G$1" pin="VDDCORE3" pad="39"/>
<connect gate="G$1" pin="VDDCORE4" pad="76"/>
<connect gate="G$1" pin="VDDIN" pad="5"/>
<connect gate="G$1" pin="VDDIO1" pad="19"/>
<connect gate="G$1" pin="VDDIO2" pad="28"/>
<connect gate="G$1" pin="VDDIO3" pad="68"/>
<connect gate="G$1" pin="VDDIO4" pad="81"/>
<connect gate="G$1" pin="VDDOUT" pad="4"/>
<connect gate="G$1" pin="VDDPLL" pad="86"/>
<connect gate="G$1" pin="VDDPLLUSB" pad="90"/>
<connect gate="G$1" pin="VDDUTMIC" pad="96"/>
<connect gate="G$1" pin="VDDUTMII" pad="93"/>
<connect gate="G$1" pin="VREFN" pad="6"/>
<connect gate="G$1" pin="VREFP" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISL3177E" prefix="U">
<gates>
<gate name="G$1" symbol="ISL3177E"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="G$1" pin="A" pad="8"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="Y" pad="5"/>
<connect gate="G$1" pin="Z" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MILL" package="MSOP8-8MILPADS">
<connects>
<connect gate="G$1" pin="A" pad="8"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="Y" pad="5"/>
<connect gate="G$1" pin="Z" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REGULATOR_SOT223" prefix="U">
<gates>
<gate name="G$1" symbol="REGULATOR_SOT223"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_03X2" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;You can populate with any combo of single row headers, but if you'd like an exact match, check these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12807"&gt; Header - 2x3 (Male, 0.1")&lt;/a&gt; (PRT-12807)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13010"&gt; Header - 2x3 (Female, 0.1")&lt;/a&gt; (PRT-13010)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10877"&gt; 2x3 Pin Shrouded Header&lt;/a&gt; (PRT-10877)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special note: the shrouded connector mates well with our 3x2 ribbon cables:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10651"&gt; Ribbon Crimp Connector - 6-pin (2x3, Female)&lt;/a&gt; (PRT-10651)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10646"&gt; Ribbon Cable - 6 wire (15ft)&lt;/a&gt; (PRT-10646)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_03X2"/>
</gates>
<devices>
<device name="SHROUD" package="2X3-SHROUDED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10681"/>
<attribute name="SF_ID" value="PRT_10877"/>
</technology>
</technologies>
</device>
<device name="SMT" package="2X3_SMT_POSTS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11415"/>
</technology>
</technologies>
</device>
<device name="POGO_PINS" package="2X3_POGO">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="HW-11044"/>
</technology>
</technologies>
</device>
<device name="2X3_SILK_MALE_PTH" package="2X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09701"/>
</technology>
</technologies>
</device>
<device name="NO_SILK" package="2X3-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FEMALE_SMD" package="2X3_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11290"/>
</technology>
</technologies>
</device>
<device name="FEMALE" package="2X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11566"/>
<attribute name="VALUE" value="FEMALE 2x3"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_04X2" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_04X2"/>
</gates>
<devices>
<device name="" package="2X4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHROUDED" package="2X4-SHROUDED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHROUDED-SQUISH" package="2X4-SHROUDED-SQUISH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMA-B" prefix="R" uservalue="yes">
<description>&lt;b&gt;SMD SHUNT RESISTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="R-4"/>
</gates>
<devices>
<device name="" package="PMA-B">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="SA" pad="SA"/>
<connect gate="G$1" pin="SB" pad="SB"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WSL2726" prefix="R" uservalue="yes">
<description>&lt;b&gt;SMD SHUNT RESISTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="WSL2726"/>
</gates>
<devices>
<device name="" package="WSL2726">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="SA" pad="SA"/>
<connect gate="G$1" pin="SB" pad="SB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DRV8302">
<gates>
<gate name="G$1" symbol="DRV8302"/>
</gates>
<devices>
<device name="" package="HTSSOP-56">
<connects>
<connect gate="G$1" pin="AGND" pad="P$28"/>
<connect gate="G$1" pin="AVDD" pad="P$27"/>
<connect gate="G$1" pin="BIAS" pad="P$49"/>
<connect gate="G$1" pin="BST_A" pad="P$48"/>
<connect gate="G$1" pin="BST_B" pad="P$43"/>
<connect gate="G$1" pin="BST_BK" pad="P$52"/>
<connect gate="G$1" pin="BST_C" pad="P$38"/>
<connect gate="G$1" pin="COMP" pad="P$2"/>
<connect gate="G$1" pin="CP1" pad="P$14"/>
<connect gate="G$1" pin="CP2" pad="P$15"/>
<connect gate="G$1" pin="DC_CAL" pad="P$12"/>
<connect gate="G$1" pin="DTC" pad="P$7"/>
<connect gate="G$1" pin="DVDD" pad="P$23"/>
<connect gate="G$1" pin="EN_BUCK" pad="P$55"/>
<connect gate="G$1" pin="EN_GATE" pad="P$16"/>
<connect gate="G$1" pin="GAIN" pad="P$10"/>
<connect gate="G$1" pin="GH_A" pad="P$47"/>
<connect gate="G$1" pin="GH_B" pad="P$42"/>
<connect gate="G$1" pin="GH_C" pad="P$37"/>
<connect gate="G$1" pin="GL_A" pad="P$45"/>
<connect gate="G$1" pin="GL_B" pad="P$40"/>
<connect gate="G$1" pin="GL_C" pad="P$35"/>
<connect gate="G$1" pin="GNDPAD" pad="P$57"/>
<connect gate="G$1" pin="GVDD" pad="P$13"/>
<connect gate="G$1" pin="INH_A" pad="P$17"/>
<connect gate="G$1" pin="INH_B" pad="P$19"/>
<connect gate="G$1" pin="INH_C" pad="P$21"/>
<connect gate="G$1" pin="INL_A" pad="P$18"/>
<connect gate="G$1" pin="INL_B" pad="P$20"/>
<connect gate="G$1" pin="INL_C" pad="P$22"/>
<connect gate="G$1" pin="M_OC" pad="P$9"/>
<connect gate="G$1" pin="M_PWM" pad="P$8"/>
<connect gate="G$1" pin="NFAULT" pad="P$6"/>
<connect gate="G$1" pin="NOCTW" pad="P$5"/>
<connect gate="G$1" pin="OC_ADJ" pad="P$11"/>
<connect gate="G$1" pin="PH1" pad="P$50"/>
<connect gate="G$1" pin="PH2" pad="P$51"/>
<connect gate="G$1" pin="PVDD1" pad="P$29"/>
<connect gate="G$1" pin="PVDD2-1" pad="P$53"/>
<connect gate="G$1" pin="PVDD2-2" pad="P$54"/>
<connect gate="G$1" pin="PWRGND" pad="P$4"/>
<connect gate="G$1" pin="REF" pad="P$24"/>
<connect gate="G$1" pin="RT_CLK" pad="P$1"/>
<connect gate="G$1" pin="SH_A" pad="P$46"/>
<connect gate="G$1" pin="SH_B" pad="P$41"/>
<connect gate="G$1" pin="SH_C" pad="P$36"/>
<connect gate="G$1" pin="SL_A" pad="P$44"/>
<connect gate="G$1" pin="SL_B" pad="P$39"/>
<connect gate="G$1" pin="SL_C" pad="P$34"/>
<connect gate="G$1" pin="SN1" pad="P$33"/>
<connect gate="G$1" pin="SN2" pad="P$31"/>
<connect gate="G$1" pin="SO1" pad="P$25"/>
<connect gate="G$1" pin="SO2" pad="P$26"/>
<connect gate="G$1" pin="SP1" pad="P$32"/>
<connect gate="G$1" pin="SP2" pad="P$30"/>
<connect gate="G$1" pin="SS_TR" pad="P$56"/>
<connect gate="G$1" pin="VSENSE" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BFC" prefix="BFC">
<gates>
<gate name="G$1" symbol="C-US"/>
</gates>
<devices>
<device name="" package="BFC">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PWRPAD" prefix="J">
<gates>
<gate name="G$1" symbol="PWRPAD"/>
</gates>
<devices>
<device name="2-5MM" package="PWRPAD_2-5MM">
<connects>
<connect gate="G$1" pin="PWRPAD" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4MM" package="PWRPAD_4MM">
<connects>
<connect gate="G$1" pin="PWRPAD" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CBA-LOGO">
<gates>
</gates>
<devices>
<device name="" package="CBA-SILK-LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MK-LOGO">
<gates>
</gates>
<devices>
<device name="" package="MK-LOGO-SILK">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AS5304-6">
<gates>
<gate name="G$1" symbol="AS5304-6"/>
</gates>
<devices>
<device name="" package="TSSOP20-08THIN">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="AO" pad="6"/>
<connect gate="G$1" pin="B" pad="4"/>
<connect gate="G$1" pin="INDEX" pad="8"/>
<connect gate="G$1" pin="NC1" pad="9"/>
<connect gate="G$1" pin="NC2" pad="10"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="TEST1" pad="5"/>
<connect gate="G$1" pin="TEST2" pad="12"/>
<connect gate="G$1" pin="TEST3" pad="13"/>
<connect gate="G$1" pin="TEST4" pad="14"/>
<connect gate="G$1" pin="TEST5" pad="17"/>
<connect gate="G$1" pin="TEST6" pad="18"/>
<connect gate="G$1" pin="TEST7" pad="19"/>
<connect gate="G$1" pin="TEST_GND" pad="15"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDDA" pad="16"/>
<connect gate="G$1" pin="VDDP" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
<connect gate="G$1" pin="ZPZ" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARM_10" prefix="J" uservalue="yes">
<gates>
<gate name="G$1" symbol="ARM_SWD_10"/>
</gates>
<devices>
<device name="SMD" package="2X5_1.27MM_SMD">
<connects>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="NC/TDI" pad="8"/>
<connect gate="G$1" pin="NRESET" pad="10"/>
<connect gate="G$1" pin="SWDCLK/TCK" pad="4"/>
<connect gate="G$1" pin="SWDIO/TMS" pad="2"/>
<connect gate="G$1" pin="SWO/TDO" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PACKAGE" value="2x5_1.27MM_SMD"/>
</technology>
</technologies>
</device>
<device name="PTH" package="2X5_1.27MM_PTH">
<connects>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="NC/TDI" pad="8"/>
<connect gate="G$1" pin="NRESET" pad="10"/>
<connect gate="G$1" pin="SWDCLK/TCK" pad="4"/>
<connect gate="G$1" pin="SWDIO/TMS" pad="2"/>
<connect gate="G$1" pin="SWO/TDO" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PACKAGE" value="2x5_1.27MM_PTH"/>
</technology>
</technologies>
</device>
<device name="TDC2050-IDC" package="TC2050-IDC">
<connects>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="NC/TDI" pad="8"/>
<connect gate="G$1" pin="NRESET" pad="10"/>
<connect gate="G$1" pin="SWDCLK/TCK" pad="4"/>
<connect gate="G$1" pin="SWDIO/TMS" pad="2"/>
<connect gate="G$1" pin="SWO/TDO" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PACKAGE" value="TC2050-IDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_05X2" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;h3&gt;For AVR SPI programming port, see special device with nice symbol: "AVR_SPI_PROG_5x2.dev"&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;You can populate with any combo of single row headers, but if you'd like an exact match, check these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/778"&gt; 2x5 AVR ICSP Male Header&lt;/a&gt; (PRT-00778)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8506"&gt; 2x5 Pin Shrouded Header&lt;/a&gt; (PRT-08506)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special note: the shrouded connector mates well with our 5x2 ribbon cables:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8535"&gt; 2x5 Pin IDC Ribbon Cable&lt;/a&gt; (PRT-08535)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_05X2"/>
</gates>
<devices>
<device name="PTH" package="2X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08499"/>
<attribute name="SF_ID" value="PRT-0778"/>
</technology>
</technologies>
</device>
<device name="RA" package="2X5-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RAF" package="2X5-RAF">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHD" package="2X5-SHROUDED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08671"/>
<attribute name="SF_ID" value="PRT-08506"/>
</technology>
</technologies>
</device>
<device name="SHD_LOCK" package="2X5-SHROUDED_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08671"/>
<attribute name="SF_ID" value="PRT-08506"/>
</technology>
</technologies>
</device>
<device name="SHD_SMD" package="2X5-SHROUDED_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09508"/>
</technology>
</technologies>
</device>
<device name="NO_SILK" package="2X5_NOSILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0.05_IN_PTH_SILK" package="2X5_PTH_SILK_.05">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHD-NS" package="2X5-SHROUDED-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08671"/>
<attribute name="SF_ID" value="PRT-08506"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XR21V410-USB-UART">
<gates>
<gate name="G$1" symbol="XR21V410-USB-UART"/>
</gates>
<devices>
<device name="" package="QFN-16-3X3-1-100">
<connects>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="13"/>
<connect gate="G$1" pin="GND_PAD" pad="EXP"/>
<connect gate="G$1" pin="GPIO0" pad="8"/>
<connect gate="G$1" pin="GPIO1" pad="7"/>
<connect gate="G$1" pin="GPIO2" pad="6"/>
<connect gate="G$1" pin="GPIO3" pad="5"/>
<connect gate="G$1" pin="GPIO4" pad="4"/>
<connect gate="G$1" pin="GPIO5" pad="3"/>
<connect gate="G$1" pin="LOWPOWER" pad="2"/>
<connect gate="G$1" pin="RX" pad="10"/>
<connect gate="G$1" pin="SCL" pad="12"/>
<connect gate="G$1" pin="SDA" pad="11"/>
<connect gate="G$1" pin="TX" pad="9"/>
<connect gate="G$1" pin="USBD+" pad="15"/>
<connect gate="G$1" pin="USBD-" pad="14"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGA_A3U">
<gates>
<gate name="G$1" symbol="ATXMEGA_A3U"/>
</gates>
<devices>
<device name="" package="TQFP64_14X14MM-013THIN">
<connects>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="24"/>
<connect gate="G$1" pin="GND@3" pad="34"/>
<connect gate="G$1" pin="GND@4" pad="44"/>
<connect gate="G$1" pin="GND@5" pad="52"/>
<connect gate="G$1" pin="GND@6" pad="60"/>
<connect gate="G$1" pin="PA0/AREF" pad="62"/>
<connect gate="G$1" pin="PA1" pad="63"/>
<connect gate="G$1" pin="PA2" pad="64"/>
<connect gate="G$1" pin="PA3" pad="1"/>
<connect gate="G$1" pin="PA4" pad="2"/>
<connect gate="G$1" pin="PA5" pad="3"/>
<connect gate="G$1" pin="PA6" pad="4"/>
<connect gate="G$1" pin="PA7" pad="5"/>
<connect gate="G$1" pin="PB0/AREF" pad="6"/>
<connect gate="G$1" pin="PB1" pad="7"/>
<connect gate="G$1" pin="PB2/DAC0" pad="8"/>
<connect gate="G$1" pin="PB3/DAC1" pad="9"/>
<connect gate="G$1" pin="PB4" pad="10"/>
<connect gate="G$1" pin="PB5" pad="11"/>
<connect gate="G$1" pin="PB6" pad="12"/>
<connect gate="G$1" pin="PB7" pad="13"/>
<connect gate="G$1" pin="PC0/SDA" pad="16"/>
<connect gate="G$1" pin="PC1/SCL/XCK0" pad="17"/>
<connect gate="G$1" pin="PC2/RXD0" pad="18"/>
<connect gate="G$1" pin="PC3/TXD0" pad="19"/>
<connect gate="G$1" pin="PC4/SS" pad="20"/>
<connect gate="G$1" pin="PC5/XCK1/MOSI" pad="21"/>
<connect gate="G$1" pin="PC6/RXD1/MISO" pad="22"/>
<connect gate="G$1" pin="PC7/TXD1/SCK" pad="23"/>
<connect gate="G$1" pin="PD0" pad="26"/>
<connect gate="G$1" pin="PD1/XCK0" pad="27"/>
<connect gate="G$1" pin="PD2/RXD0" pad="28"/>
<connect gate="G$1" pin="PD3/TXD0" pad="29"/>
<connect gate="G$1" pin="PD4/SS" pad="30"/>
<connect gate="G$1" pin="PD5/XCK/MOSI" pad="31"/>
<connect gate="G$1" pin="PD6/RXD1/MISO/D-" pad="32"/>
<connect gate="G$1" pin="PD7/TXD1/SCK/D+" pad="33"/>
<connect gate="G$1" pin="PDI_DATA" pad="56"/>
<connect gate="G$1" pin="PE0/SDA" pad="36"/>
<connect gate="G$1" pin="PE1/SCL/XCK0" pad="37"/>
<connect gate="G$1" pin="PE2/RXD0" pad="38"/>
<connect gate="G$1" pin="PE3/TXD0" pad="39"/>
<connect gate="G$1" pin="PE4/SS" pad="40"/>
<connect gate="G$1" pin="PE5/XCK1/MOSI" pad="41"/>
<connect gate="G$1" pin="PE6/RXD1/MISO" pad="42"/>
<connect gate="G$1" pin="PE7/TXD1/SCK" pad="43"/>
<connect gate="G$1" pin="PF0" pad="46"/>
<connect gate="G$1" pin="PF1/XCK0" pad="47"/>
<connect gate="G$1" pin="PF2/RXD0" pad="48"/>
<connect gate="G$1" pin="PF3/TXD0" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0/XTAL2" pad="58"/>
<connect gate="G$1" pin="PR1/XTAL1" pad="59"/>
<connect gate="G$1" pin="RESET/PDI_CLK" pad="57"/>
<connect gate="G$1" pin="VCC@1" pad="15"/>
<connect gate="G$1" pin="VCC@2" pad="25"/>
<connect gate="G$1" pin="VCC@3" pad="35"/>
<connect gate="G$1" pin="VCC@4" pad="45"/>
<connect gate="G$1" pin="VCC@5" pad="53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
