<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<schematic>
<libraries>
<library name="01-adafruit">
<packages>
<package name="1X15">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X15-CB">
</package>
</packages>
<symbols>
<symbol name="PINHD15">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X15" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD15"/>
</gates>
<devices>
<device name="" package="1X15">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CB" package="1X15-CB">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="01_fab">
<packages>
<package name="1X06SMD">
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
</packages>
<symbols>
<symbol name="FTDI">
<pin name="GND"/>
<pin name="CTS"/>
<pin name="VCC"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="RTS"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="FTDI-SMD-HEADER">
<gates>
<gate name="G$1" symbol="FTDI"/>
</gates>
<devices>
<device name="" package="1X06SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RTS" pad="6"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TXD" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="JP3" library="01-adafruit" deviceset="PINHD-1X15" device=""/>
<part name="JP4" library="01-adafruit" deviceset="PINHD-1X15" device=""/>
<part name="JP1" library="01-adafruit" deviceset="PINHD-1X15" device=""/>
<part name="JP2" library="01-adafruit" deviceset="PINHD-1X15" device=""/>
<part name="SENSOR" library="01_fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="R1" library="01_fab" deviceset="RES-US" device="1206FAB"/>
</parts>
<sheets>
<sheet>
<plain>
<text>TO REGULATED SUPPLY</text>
<text>SENSOR TRANSMIT 3.3V PIN(3)</text>
<text>SENSOR RECEIVE 3.3V PIN(4)</text>
<text> (5V+)</text>
<text>GND</text>
</plain>
<busses>
</busses>
<nets>
<net name="RSV">
<segment>
<pinref part="JP2" gate="A" pin="2"/>
<pinref part="JP1" gate="A" pin="2"/>
</segment>
</net>
<net name="SD3">
<segment>
<pinref part="JP2" gate="A" pin="4"/>
<pinref part="JP1" gate="A" pin="4"/>
</segment>
</net>
<net name="SD1">
<segment>
<pinref part="JP2" gate="A" pin="6"/>
<pinref part="JP1" gate="A" pin="6"/>
</segment>
</net>
<net name="SD0">
<segment>
<pinref part="JP2" gate="A" pin="8"/>
<pinref part="JP1" gate="A" pin="8"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="JP2" gate="A" pin="10"/>
<pinref part="JP1" gate="A" pin="10"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="14"/>
<pinref part="JP1" gate="A" pin="14"/>
</segment>
<segment>
<pinref part="JP3" gate="A" pin="14"/>
<pinref part="JP4" gate="A" pin="14"/>
</segment>
<segment>
<pinref part="JP3" gate="A" pin="7"/>
<pinref part="JP4" gate="A" pin="7"/>
</segment>
<segment>
<pinref part="SENSOR" gate="G$1" pin="GND"/>
</segment>
</net>
<net name="EN">
<segment>
<pinref part="JP2" gate="A" pin="12"/>
<pinref part="JP1" gate="A" pin="12"/>
</segment>
</net>
<net name="VIN">
<segment>
<pinref part="JP2" gate="A" pin="15"/>
<pinref part="JP1" gate="A" pin="15"/>
</segment>
</net>
<net name="D0">
<segment>
<pinref part="JP3" gate="A" pin="1"/>
<pinref part="JP4" gate="A" pin="1"/>
</segment>
</net>
<net name="D2">
<segment>
<pinref part="JP3" gate="A" pin="3"/>
<pinref part="JP4" gate="A" pin="3"/>
</segment>
</net>
<net name="D4">
<segment>
<pinref part="JP3" gate="A" pin="5"/>
<pinref part="JP4" gate="A" pin="5"/>
</segment>
</net>
<net name="D6">
<segment>
<pinref part="JP3" gate="A" pin="9"/>
<pinref part="JP4" gate="A" pin="9"/>
</segment>
</net>
<net name="D8">
<segment>
<pinref part="JP3" gate="A" pin="11"/>
<pinref part="JP4" gate="A" pin="11"/>
</segment>
</net>
<net name="TX">
<segment>
<pinref part="JP3" gate="A" pin="13"/>
<pinref part="JP4" gate="A" pin="13"/>
</segment>
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="A0">
<segment>
<pinref part="JP2" gate="A" pin="1"/>
<pinref part="JP1" gate="A" pin="1"/>
</segment>
</net>
<net name="RSVV">
<segment>
<pinref part="JP2" gate="A" pin="3"/>
<pinref part="JP1" gate="A" pin="3"/>
</segment>
</net>
<net name="SD2">
<segment>
<pinref part="JP2" gate="A" pin="5"/>
<pinref part="JP1" gate="A" pin="5"/>
</segment>
</net>
<net name="CMD">
<segment>
<pinref part="JP2" gate="A" pin="7"/>
<pinref part="JP1" gate="A" pin="7"/>
</segment>
</net>
<net name="CLK">
<segment>
<pinref part="JP2" gate="A" pin="9"/>
<pinref part="JP1" gate="A" pin="9"/>
</segment>
</net>
<net name="3V3">
<segment>
<pinref part="JP2" gate="A" pin="11"/>
<pinref part="JP1" gate="A" pin="11"/>
</segment>
<segment>
<pinref part="JP3" gate="A" pin="15"/>
<pinref part="JP4" gate="A" pin="15"/>
</segment>
<segment>
<pinref part="JP3" gate="A" pin="6"/>
<pinref part="JP4" gate="A" pin="6"/>
</segment>
</net>
<net name="RST">
<segment>
<pinref part="JP2" gate="A" pin="13"/>
<pinref part="JP1" gate="A" pin="13"/>
</segment>
</net>
<net name="RX">
<segment>
<pinref part="JP3" gate="A" pin="12"/>
<pinref part="JP4" gate="A" pin="12"/>
</segment>
<segment>
<pinref part="SENSOR" gate="G$1" pin="RXD"/>
</segment>
</net>
<net name="D7">
<segment>
<pinref part="JP3" gate="A" pin="10"/>
<pinref part="JP4" gate="A" pin="10"/>
</segment>
</net>
<net name="D5">
<segment>
<pinref part="JP3" gate="A" pin="8"/>
<pinref part="JP4" gate="A" pin="8"/>
</segment>
</net>
<net name="D3">
<segment>
<pinref part="JP3" gate="A" pin="4"/>
<pinref part="JP4" gate="A" pin="4"/>
</segment>
</net>
<net name="D1">
<segment>
<pinref part="JP3" gate="A" pin="2"/>
<pinref part="JP4" gate="A" pin="2"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="SENSOR" gate="G$1" pin="VCC"/>
</segment>
</net>
<net name="TXD">
<segment>
<pinref part="SENSOR" gate="G$1" pin="TXD"/>
<pinref part="R1" gate="G$1" pin="2"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
