<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.1">
<drawing>
<schematic>
<libraries>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="QFP80P900X900X120-32N">
</package>
</packages>
<symbols>
<symbol name="ATMEGA328P-AU">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="ADC6" direction="in"/>
<pin name="ADC7" direction="in"/>
<pin name="AREF" direction="in"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATMEGA328P-AU" prefix="U">
<description>8-bit Microcontroller with In-System Programmable Flash</description>
<gates>
<gate name="A" symbol="ATMEGA328P-AU"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X120-32N">
<connects>
<connect gate="A" pin="ADC6" pad="19"/>
<connect gate="A" pin="ADC7" pad="22"/>
<connect gate="A" pin="AREF" pad="20"/>
<connect gate="A" pin="AVCC" pad="18"/>
<connect gate="A" pin="GND" pad="21"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="GND_3" pad="5"/>
<connect gate="A" pin="PB0" pad="12"/>
<connect gate="A" pin="PB1" pad="13"/>
<connect gate="A" pin="PB2" pad="14"/>
<connect gate="A" pin="PB3" pad="15"/>
<connect gate="A" pin="PB4" pad="16"/>
<connect gate="A" pin="PB5" pad="17"/>
<connect gate="A" pin="PB6" pad="7"/>
<connect gate="A" pin="PB7" pad="8"/>
<connect gate="A" pin="PC0" pad="23"/>
<connect gate="A" pin="PC1" pad="24"/>
<connect gate="A" pin="PC2" pad="25"/>
<connect gate="A" pin="PC3" pad="26"/>
<connect gate="A" pin="PC4" pad="27"/>
<connect gate="A" pin="PC5" pad="28"/>
<connect gate="A" pin="PC6" pad="29"/>
<connect gate="A" pin="PD0" pad="30"/>
<connect gate="A" pin="PD1" pad="31"/>
<connect gate="A" pin="PD2" pad="32"/>
<connect gate="A" pin="PD3" pad="1"/>
<connect gate="A" pin="PD4" pad="2"/>
<connect gate="A" pin="PD5" pad="9"/>
<connect gate="A" pin="PD6" pad="10"/>
<connect gate="A" pin="PD7" pad="11"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VCC_2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATMEGA328P-AU"/>
<attribute name="OC_FARNELL" value="1715486"/>
<attribute name="OC_NEWARK" value="14R4631"/>
<attribute name="PACKAGE" value="TQFP-32"/>
<attribute name="SUPPLIER" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="fab">
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="C1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="EFOBM">
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
<package name="P-LCC-4">
<description>&lt;b&gt;Power TOPLED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LA_LY E67B.pdf</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="2X02SMD">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="AYZ0102AGRLC">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="C-US">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="AVRISP">
<pin name="MISO" direction="pas" function="dot"/>
<pin name="VCC" direction="pas" function="dot"/>
<pin name="SCK" direction="pas" function="dot"/>
<pin name="MOSI" direction="pas" function="dot"/>
<pin name="RST" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CERAMIC_RESONATOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="LED">
<description>LED</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="LED-RGB">
<pin name="CGREEN" direction="pas"/>
<pin name="CBLUE" direction="pas"/>
<pin name="CRED" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="REGULATOR">
<pin name="IN"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="PINH2X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="REGULATOR_SOT223">
<pin name="IN"/>
<pin name="GND"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
</symbol>
<symbol name="SWITCH-SPDT">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
</symbol>
<symbol name="TS2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CAP-US" prefix="C">
<gates>
<gate name="G$1" symbol="C-US"/>
</gates>
<devices>
<device name="1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206K" package="C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="C1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVRISP">
<gates>
<gate name="G$1" symbol="AVRISP"/>
</gates>
<devices>
<device name="SMD" package="2X03SMD">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="2X03">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR">
<gates>
<gate name="G$1" symbol="CERAMIC_RESONATOR"/>
</gates>
<devices>
<device name="" package="EFOBM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB1206" package="LED1206FAB">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LEDRGBNEW" prefix="D">
<gates>
<gate name="G$1" symbol="LED-RGB"/>
</gates>
<devices>
<device name="" package="P-LCC-4">
<connects>
<connect gate="G$1" pin="A2" pad="A"/>
<connect gate="G$1" pin="CBLUE" pad="B"/>
<connect gate="G$1" pin="CGREEN" pad="G"/>
<connect gate="G$1" pin="CRED" pad="R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REGULATOR" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="REGULATOR"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X2-SMD">
<gates>
<gate name="G$1" symbol="PINH2X2"/>
</gates>
<devices>
<device name="" package="2X02SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REGULATOR_SOT223" prefix="U">
<gates>
<gate name="G$1" symbol="REGULATOR_SOT223"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SLIDE-SWITCH" prefix="S">
<description>SMD slide-switch AYZ0102AGRLC as found in the fablab inventory.  Includes the mounting holes.

&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="G$1" symbol="SWITCH-SPDT"/>
</gates>
<devices>
<device name="" package="AYZ0102AGRLC">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6MM_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
<gates>
<gate name="2" symbol="TS2"/>
</gates>
<devices>
<device name="6MM_SWITCH" package="6MM_SWITCH">
<connects>
<connect gate="2" pin="P" pad="1"/>
<connect gate="2" pin="P1" pad="2"/>
<connect gate="2" pin="S" pad="3"/>
<connect gate="2" pin="S1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCC" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="VCC" symbol="VCC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="adxl345">
<description>3-Axis MEMS Digital accelerometer Analog Devices</description>
<packages>
<package name="LGA14">
<description>Land Grid Array (LGA-14)</description>
</package>
</packages>
<symbols>
<symbol name="ADXL345">
<pin name="VDDIO" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="GND$1" direction="pwr"/>
<pin name="GND$2" direction="pwr"/>
<pin name="GND$3" direction="pwr"/>
<pin name="NC"/>
<pin name="RESERVED$1"/>
<pin name="INT2" direction="out"/>
<pin name="INT1" direction="out"/>
<pin name="!CS" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="MISO" direction="out"/>
<pin name="MOSI" direction="in"/>
<pin name="RESERVED$2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ADXL345">
<description>3-Axis, ±2 g/±4 g/±8 g/±16 g Digital Accelerometer</description>
<gates>
<gate name="G$1" symbol="ADXL345"/>
</gates>
<devices>
<device name="" package="LGA14">
<connects>
<connect gate="G$1" pin="!CS" pad="P$7"/>
<connect gate="G$1" pin="GND$1" pad="P$2"/>
<connect gate="G$1" pin="GND$2" pad="P$4"/>
<connect gate="G$1" pin="GND$3" pad="P$5"/>
<connect gate="G$1" pin="INT1" pad="P$8"/>
<connect gate="G$1" pin="INT2" pad="P$9"/>
<connect gate="G$1" pin="MISO" pad="P$12"/>
<connect gate="G$1" pin="MOSI" pad="P$13"/>
<connect gate="G$1" pin="NC" pad="P$10"/>
<connect gate="G$1" pin="RESERVED$1" pad="P$3"/>
<connect gate="G$1" pin="RESERVED$2" pad="P$11"/>
<connect gate="G$1" pin="SCLK" pad="P$14"/>
<connect gate="G$1" pin="VDDIO" pad="P$1"/>
<connect gate="G$1" pin="VS" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply2">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
Please keep in mind, that these devices are necessary for the
automatic wiring of the supply signals.&lt;p&gt;
The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="+09V">
<pin name="+9V" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="+9V" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="+09V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="1" library="Atmel_By_element14_Batch_1-00" deviceset="ATMEGA328P-AU" device="" value="mega"/>
<part name="C1" library="fab" deviceset="CAP-US" device="1206FAB" value="1uF"/>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
<part name="P+1" library="supply1" deviceset="VCC" device=""/>
<part name="ISP" library="fab" deviceset="AVRISP" device="SMD"/>
<part name="R1" library="fab" deviceset="RES-US" device="1206FAB" value="10k"/>
<part name="RESONATOR" library="fab" deviceset="RESONATOR" device="" value="16MHz"/>
<part name="GND2" library="supply1" deviceset="GND" device=""/>
<part name="R2" library="fab" deviceset="RES-US" device="1206FAB" value="1k"/>
<part name="R3" library="fab" deviceset="RES-US" device="1206FAB" value="499"/>
<part name="R4" library="fab" deviceset="RES-US" device="1206FAB" value="1k"/>
<part name="P+2" library="supply1" deviceset="VCC" device=""/>
<part name="R5" library="fab" deviceset="RES-US" device="1206FAB" value="1k"/>
<part name="RED" library="fab" deviceset="LED" device="FAB1206" value="LED"/>
<part name="GND3" library="supply1" deviceset="GND" device=""/>
<part name="D1" library="fab" deviceset="LEDRGBNEW" device=""/>
<part name="IC1" library="fab" deviceset="REGULATOR" device="SOT23"/>
<part name="U$2" library="adxl345" deviceset="ADXL345" device=""/>
<part name="R7" library="fab" deviceset="RES-US" device="1206FAB" value="10k"/>
<part name="R8" library="fab" deviceset="RES-US" device="1206FAB" value="10k"/>
<part name="C2" library="fab" deviceset="CAP-US" device="1206FAB" value="0.1uF"/>
<part name="U$5" library="fab" deviceset="PINHD-2X2-SMD" device="" value="Supply"/>
<part name="U$6" library="fab" deviceset="PINHD-2X2-SMD" device="" value="Rx/Tx"/>
<part name="GND5" library="supply1" deviceset="GND" device=""/>
<part name="GND6" library="supply1" deviceset="GND" device=""/>
<part name="U1" library="fab" deviceset="REGULATOR_SOT223" device=""/>
<part name="S1" library="fab" deviceset="SLIDE-SWITCH" device=""/>
<part name="R9" library="fab" deviceset="RES-US" device="1206FAB" value="1k"/>
<part name="GREEN" library="fab" deviceset="LED" device="FAB1206" value="LED"/>
<part name="GND7" library="supply1" deviceset="GND" device=""/>
<part name="P+3" library="supply1" deviceset="VCC" device=""/>
<part name="SUPPLY1" library="supply2" deviceset="+9V" device=""/>
<part name="C3" library="fab" deviceset="CAP-US" device="1206FAB" value="10uF"/>
<part name="C4" library="fab" deviceset="CAP-US" device="1206FAB" value="100uF"/>
<part name="R10" library="fab" deviceset="RES-US" device="1206FAB" value="330"/>
<part name="R11" library="fab" deviceset="RES-US" device="1206FAB" value="110"/>
<part name="GND8" library="supply1" deviceset="GND" device=""/>
<part name="S2" library="fab" deviceset="6MM_SWITCH" device="6MM_SWITCH"/>
<part name="R12" library="fab" deviceset="RES-US" device="1206FAB" value="49.9k"/>
<part name="R13" library="fab" deviceset="RES-US" device="1206FAB" value="49.9k"/>
<part name="C5" library="fab" deviceset="CAP-US" device="1206FAB" value="10nF"/>
<part name="GND9" library="supply1" deviceset="GND" device=""/>
<part name="P+4" library="supply1" deviceset="VCC" device=""/>
<part name="S3" library="fab" deviceset="6MM_SWITCH" device="6MM_SWITCH"/>
<part name="R14" library="fab" deviceset="RES-US" device="1206FAB" value="49.9k"/>
<part name="R15" library="fab" deviceset="RES-US" device="1206FAB" value="49.9k"/>
<part name="C6" library="fab" deviceset="CAP-US" device="1206FAB" value="10nF"/>
<part name="GND10" library="supply1" deviceset="GND" device=""/>
<part name="P+5" library="supply1" deviceset="VCC" device=""/>
<part name="JUMPER" library="fab" deviceset="RES-US" device="1206FAB" value="0"/>
<part name="GND11" library="supply1" deviceset="GND" device=""/>
<part name="GND12" library="supply1" deviceset="GND" device=""/>
<part name="JUMPER1" library="fab" deviceset="RES-US" device="1206FAB" value="0"/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="GND">
<segment>
<pinref part="1" gate="A" pin="GND_2"/>
<pinref part="1" gate="A" pin="GND_3"/>
<pinref part="1" gate="A" pin="GND"/>
<pinref part="GND1" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="ISP" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="C1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="RESONATOR" gate="G$1" pin="2"/>
<pinref part="GND2" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="RED" gate="G$1" pin="C"/>
<pinref part="GND3" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="GND$1"/>
<pinref part="U$2" gate="G$1" pin="GND$2"/>
<pinref part="U$2" gate="G$1" pin="GND$3"/>
<pinref part="GND5" gate="1" pin="GND"/>
<pinref part="C2" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="MISO"/>
<pinref part="GND6" gate="1" pin="GND"/>
<pinref part="IC1" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="GREEN" gate="G$1" pin="C"/>
<pinref part="GND7" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C4" gate="G$1" pin="1"/>
<pinref part="GND8" gate="1" pin="GND"/>
<pinref part="R10" gate="G$1" pin="1"/>
<pinref part="C3" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="U$5" gate="G$1" pin="2"/>
<pinref part="U$5" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="C5" gate="G$1" pin="2"/>
<pinref part="S2" gate="2" pin="S1"/>
<pinref part="GND9" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C6" gate="G$1" pin="2"/>
<pinref part="S3" gate="2" pin="S1"/>
<pinref part="GND10" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND12" gate="1" pin="GND"/>
<pinref part="JUMPER" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="JUMPER" gate="G$1" pin="1"/>
<pinref part="GND11" gate="1" pin="GND"/>
</segment>
</net>
<net name="VCC">
<segment>
<pinref part="1" gate="A" pin="AVCC"/>
<pinref part="1" gate="A" pin="VCC"/>
<pinref part="1" gate="A" pin="VCC_2"/>
<pinref part="1" gate="A" pin="AREF"/>
<pinref part="P+1" gate="VCC" pin="VCC"/>
</segment>
<segment>
<pinref part="ISP" gate="G$1" pin="VCC"/>
</segment>
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="C1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="P+2" gate="VCC" pin="VCC"/>
<pinref part="D1" gate="G$1" pin="A2"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="IN"/>
</segment>
<segment>
<pinref part="U1" gate="G$1" pin="OUT1"/>
<pinref part="R9" gate="G$1" pin="1"/>
<pinref part="P+3" gate="VCC" pin="VCC"/>
<pinref part="C4" gate="G$1" pin="2"/>
<pinref part="R11" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="U$5" gate="G$1" pin="4"/>
<pinref part="U$5" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="P+4" gate="VCC" pin="VCC"/>
<pinref part="R13" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+5" gate="VCC" pin="VCC"/>
<pinref part="R15" gate="G$1" pin="2"/>
</segment>
</net>
<net name="RX">
<segment>
<pinref part="1" gate="A" pin="PD1"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="3"/>
</segment>
</net>
<net name="TX">
<segment>
<pinref part="1" gate="A" pin="PD0"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="4"/>
</segment>
<segment>
<pinref part="U$6" gate="G$1" pin="1"/>
</segment>
</net>
<net name="CTS">
<segment>
<pinref part="1" gate="A" pin="PD2"/>
</segment>
</net>
<net name="PD3">
<segment>
<pinref part="1" gate="A" pin="PD3"/>
</segment>
</net>
<net name="PD4">
<segment>
<pinref part="1" gate="A" pin="PD4"/>
</segment>
</net>
<net name="PD5">
<segment>
<pinref part="1" gate="A" pin="PD5"/>
</segment>
<segment>
<pinref part="R5" gate="G$1" pin="2"/>
</segment>
</net>
<net name="PD6">
<segment>
<pinref part="1" gate="A" pin="PD6"/>
</segment>
<segment>
<pinref part="R12" gate="G$1" pin="1"/>
<pinref part="C5" gate="G$1" pin="1"/>
</segment>
</net>
<net name="PD7">
<segment>
<pinref part="1" gate="A" pin="PD7"/>
</segment>
<segment>
<pinref part="R4" gate="G$1" pin="2"/>
</segment>
</net>
<net name="PC5">
<segment>
<pinref part="1" gate="A" pin="PC5"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="SCLK"/>
<pinref part="R8" gate="G$1" pin="1"/>
</segment>
</net>
<net name="PC4">
<segment>
<pinref part="1" gate="A" pin="PC4"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="MOSI"/>
<pinref part="R7" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="JUMPER1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="JUMPER1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="PC3">
<segment>
<pinref part="1" gate="A" pin="PC3"/>
</segment>
</net>
<net name="PC2">
<segment>
<pinref part="1" gate="A" pin="PC2"/>
</segment>
</net>
<net name="PC1">
<segment>
<pinref part="1" gate="A" pin="PC1"/>
</segment>
</net>
<net name="PC0">
<segment>
<pinref part="1" gate="A" pin="PC0"/>
</segment>
</net>
<net name="MOSI">
<segment>
<pinref part="ISP" gate="G$1" pin="MOSI"/>
</segment>
<segment>
<pinref part="1" gate="A" pin="PB3"/>
</segment>
</net>
<net name="PC6">
<segment>
<pinref part="ISP" gate="G$1" pin="RST"/>
<pinref part="R1" gate="G$1" pin="2"/>
<pinref part="1" gate="A" pin="PC6"/>
</segment>
</net>
<net name="SCK">
<segment>
<pinref part="ISP" gate="G$1" pin="SCK"/>
</segment>
<segment>
<pinref part="1" gate="A" pin="PB5"/>
</segment>
</net>
<net name="MISO">
<segment>
<pinref part="ISP" gate="G$1" pin="MISO"/>
</segment>
<segment>
<pinref part="1" gate="A" pin="PB4"/>
</segment>
</net>
<net name="PB7">
<segment>
<pinref part="1" gate="A" pin="PB7"/>
<pinref part="RESONATOR" gate="G$1" pin="3"/>
</segment>
</net>
<net name="PB6">
<segment>
<pinref part="1" gate="A" pin="PB6"/>
<pinref part="RESONATOR" gate="G$1" pin="1"/>
</segment>
</net>
<net name="ADC7">
<segment>
<pinref part="1" gate="A" pin="ADC7"/>
</segment>
</net>
<net name="ADC6">
<segment>
<pinref part="1" gate="A" pin="ADC6"/>
</segment>
</net>
<net name="N$11">
<segment>
<pinref part="R4" gate="G$1" pin="1"/>
<pinref part="D1" gate="G$1" pin="CRED"/>
</segment>
</net>
<net name="N$12">
<segment>
<pinref part="R3" gate="G$1" pin="1"/>
<pinref part="D1" gate="G$1" pin="CBLUE"/>
</segment>
</net>
<net name="N$18">
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="D1" gate="G$1" pin="CGREEN"/>
</segment>
</net>
<net name="N$6">
<segment>
<pinref part="R5" gate="G$1" pin="1"/>
<pinref part="RED" gate="G$1" pin="A"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="U$2" gate="G$1" pin="!CS"/>
<pinref part="U$2" gate="G$1" pin="VS"/>
<pinref part="U$2" gate="G$1" pin="VDDIO"/>
<pinref part="R7" gate="G$1" pin="2"/>
<pinref part="R8" gate="G$1" pin="2"/>
<pinref part="IC1" gate="G$1" pin="OUT"/>
<pinref part="C2" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="R9" gate="G$1" pin="2"/>
<pinref part="GREEN" gate="G$1" pin="A"/>
</segment>
</net>
<net name="N$7">
<segment>
<pinref part="S1" gate="G$1" pin="1"/>
<pinref part="U1" gate="G$1" pin="IN"/>
<pinref part="C3" gate="G$1" pin="2"/>
</segment>
</net>
<net name="+9V">
<segment>
<pinref part="S1" gate="G$1" pin="2"/>
<pinref part="SUPPLY1" gate="G$1" pin="+9V"/>
</segment>
</net>
<net name="N$8">
<segment>
<pinref part="U1" gate="G$1" pin="GND"/>
<pinref part="R10" gate="G$1" pin="2"/>
<pinref part="R11" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="R13" gate="G$1" pin="1"/>
<pinref part="S2" gate="2" pin="P1"/>
<pinref part="R12" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="R15" gate="G$1" pin="1"/>
<pinref part="S3" gate="2" pin="P1"/>
<pinref part="R14" gate="G$1" pin="2"/>
</segment>
</net>
<net name="PB0">
<segment>
<pinref part="1" gate="A" pin="PB0"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="2"/>
</segment>
</net>
<net name="PB1">
<segment>
<pinref part="1" gate="A" pin="PB1"/>
</segment>
<segment>
<pinref part="R3" gate="G$1" pin="2"/>
</segment>
</net>
<net name="PB2">
<segment>
<pinref part="1" gate="A" pin="PB2"/>
</segment>
<segment>
<pinref part="R14" gate="G$1" pin="1"/>
<pinref part="C6" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$5">
<segment>
<pinref part="U$2" gate="G$1" pin="INT1"/>
</segment>
</net>
<net name="N$9">
<segment>
<pinref part="U$2" gate="G$1" pin="INT2"/>
</segment>
</net>
<net name="N$10">
<segment>
<pinref part="U$2" gate="G$1" pin="NC"/>
</segment>
</net>
<net name="N$13">
<segment>
<pinref part="U$2" gate="G$1" pin="RESERVED$1"/>
</segment>
</net>
<net name="N$14">
<segment>
<pinref part="U$2" gate="G$1" pin="RESERVED$2"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
