<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.3">
<drawing>
<schematic>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PAD">
<pin name="P" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SMD2" prefix="PAD" uservalue="yes">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="PAD"/>
</gates>
<devices>
<device name="" package="SMD1,27-2,54">
<connects>
<connect gate="1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="+5V">
<pin name="+5V" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="+5V" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="+5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply2">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
Please keep in mind, that these devices are necessary for the
automatic wiring of the supply signals.&lt;p&gt;
The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="GND1">
<pin name="GND1" direction="sup"/>
</symbol>
<symbol name="GND2">
<pin name="GND2" direction="sup"/>
</symbol>
<symbol name="GND3">
<pin name="GND3" direction="sup"/>
</symbol>
<symbol name="GND4">
<pin name="GND4" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND1" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="GND1"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND2" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="GND2"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND3" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="GND3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND4" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="GND4"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="PAD1" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD2" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD3" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD4" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD5" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD6" library="wirepad" deviceset="SMD2" device=""/>
<part name="+5V" library="wirepad" deviceset="SMD2" device=""/>
<part name="D0" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD9" library="wirepad" deviceset="SMD2" device=""/>
<part name="GND" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD11" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD12" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD13" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD14" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD15" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD16" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD17" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD18" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD37" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD38" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD39" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD40" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD41" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD42" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD43" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD44" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD45" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD46" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD47" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD48" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD49" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD50" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD51" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD52" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD53" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD54" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD79" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD80" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD81" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD82" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD83" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD84" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD85" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD86" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD87" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD88" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD89" library="wirepad" deviceset="SMD2" device=""/>
<part name="PAD90" library="wirepad" deviceset="SMD2" device=""/>
<part name="P+1" library="supply1" deviceset="+5V" device=""/>
<part name="SUPPLY4" library="supply2" deviceset="GND1" device=""/>
<part name="SUPPLY5" library="supply2" deviceset="GND2" device=""/>
<part name="SUPPLY6" library="supply2" deviceset="GND3" device=""/>
<part name="SUPPLY1" library="supply2" deviceset="GND4" device=""/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="+5V">
<segment>
<pinref part="PAD12" gate="1" pin="P"/>
<pinref part="+5V" gate="1" pin="P"/>
</segment>
<segment>
<pinref part="P+1" gate="1" pin="+5V"/>
</segment>
</net>
<net name="N$8">
<segment>
<pinref part="PAD14" gate="1" pin="P"/>
<pinref part="PAD17" gate="1" pin="P"/>
</segment>
</net>
<net name="N$9">
<segment>
<pinref part="PAD13" gate="1" pin="P"/>
<pinref part="PAD18" gate="1" pin="P"/>
</segment>
</net>
<net name="N$20">
<segment>
<pinref part="PAD50" gate="1" pin="P"/>
<pinref part="PAD53" gate="1" pin="P"/>
</segment>
</net>
<net name="N$25">
<segment>
<pinref part="PAD38" gate="1" pin="P"/>
<pinref part="PAD41" gate="1" pin="P"/>
</segment>
</net>
<net name="N$37">
<segment>
<pinref part="PAD87" gate="1" pin="P"/>
<pinref part="PAD88" gate="1" pin="P"/>
</segment>
</net>
<net name="N$38">
<segment>
<pinref part="PAD86" gate="1" pin="P"/>
<pinref part="PAD89" gate="1" pin="P"/>
</segment>
</net>
<net name="N$41">
<segment>
<pinref part="PAD80" gate="1" pin="P"/>
<pinref part="PAD83" gate="1" pin="P"/>
</segment>
</net>
<net name="N$42">
<segment>
<pinref part="PAD79" gate="1" pin="P"/>
<pinref part="PAD84" gate="1" pin="P"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="PAD1" gate="1" pin="P"/>
<pinref part="PAD6" gate="1" pin="P"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="PAD52" gate="1" pin="P"/>
<pinref part="PAD51" gate="1" pin="P"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="PAD46" gate="1" pin="P"/>
<pinref part="PAD45" gate="1" pin="P"/>
</segment>
</net>
<net name="N$5">
<segment>
<pinref part="PAD40" gate="1" pin="P"/>
<pinref part="PAD39" gate="1" pin="P"/>
</segment>
</net>
<net name="N$6">
<segment>
<pinref part="PAD47" gate="1" pin="P"/>
<pinref part="PAD44" gate="1" pin="P"/>
</segment>
</net>
<net name="GND1">
<segment>
<pinref part="SUPPLY4" gate="G$1" pin="GND1"/>
<pinref part="PAD16" gate="1" pin="P"/>
<pinref part="PAD15" gate="1" pin="P"/>
<pinref part="PAD3" gate="1" pin="P"/>
<pinref part="PAD4" gate="1" pin="P"/>
<pinref part="GND" gate="1" pin="P"/>
<pinref part="PAD9" gate="1" pin="P"/>
</segment>
</net>
<net name="GND2">
<segment>
<pinref part="PAD49" gate="1" pin="P"/>
<pinref part="PAD54" gate="1" pin="P"/>
<pinref part="PAD48" gate="1" pin="P"/>
<pinref part="PAD43" gate="1" pin="P"/>
<pinref part="SUPPLY5" gate="G$1" pin="GND2"/>
<pinref part="PAD42" gate="1" pin="P"/>
<pinref part="PAD37" gate="1" pin="P"/>
</segment>
</net>
<net name="GND3">
<segment>
<pinref part="PAD81" gate="1" pin="P"/>
<pinref part="PAD82" gate="1" pin="P"/>
<pinref part="SUPPLY6" gate="G$1" pin="GND3"/>
</segment>
</net>
<net name="GND4">
<segment>
<pinref part="PAD85" gate="1" pin="P"/>
<pinref part="PAD90" gate="1" pin="P"/>
<pinref part="SUPPLY1" gate="G$1" pin="GND4"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="PAD2" gate="1" pin="P"/>
<pinref part="PAD5" gate="1" pin="P"/>
</segment>
</net>
<net name="N$10">
<segment>
<pinref part="D0" gate="1" pin="P"/>
<pinref part="PAD11" gate="1" pin="P"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
