<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.3">
<drawing>
<schematic>
<libraries>
<library name="fab">
<packages>
<package name="2X02SMD">
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="C1206FAB">
</package>
</packages>
<symbols>
<symbol name="PINH2X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="C-US">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-2X2-SMD">
<gates>
<gate name="G$1" symbol="PINH2X2"/>
</gates>
<devices>
<device name="" package="2X02SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-US" prefix="C">
<gates>
<gate name="G$1" symbol="C-US"/>
</gates>
<devices>
<device name="1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206K" package="C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="C1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply2">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
Please keep in mind, that these devices are necessary for the
automatic wiring of the supply signals.&lt;p&gt;
The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="+05V/4">
<pin name="+5V/4" direction="sup"/>
</symbol>
<symbol name="GND4">
<pin name="GND4" direction="sup"/>
</symbol>
<symbol name="GND5">
<pin name="GND5" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="+5V/4" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="+05V/4"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND4" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="GND4"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND5" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="GND5"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="NTC3" library="fab" deviceset="PINHD-2X2-SMD" device="" value=""/>
<part name="C3" library="fab" deviceset="CAP-US" device="1206FAB" value="1 nF"/>
<part name="R16" library="fab" deviceset="RES-US" device="1206FAB" value="10 k Ω"/>
<part name="R15" library="fab" deviceset="RES-US" device="1206FAB" value="NTC"/>
<part name="SUPPLY9" library="supply2" deviceset="+5V/4" device=""/>
<part name="SUPPLY10" library="supply2" deviceset="GND4" device=""/>
<part name="U$2" library="fab" deviceset="PINHD-2X2-SMD" device="" value=""/>
<part name="U$3" library="fab" deviceset="PINHD-2X2-SMD" device="" value=""/>
<part name="SUPPLY7" library="supply2" deviceset="GND5" device=""/>
</parts>
<sheets>
<sheet>
<plain>
<text>NTC_THERM3</text>
<text>NTC_THERM3_SENSOR</text>
</plain>
<busses>
</busses>
<nets>
<net name="GND4">
<segment>
<pinref part="NTC3" gate="G$1" pin="4"/>
<pinref part="SUPPLY10" gate="G$1" pin="GND4"/>
<pinref part="C3" gate="G$1" pin="2"/>
<pinref part="NTC3" gate="G$1" pin="3"/>
<pinref part="R16" gate="G$1" pin="2"/>
<pinref part="U$2" gate="G$1" pin="2"/>
<pinref part="U$2" gate="G$1" pin="4"/>
</segment>
</net>
<net name="N$11">
<segment>
<pinref part="R15" gate="G$1" pin="2"/>
<pinref part="U$3" gate="G$1" pin="3"/>
</segment>
</net>
<net name="N$15">
<segment>
<pinref part="R15" gate="G$1" pin="1"/>
<pinref part="U$3" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$23">
<segment>
<pinref part="R16" gate="G$1" pin="1"/>
<pinref part="NTC3" gate="G$1" pin="1"/>
<pinref part="U$2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="+5V/4">
<segment>
<pinref part="NTC3" gate="G$1" pin="2"/>
<pinref part="C3" gate="G$1" pin="1"/>
<pinref part="U$2" gate="G$1" pin="3"/>
<pinref part="SUPPLY9" gate="G$1" pin="+5V/4"/>
</segment>
</net>
<net name="GND5">
<segment>
<pinref part="U$3" gate="G$1" pin="4"/>
<pinref part="U$3" gate="G$1" pin="2"/>
<pinref part="SUPPLY7" gate="G$1" pin="GND5"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
