<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="95.428" y2="-0.127" width="0" layer="20"/>
<wire x1="95.428" y1="-0.127" x2="95.453" y2="67.935" width="0" layer="20"/>
<wire x1="95.453" y1="67.935" x2="0" y2="67.681" width="0" layer="20"/>
<wire x1="0" y1="67.681" x2="0" y2="0" width="0" layer="20"/>
<wire x1="23.622" y1="52.705" x2="24.892" y2="52.07" width="1.016" layer="46"/>
<wire x1="24.892" y1="52.07" x2="29.718" y2="62.484" width="1.016" layer="46" curve="-90"/>
<wire x1="29.718" y1="62.484" x2="31.623" y2="60.706" width="1.016" layer="46"/>
<wire x1="31.623" y1="60.706" x2="38.735" y2="51.308" width="1.016" layer="46" curve="-90"/>
<wire x1="38.735" y1="51.308" x2="46.355" y2="55.372" width="1.016" layer="46"/>
<wire x1="46.355" y1="55.372" x2="50.8" y2="43.434" width="1.016" layer="46" curve="-90"/>
<wire x1="50.8" y1="43.434" x2="50.165" y2="42.418" width="1.016" layer="46"/>
<wire x1="50.165" y1="42.418" x2="59.944" y2="36.576" width="1.016" layer="46" curve="-90"/>
<wire x1="59.944" y1="36.576" x2="58.928" y2="35.433" width="1.016" layer="46"/>
<wire x1="58.928" y1="35.433" x2="52.451" y2="29.337" width="1.016" layer="46" curve="-90"/>
<wire x1="52.451" y1="29.337" x2="51.689" y2="29.21" width="1.016" layer="46"/>
<wire x1="51.689" y1="29.21" x2="59.182" y2="14.986" width="1.016" layer="46" curve="-90"/>
<wire x1="59.182" y1="14.986" x2="60.833" y2="9.271" width="1.016" layer="46"/>
<wire x1="60.833" y1="9.271" x2="39.243" y2="4.318" width="1.016" layer="46" curve="-90"/>
<wire x1="39.243" y1="4.318" x2="35.433" y2="7.493" width="1.016" layer="46"/>
<wire x1="35.433" y1="7.493" x2="9.398" y2="6.858" width="1.016" layer="46" curve="-90"/>
<wire x1="9.398" y1="6.858" x2="12.192" y2="17.653" width="1.016" layer="46" curve="-31.802779"/>
<wire x1="12.192" y1="17.653" x2="1.905" y2="26.416" width="1.016" layer="46" curve="-90"/>
<wire x1="1.905" y1="26.416" x2="6.858" y2="33.147" width="1.016" layer="46"/>
<wire x1="6.858" y1="33.147" x2="6.35" y2="51.689" width="1.016" layer="46" curve="-90"/>
<wire x1="6.35" y1="51.689" x2="23.622" y2="52.705" width="1.016" layer="46" curve="-48.386418"/>
<wire x1="75.184" y1="64.008" x2="91.059" y2="64.008" width="1.016" layer="46"/>
<wire x1="91.059" y1="64.008" x2="93.726" y2="61.341" width="1.016" layer="46" curve="-90"/>
<wire x1="93.726" y1="61.341" x2="93.599" y2="53.467" width="1.016" layer="46"/>
<wire x1="93.599" y1="53.467" x2="91.313" y2="50.419" width="1.016" layer="46" curve="-90"/>
<wire x1="91.313" y1="50.419" x2="75.946" y2="50.419" width="1.016" layer="46"/>
<wire x1="75.946" y1="50.419" x2="72.517" y2="52.832" width="1.016" layer="46" curve="-90"/>
<wire x1="72.517" y1="52.832" x2="72.517" y2="61.341" width="1.016" layer="46"/>
<wire x1="72.517" y1="61.341" x2="75.184" y2="64.008" width="1.016" layer="46" curve="-90"/>
<wire x1="53.975" y1="63.373" x2="53.975" y2="46.863" width="1.016" layer="46"/>
<wire x1="53.975" y1="46.863" x2="56.642" y2="44.196" width="1.016" layer="46" curve="90"/>
<wire x1="56.642" y1="44.196" x2="68.072" y2="44.196" width="1.016" layer="46"/>
<wire x1="68.072" y1="44.196" x2="70.485" y2="46.609" width="1.016" layer="46" curve="90"/>
<wire x1="70.485" y1="46.609" x2="70.485" y2="63.373" width="1.016" layer="46"/>
<wire x1="70.485" y1="63.373" x2="68.707" y2="65.151" width="1.016" layer="46" curve="90"/>
<wire x1="68.707" y1="65.151" x2="56.134" y2="65.151" width="1.016" layer="46"/>
<wire x1="56.134" y1="65.151" x2="53.975" y2="63.373" width="1.016" layer="46" curve="90"/>
<text>KatPit</text>
<wire x1="72.39" y1="43.688" x2="78.867" y2="47.625" width="1.016" layer="46" curve="-90"/>
<wire x1="78.867" y1="47.625" x2="79.121" y2="46.736" width="1.016" layer="46"/>
<wire x1="79.121" y1="46.736" x2="81.788" y2="44.831" width="1.016" layer="46" curve="90"/>
<wire x1="81.788" y1="44.831" x2="86.741" y2="41.148" width="1.016" layer="46" curve="-90"/>
<wire x1="86.741" y1="41.148" x2="86.614" y2="39.116" width="1.016" layer="46"/>
<wire x1="86.614" y1="39.116" x2="84.074" y2="36.068" width="1.016" layer="46" curve="-90"/>
<wire x1="84.074" y1="36.068" x2="90.17" y2="36.576" width="1.016" layer="46"/>
<wire x1="90.17" y1="36.576" x2="92.583" y2="33.02" width="1.016" layer="46" curve="-90"/>
<wire x1="92.583" y1="33.02" x2="91.567" y2="33.02" width="1.016" layer="46"/>
<wire x1="91.567" y1="33.02" x2="89.662" y2="29.464" width="1.016" layer="46" curve="90"/>
<wire x1="89.662" y1="29.464" x2="89.662" y2="28.067" width="1.016" layer="46"/>
<wire x1="89.662" y1="28.067" x2="86.487" y2="25.273" width="1.016" layer="46" curve="-90"/>
<wire x1="86.487" y1="25.273" x2="82.296" y2="25.781" width="1.016" layer="46" curve="-90"/>
<wire x1="82.296" y1="25.781" x2="83.947" y2="21.717" width="1.016" layer="46"/>
<wire x1="83.947" y1="21.717" x2="74.549" y2="21.209" width="1.016" layer="46" curve="-90"/>
<wire x1="74.549" y1="21.209" x2="72.644" y2="27.559" width="1.016" layer="46" curve="-90"/>
<wire x1="72.644" y1="27.559" x2="71.12" y2="25.4" width="1.016" layer="46"/>
<wire x1="71.12" y1="25.4" x2="63.627" y2="25.019" width="1.016" layer="46" curve="-90"/>
<wire x1="63.627" y1="25.019" x2="60.579" y2="27.051" width="1.016" layer="46"/>
<wire x1="60.579" y1="27.051" x2="64.897" y2="31.75" width="1.016" layer="46" curve="-90"/>
<wire x1="64.897" y1="31.75" x2="68.326" y2="32.512" width="1.016" layer="46" curve="90"/>
<wire x1="68.326" y1="32.512" x2="67.945" y2="33.655" width="1.016" layer="46"/>
<wire x1="67.945" y1="33.655" x2="64.643" y2="34.29" width="1.016" layer="46" curve="90"/>
<wire x1="64.643" y1="34.29" x2="64.262" y2="36.576" width="1.016" layer="46"/>
<wire x1="64.262" y1="36.576" x2="68.58" y2="41.402" width="1.016" layer="46" curve="-90"/>
<wire x1="68.58" y1="41.402" x2="72.263" y2="39.37" width="1.016" layer="46" curve="-90"/>
<wire x1="72.263" y1="39.37" x2="72.263" y2="42.418" width="1.016" layer="46"/>
<wire x1="72.39" y1="43.688" x2="72.263" y2="42.418" width="1.016" layer="46"/>
<wire x1="62.738" y1="11.938" x2="67.818" y2="17.018" width="1.016" layer="46" curve="-90"/>
<wire x1="67.818" y1="17.018" x2="86.487" y2="17.018" width="1.016" layer="46"/>
<wire x1="86.487" y1="17.018" x2="91.567" y2="12.827" width="1.016" layer="46" curve="-90"/>
<wire x1="91.567" y1="12.827" x2="91.567" y2="5.334" width="1.016" layer="46"/>
<wire x1="91.567" y1="5.334" x2="87.884" y2="1.651" width="1.016" layer="46" curve="-90"/>
<wire x1="87.884" y1="1.651" x2="67.945" y2="1.651" width="1.016" layer="46"/>
<wire x1="67.945" y1="1.651" x2="62.738" y2="6.858" width="1.016" layer="46" curve="-90"/>
<wire x1="62.738" y1="6.858" x2="62.738" y2="11.938" width="1.016" layer="46"/>
<wire x1="62.738" y1="11.938" x2="62.738" y2="12.446" width="1.016" layer="46"/>
<wire x1="2.54" y1="63.5" x2="5.334" y2="65.913" width="1.016" layer="46" curve="-90"/>
<wire x1="19.304" y1="56.896" x2="4.572" y2="56.896" width="1.016" layer="46"/>
<wire x1="4.572" y1="56.896" x2="2.54" y2="58.928" width="1.016" layer="46" curve="-90"/>
<wire x1="2.54" y1="58.928" x2="2.54" y2="63.5" width="1.016" layer="46"/>
<wire x1="5.207" y1="65.913" x2="5.334" y2="65.913" width="1.016" layer="46"/>
<wire x1="5.334" y1="65.913" x2="18.161" y2="65.913" width="1.016" layer="46"/>
<wire x1="18.161" y1="65.913" x2="18.542" y2="65.913" width="1.016" layer="46"/>
<wire x1="18.161" y1="65.913" x2="20.701" y2="63.754" width="1.016" layer="46" curve="-90"/>
<wire x1="20.701" y1="63.754" x2="20.701" y2="59.055" width="1.016" layer="46"/>
<wire x1="20.701" y1="59.055" x2="19.304" y2="56.896" width="1.016" layer="46" curve="-90"/>
<text>2018</text>
<circle x="31.496" y="55.118" radius="1.17088125" width="1.016" layer="46"/>
<text>LIGHT</text>
<text>TEMP3</text>
<text>TEMP2</text>
<text>TEMP1</text>
<text>Light</text>
<text>StepperM</text>
<text>Neopxl</text>
<text>Temp1</text>
<text>Temp2</text>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="2X03SMD">
</package>
<package name="2X02SMD">
</package>
<package name="R1206FAB">
</package>
<package name="EFOBM">
</package>
<package name="1X06SMD">
</package>
<package name="OP1206">
</package>
<package name="DX4R005HJ5_64">
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="QFP80P900X900X120-32N">
</package>
</packages>
</library>
<library name="Bourns_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:04:24</description>
<packages>
<package name="INDC3225X22N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1 uF"/>
<element name="C2" library="fab" package="C1206FAB" value="1 nF"/>
<element name="D1" library="fab" package="LED1206FAB" value="LED GREEN"/>
<element name="D2" library="fab" package="LED1206FAB" value="LED RED"/>
<element name="J1" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="NEOPIX_C" library="fab" package="2X03SMD" value=""/>
<element name="NTC1" library="fab" package="2X02SMD" value=""/>
<element name="NTC2" library="fab" package="2X02SMD" value=""/>
<element name="NTC1_C" library="fab" package="2X02SMD" value=""/>
<element name="PHOTOTR_C" library="fab" package="2X02SMD" value=""/>
<element name="STEPPERM_C" library="fab" package="2X02SMD" value=""/>
<element name="PHOTOTR" library="fab" package="2X02SMD" value=""/>
<element name="NTC2_C" library="fab" package="2X02SMD" value=""/>
<element name="R1" library="fab" package="R1206FAB" value="NTC"/>
<element name="R10" library="fab" package="R1206FAB" value="10 k Ω"/>
<element name="R2" library="fab" package="R1206FAB" value="10 k Ω"/>
<element name="R3" library="fab" package="R1206FAB" value="10 k Ω"/>
<element name="R4" library="fab" package="R1206FAB" value="10 k Ω"/>
<element name="R5" library="fab" package="R1206FAB" value="499 Ω"/>
<element name="R6" library="fab" package="R1206FAB" value="1 k Ω"/>
<element name="R7" library="fab" package="R1206FAB" value="10 k Ω"/>
<element name="R8" library="fab" package="R1206FAB" value="NTC"/>
<element name="R9" library="fab" package="R1206FAB" value="10 k Ω"/>
<element name="RESONATOR" library="fab" package="EFOBM" value="16 MHz"/>
<element name="U$1" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="U$4" library="fab" package="OP1206" value="PHOTOTR-NPN"/>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="QFP80P900X900X120-32N" value="ATMEGA328P-AU">
<attribute name="MPN" value="ATMEGA328P-AU"/>
<attribute name="OC_FARNELL" value="1715486"/>
<attribute name="OC_NEWARK" value="14R4631"/>
<attribute name="PACKAGE" value="TQFP-32"/>
<attribute name="SUPPLIER" value="Atmel"/>
</element>
<element name="R14" library="fab" package="R1206FAB" value="0 k Ω"/>
<element name="R11" library="fab" package="R1206FAB" value="0 k Ω"/>
<element name="R12" library="fab" package="R1206FAB" value="0 k Ω"/>
<element name="R13" library="fab" package="R1206FAB" value="0 k Ω"/>
<element name="NTC3" library="fab" package="2X02SMD" value=""/>
<element name="C3" library="fab" package="C1206FAB" value="1 nF"/>
<element name="R16" library="fab" package="R1206FAB" value="10 k Ω"/>
<element name="R15" library="fab" package="R1206FAB" value="NTC"/>
<element name="U$2" library="fab" package="2X02SMD" value=""/>
<element name="U$3" library="fab" package="2X02SMD" value=""/>
<element name="C4" library="fab" package="C1206FAB" value="100 nF"/>
<element name="L1" library="Bourns_By_element14_Batch_1" package="INDC3225X22N" value="10 uH">
<attribute name="MPN" value="PM1210-100J-RC"/>
<attribute name="OC_FARNELL" value="1180465"/>
<attribute name="OC_NEWARK" value="63K3094"/>
<attribute name="SUPPLIER" value="BOURNS"/>
<attribute name="TOLERANCE" value="±5 %"/>
</element>
<element name="C5" library="fab" package="C1206FAB" value="1 uF"/>
<element name="R17" library="fab" package="R1206FAB" value="1 k Ω"/>
<element name="R18" library="fab" package="R1206FAB" value="2 k Ω"/>
<element name="R19" library="fab" package="R1206FAB" value="0 k Ω"/>
<element name="U$6" library="fab" package="DX4R005HJ5_64" value="MICRO-USB_1/64"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="3"/>
<contactref element="NEOPIX_C" pad="2"/>
<contactref element="NEOPIX_C" pad="1"/>
<contactref element="PHOTOTR_C" pad="1"/>
<contactref element="NTC2_C" pad="1"/>
<contactref element="STEPPERM_C" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="NTC1_C" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U$6" pad="VBUS"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="1"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="D1" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="NTC1_C" pad="3"/>
<contactref element="RESONATOR" pad="2"/>
<contactref element="PHOTOTR_C" pad="4"/>
<contactref element="PHOTOTR_C" pad="3"/>
<contactref element="J1" pad="6"/>
<contactref element="NTC2_C" pad="3"/>
<contactref element="NTC2_C" pad="4"/>
<contactref element="NEOPIX_C" pad="6"/>
<contactref element="NEOPIX_C" pad="5"/>
<contactref element="STEPPERM_C" pad="4"/>
<contactref element="STEPPERM_C" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R18" pad="1"/>
<contactref element="U$6" pad="GND"/>
</signal>
<signal name="N$9">
<contactref element="RESONATOR" pad="3"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$10">
<contactref element="RESONATOR" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="NTC1" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="R2" pad="2"/>
<contactref element="NTC1" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R5" pad="1"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R7" pad="2"/>
<contactref element="U$4" pad="COLLECTOR"/>
<contactref element="PHOTOTR" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="28"/>
<contactref element="PHOTOTR_C" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R9" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="NTC2" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="NEOPIX_C" pad="4"/>
<contactref element="NEOPIX_C" pad="3"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="+5V/2">
<contactref element="NTC1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="+5V/3">
<contactref element="NTC2" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="GND1">
<contactref element="U$4" pad="EMITTER"/>
<contactref element="PHOTOTR" pad="3"/>
<contactref element="PHOTOTR" pad="4"/>
</signal>
<signal name="GND3">
<contactref element="NTC2" pad="3"/>
<contactref element="R9" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="NTC2" pad="4"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="5"/>
<contactref element="R17" pad="1"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="NTC1_C" pad="4"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="N$17">
<contactref element="R10" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="4"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="29"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="15"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="27"/>
<contactref element="STEPPERM_C" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="J1" pad="3"/>
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="N$28">
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="N$30">
<contactref element="J1" pad="4"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="5"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="NTC1_C" pad="2"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="GND4">
<contactref element="NTC3" pad="4"/>
<contactref element="C3" pad="2"/>
<contactref element="NTC3" pad="3"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R15" pad="2"/>
<contactref element="U$3" pad="3"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="R15" pad="1"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="U$2" pad="1"/>
<contactref element="U$2" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="NTC3" pad="1"/>
</signal>
<signal name="+5V/1">
<contactref element="R7" pad="1"/>
<contactref element="PHOTOTR" pad="1"/>
</signal>
<signal name="+5V/4">
<contactref element="NTC3" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="GND2">
<contactref element="NTC1" pad="3"/>
<contactref element="R4" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="NTC2_C" pad="2"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="N$25">
<contactref element="U1" pad="18"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="20"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="R17" pad="2"/>
<contactref element="U1" pad="31"/>
</signal>
<signal name="N$29">
<contactref element="R11" pad="2"/>
<contactref element="R19" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
