<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
<wire x1="22.86" y1="3.81" x2="59.36" y2="3.81" width="0" layer="20"/>
<wire x1="59.36" y1="3.81" x2="59.36" y2="48.25" width="0" layer="20"/>
<wire x1="59.36" y1="48.25" x2="22.86" y2="48.25" width="0" layer="20"/>
<wire x1="22.86" y1="48.25" x2="22.86" y2="3.81" width="0" layer="20"/>
<wire x1="23.368" y1="47.244" x2="23.368" y2="4.191" width="1.016" layer="46"/>
<wire x1="23.368" y1="4.191" x2="23.241" y2="4.064" width="1.016" layer="46"/>
<wire x1="23.241" y1="4.064" x2="58.928" y2="4.064" width="1.016" layer="46"/>
<wire x1="58.928" y1="4.064" x2="59.436" y2="4.572" width="1.016" layer="46"/>
<wire x1="23.241" y1="47.625" x2="58.801" y2="47.625" width="1.016" layer="46"/>
<wire x1="58.801" y1="47.625" x2="58.928" y2="47.498" width="1.016" layer="46"/>
<wire x1="58.928" y1="47.498" x2="58.928" y2="4.318" width="1.016" layer="46"/>
<wire x1="58.928" y1="4.318" x2="58.801" y2="4.191" width="1.016" layer="46"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="R1206FAB">
</package>
<package name="EFOBM">
</package>
<package name="2X03SMD">
</package>
<package name="1X06SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="2X02SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1uF"/>
<element name="IC1" library="fab" package="SOIC14" value="ATTINY44-SSU"/>
<element name="R1" library="fab" package="R1206FAB" value="10k"/>
<element name="R4" library="fab" package="R1206FAB" value="1k"/>
<element name="U$1" library="fab" package="EFOBM" value="RESONATOR"/>
<element name="U$2" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$3" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="U$4" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$5" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$7" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="R2" library="fab" package="R1206FAB" value="0"/>
<element name="R3" library="fab" package="R1206FAB" value="0"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="3"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="U$5" pad="2"/>
<contactref element="U$7" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="4"/>
<contactref element="U$2" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="6"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="14"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$7" pad="6"/>
<contactref element="U$5" pad="4"/>
<contactref element="R3" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="3"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="3"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U$2" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="9"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="8"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U$4" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U$7" pad="4"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$23">
<contactref element="U$5" pad="3"/>
<contactref element="U$3" pad="5"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$13">
<contactref element="U$5" pad="1"/>
<contactref element="IC1" pad="13"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="11"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="6"/>
<contactref element="U$7" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U$7" pad="3"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$4">
<contactref element="U$7" pad="5"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
