<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<schematic>
<libraries>
<library name="fab">
<packages>
<package name="2X03SMD">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
</packages>
<symbols>
<symbol name="AVRISP">
<pin name="MISO" direction="pas" function="dot"/>
<pin name="VCC" direction="pas" function="dot"/>
<pin name="SCK" direction="pas" function="dot"/>
<pin name="MOSI" direction="pas" function="dot"/>
<pin name="RST" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AVRISP">
<gates>
<gate name="G$1" symbol="AVRISP"/>
</gates>
<devices>
<device name="SMD" package="2X03SMD">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="2X03">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="U$2" library="fab" deviceset="AVRISP" device="SMD"/>
<part name="R4" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R5" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R6" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R7" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="U$1" library="fab" deviceset="AVRISP" device="SMD"/>
<part name="R1" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="N$3">
<segment>
<pinref part="R5" gate="G$1" pin="1"/>
<pinref part="U$2" gate="G$1" pin="MISO"/>
</segment>
</net>
<net name="N$5">
<segment>
<pinref part="R4" gate="G$1" pin="1"/>
<pinref part="U$2" gate="G$1" pin="MOSI"/>
</segment>
</net>
<net name="N$6">
<segment>
<pinref part="R7" gate="G$1" pin="1"/>
<pinref part="U$2" gate="G$1" pin="SCK"/>
</segment>
</net>
<net name="N$7">
<segment>
<pinref part="R6" gate="G$1" pin="1"/>
<pinref part="U$2" gate="G$1" pin="RST"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="U$2" gate="G$1" pin="VCC"/>
<pinref part="R1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="U$1" gate="G$1" pin="VCC"/>
<pinref part="R1" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$8">
<segment>
<pinref part="R4" gate="G$1" pin="2"/>
<pinref part="U$1" gate="G$1" pin="MOSI"/>
</segment>
</net>
<net name="N$9">
<segment>
<pinref part="R6" gate="G$1" pin="2"/>
<pinref part="U$1" gate="G$1" pin="RST"/>
</segment>
</net>
<net name="N$10">
<segment>
<pinref part="U$1" gate="G$1" pin="SCK"/>
<pinref part="R7" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$12">
<segment>
<pinref part="U$1" gate="G$1" pin="MISO"/>
<pinref part="R5" gate="G$1" pin="2"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="U$2" gate="G$1" pin="GND"/>
<pinref part="U$1" gate="G$1" pin="GND"/>
<pinref part="GND1" gate="1" pin="GND"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
