<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="1.27" x2="36.5" y2="1.27" width="0" layer="20"/>
<wire x1="36.5" y1="1.27" x2="36.5" y2="45.71" width="0" layer="20"/>
<wire x1="36.5" y1="45.71" x2="0" y2="45.71" width="0" layer="20"/>
<wire x1="0" y1="45.71" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="2.667" y1="45.212" x2="3.175" y2="45.212" width="1.016" layer="46"/>
<wire x1="3.175" y1="45.212" x2="35.814" y2="45.212" width="1.016" layer="46"/>
<wire x1="35.814" y1="45.212" x2="35.814" y2="2.159" width="1.016" layer="46"/>
<wire x1="35.814" y1="2.159" x2="35.433" y2="1.778" width="1.016" layer="46"/>
<wire x1="35.433" y1="1.778" x2="0.889" y2="1.778" width="1.016" layer="46"/>
<wire x1="0.889" y1="1.778" x2="0.762" y2="1.905" width="1.016" layer="46"/>
<wire x1="0.635" y1="1.905" x2="0.635" y2="44.831" width="1.016" layer="46"/>
<wire x1="0.635" y1="44.831" x2="0.508" y2="44.958" width="1.016" layer="46"/>
<wire x1="0.508" y1="44.958" x2="0.762" y2="45.212" width="1.016" layer="46"/>
<wire x1="0.762" y1="45.212" x2="2.667" y2="45.212" width="1.016" layer="46"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="2X02SMD">
</package>
<package name="R1206FAB">
</package>
<package name="EFOBM">
</package>
<package name="2X03SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="USB_MINIB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1uF"/>
<element name="IC1" library="fab" package="SOIC14" value="ATTINY44-SSU"/>
<element name="PA0-13" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="PA1-12" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="PA3PA2-1011" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="PA7-6" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="PB2-5" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="R1" library="fab" package="R1206FAB" value="10k"/>
<element name="R4" library="fab" package="R1206FAB" value="1k"/>
<element name="U$1" library="fab" package="EFOBM" value="RESONATOR"/>
<element name="U$2" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$4" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$6" library="fab" package="USB_MINIB" value="USB_MINIB"/>
<element name="VCC" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="R2" library="fab" package="R1206FAB" value="0k"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="PB2-5" pad="2"/>
<contactref element="PA3PA2-1011" pad="2"/>
<contactref element="PA7-6" pad="2"/>
<contactref element="PA0-13" pad="2"/>
<contactref element="VCC" pad="2"/>
<contactref element="PA1-12" pad="2"/>
<contactref element="U$6" pad="VBUS"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="4"/>
<contactref element="U$2" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="6"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="14"/>
<contactref element="PB2-5" pad="3"/>
<contactref element="PA3PA2-1011" pad="3"/>
<contactref element="PA7-6" pad="3"/>
<contactref element="PA0-13" pad="3"/>
<contactref element="VCC" pad="3"/>
<contactref element="PA1-12" pad="3"/>
<contactref element="U$6" pad="GND"/>
<contactref element="R2" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="3"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="3"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U$2" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="9"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="8"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="5"/>
<contactref element="R4" pad="2"/>
<contactref element="PB2-5" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U$4" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="13"/>
<contactref element="PA0-13" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="12"/>
<contactref element="PA1-12" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="PA7-6" pad="1"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="11"/>
<contactref element="PA3PA2-1011" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="PA3PA2-1011" pad="4"/>
<contactref element="IC1" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
