<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<schematic>
<libraries>
<library name="adafruit">
<packages>
<package name="WS2812B">
</package>
<package name="WS2812B-NARROW">
</package>
<package name="LED3535">
</package>
</packages>
<symbols>
<symbol name="WS2812BLED">
<pin name="VDD" direction="pwr"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="DO" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WS2812B" prefix="LED">
<gates>
<gate name="G$1" symbol="WS2812BLED"/>
</gates>
<devices>
<device name="5050" package="WS2812B">
<connects>
<connect gate="G$1" pin="DI" pad="4-DIN"/>
<connect gate="G$1" pin="DO" pad="2-DOUT"/>
<connect gate="G$1" pin="GND" pad="3-GND"/>
<connect gate="G$1" pin="VDD" pad="1-VDD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_5050N" package="WS2812B-NARROW">
<connects>
<connect gate="G$1" pin="DI" pad="4-DIN"/>
<connect gate="G$1" pin="DO" pad="2-DOUT"/>
<connect gate="G$1" pin="GND" pad="3-GND"/>
<connect gate="G$1" pin="VDD" pad="1-VDD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3535" package="LED3535">
<connects>
<connect gate="G$1" pin="DI" pad="1"/>
<connect gate="G$1" pin="DO" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCC" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="VCC" symbol="VCC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="fab">
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="C1206FAB">
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="2X02SMD">
</package>
<package name="1X06SMD">
</package>
</packages>
<symbols>
<symbol name="C-US">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="PINH2X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="FTDI">
<pin name="GND"/>
<pin name="CTS"/>
<pin name="VCC"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="RTS"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CAP-US" prefix="C">
<gates>
<gate name="G$1" symbol="C-US"/>
</gates>
<devices>
<device name="1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206K" package="C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="C1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X2-SMD">
<gates>
<gate name="G$1" symbol="PINH2X2"/>
</gates>
<devices>
<device name="" package="2X02SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTDI-SMD-HEADER">
<gates>
<gate name="G$1" symbol="FTDI"/>
</gates>
<devices>
<device name="" package="1X06SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RTS" pad="6"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TXD" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="LED-3" library="adafruit" deviceset="WS2812B" device="5050"/>
<part name="LED-2" library="adafruit" deviceset="WS2812B" device="5050"/>
<part name="LED-4" library="adafruit" deviceset="WS2812B" device="5050"/>
<part name="LED-5" library="adafruit" deviceset="WS2812B" device="5050"/>
<part name="LED-6" library="adafruit" deviceset="WS2812B" device="5050"/>
<part name="LED-7" library="adafruit" deviceset="WS2812B" device="5050"/>
<part name="LED-9" library="adafruit" deviceset="WS2812B" device="5050"/>
<part name="LED-8" library="adafruit" deviceset="WS2812B" device="5050"/>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
<part name="GND3" library="supply1" deviceset="GND" device=""/>
<part name="GND4" library="supply1" deviceset="GND" device=""/>
<part name="GND5" library="supply1" deviceset="GND" device=""/>
<part name="GND6" library="supply1" deviceset="GND" device=""/>
<part name="GND7" library="supply1" deviceset="GND" device=""/>
<part name="GND8" library="supply1" deviceset="GND" device=""/>
<part name="GND9" library="supply1" deviceset="GND" device=""/>
<part name="P+1" library="supply1" deviceset="VCC" device=""/>
<part name="P+2" library="supply1" deviceset="VCC" device=""/>
<part name="P+3" library="supply1" deviceset="VCC" device=""/>
<part name="P+4" library="supply1" deviceset="VCC" device=""/>
<part name="P+5" library="supply1" deviceset="VCC" device=""/>
<part name="P+6" library="supply1" deviceset="VCC" device=""/>
<part name="P+7" library="supply1" deviceset="VCC" device=""/>
<part name="P+14" library="supply1" deviceset="VCC" device=""/>
<part name="C-2" library="fab" deviceset="CAP-US" device="1206FAB"/>
<part name="GND2" library="supply1" deviceset="GND" device=""/>
<part name="C-3" library="fab" deviceset="CAP-US" device="1206FAB"/>
<part name="GND16" library="supply1" deviceset="GND" device=""/>
<part name="C-6" library="fab" deviceset="CAP-US" device="1206FAB"/>
<part name="GND21" library="supply1" deviceset="GND" device=""/>
<part name="C-7" library="fab" deviceset="CAP-US" device="1206FAB"/>
<part name="GND22" library="supply1" deviceset="GND" device=""/>
<part name="C-5" library="fab" deviceset="CAP-US" device="1206FAB"/>
<part name="GND23" library="supply1" deviceset="GND" device=""/>
<part name="C-8" library="fab" deviceset="CAP-US" device="1206FAB"/>
<part name="GND25" library="supply1" deviceset="GND" device=""/>
<part name="C-9" library="fab" deviceset="CAP-US" device="1206FAB"/>
<part name="GND27" library="supply1" deviceset="GND" device=""/>
<part name="C-4" library="fab" deviceset="CAP-US" device="1206FAB"/>
<part name="GND28" library="supply1" deviceset="GND" device=""/>
<part name="LED-0" library="adafruit" deviceset="WS2812B" device="5050"/>
<part name="LED-1" library="adafruit" deviceset="WS2812B" device="5050"/>
<part name="GND33" library="supply1" deviceset="GND" device=""/>
<part name="GND34" library="supply1" deviceset="GND" device=""/>
<part name="P+17" library="supply1" deviceset="VCC" device=""/>
<part name="P+18" library="supply1" deviceset="VCC" device=""/>
<part name="C-1" library="fab" deviceset="CAP-US" device="1206FAB"/>
<part name="GND35" library="supply1" deviceset="GND" device=""/>
<part name="C-0" library="fab" deviceset="CAP-US" device="1206FAB"/>
<part name="GND36" library="supply1" deviceset="GND" device=""/>
<part name="C-30" library="fab" deviceset="CAP-US" device="1206FAB"/>
<part name="R1" library="fab" deviceset="RES-US" device="1206FAB" value="499"/>
<part name="U$1" library="fab" deviceset="PINHD-2X2-SMD" device=""/>
<part name="P+31" library="supply1" deviceset="VCC" device=""/>
<part name="GND62" library="supply1" deviceset="GND" device=""/>
<part name="GND63" library="supply1" deviceset="GND" device=""/>
<part name="U$3" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="GND10" library="supply1" deviceset="GND" device=""/>
<part name="U$2" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="GND11" library="supply1" deviceset="GND" device=""/>
<part name="U$4" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="GND12" library="supply1" deviceset="GND" device=""/>
<part name="U$5" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="GND13" library="supply1" deviceset="GND" device=""/>
<part name="U$6" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="GND14" library="supply1" deviceset="GND" device=""/>
<part name="U$7" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="GND15" library="supply1" deviceset="GND" device=""/>
<part name="U$8" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="GND17" library="supply1" deviceset="GND" device=""/>
<part name="U$9" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="GND18" library="supply1" deviceset="GND" device=""/>
<part name="U$10" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="GND19" library="supply1" deviceset="GND" device=""/>
<part name="P+20" library="supply1" deviceset="VCC" device=""/>
<part name="P+21" library="supply1" deviceset="VCC" device=""/>
<part name="P+22" library="supply1" deviceset="VCC" device=""/>
<part name="P+23" library="supply1" deviceset="VCC" device=""/>
<part name="P+24" library="supply1" deviceset="VCC" device=""/>
<part name="P+25" library="supply1" deviceset="VCC" device=""/>
<part name="P+26" library="supply1" deviceset="VCC" device=""/>
<part name="P+27" library="supply1" deviceset="VCC" device=""/>
<part name="P+28" library="supply1" deviceset="VCC" device=""/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="GND">
<segment>
<pinref part="LED-2" gate="G$1" pin="GND"/>
<pinref part="GND1" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="LED-3" gate="G$1" pin="GND"/>
<pinref part="GND3" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="LED-4" gate="G$1" pin="GND"/>
<pinref part="GND4" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="LED-5" gate="G$1" pin="GND"/>
<pinref part="GND5" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="LED-6" gate="G$1" pin="GND"/>
<pinref part="GND6" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="LED-7" gate="G$1" pin="GND"/>
<pinref part="GND7" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="LED-8" gate="G$1" pin="GND"/>
<pinref part="GND8" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="LED-9" gate="G$1" pin="GND"/>
<pinref part="GND9" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND2" gate="1" pin="GND"/>
<pinref part="C-2" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND16" gate="1" pin="GND"/>
<pinref part="C-3" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND21" gate="1" pin="GND"/>
<pinref part="C-6" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND22" gate="1" pin="GND"/>
<pinref part="C-7" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND23" gate="1" pin="GND"/>
<pinref part="C-5" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND25" gate="1" pin="GND"/>
<pinref part="C-8" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND27" gate="1" pin="GND"/>
<pinref part="C-9" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND28" gate="1" pin="GND"/>
<pinref part="C-4" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="LED-0" gate="G$1" pin="GND"/>
<pinref part="GND33" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="LED-1" gate="G$1" pin="GND"/>
<pinref part="GND34" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND35" gate="1" pin="GND"/>
<pinref part="C-1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND36" gate="1" pin="GND"/>
<pinref part="C-0" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND63" gate="1" pin="GND"/>
<pinref part="U$1" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="GND62" gate="1" pin="GND"/>
<pinref part="C-30" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND10" gate="1" pin="GND"/>
<pinref part="U$3" gate="G$1" pin="CTS"/>
</segment>
<segment>
<pinref part="GND11" gate="1" pin="GND"/>
<pinref part="U$2" gate="G$1" pin="CTS"/>
</segment>
<segment>
<pinref part="GND12" gate="1" pin="GND"/>
<pinref part="U$4" gate="G$1" pin="CTS"/>
</segment>
<segment>
<pinref part="GND13" gate="1" pin="GND"/>
<pinref part="U$5" gate="G$1" pin="CTS"/>
</segment>
<segment>
<pinref part="GND15" gate="1" pin="GND"/>
<pinref part="U$7" gate="G$1" pin="CTS"/>
</segment>
<segment>
<pinref part="GND17" gate="1" pin="GND"/>
<pinref part="U$8" gate="G$1" pin="CTS"/>
</segment>
<segment>
<pinref part="GND18" gate="1" pin="GND"/>
<pinref part="U$9" gate="G$1" pin="CTS"/>
</segment>
<segment>
<pinref part="GND19" gate="1" pin="GND"/>
<pinref part="U$10" gate="G$1" pin="CTS"/>
</segment>
<segment>
<pinref part="GND14" gate="1" pin="GND"/>
<pinref part="U$6" gate="G$1" pin="CTS"/>
</segment>
</net>
<net name="VCC">
<segment>
<pinref part="LED-3" gate="G$1" pin="VDD"/>
<pinref part="P+1" gate="VCC" pin="VCC"/>
<pinref part="C-3" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="LED-4" gate="G$1" pin="VDD"/>
<pinref part="P+2" gate="VCC" pin="VCC"/>
<pinref part="C-4" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="LED-5" gate="G$1" pin="VDD"/>
<pinref part="P+3" gate="VCC" pin="VCC"/>
<pinref part="C-5" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="LED-6" gate="G$1" pin="VDD"/>
<pinref part="P+4" gate="VCC" pin="VCC"/>
<pinref part="C-6" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="LED-7" gate="G$1" pin="VDD"/>
<pinref part="P+5" gate="VCC" pin="VCC"/>
<pinref part="C-7" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="LED-8" gate="G$1" pin="VDD"/>
<pinref part="P+6" gate="VCC" pin="VCC"/>
<pinref part="C-8" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="LED-9" gate="G$1" pin="VDD"/>
<pinref part="P+7" gate="VCC" pin="VCC"/>
<pinref part="C-9" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="LED-2" gate="G$1" pin="VDD"/>
<pinref part="P+14" gate="VCC" pin="VCC"/>
<pinref part="C-2" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="LED-0" gate="G$1" pin="VDD"/>
<pinref part="P+17" gate="VCC" pin="VCC"/>
<pinref part="C-0" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="LED-1" gate="G$1" pin="VDD"/>
<pinref part="P+18" gate="VCC" pin="VCC"/>
<pinref part="C-1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="2"/>
<pinref part="P+31" gate="VCC" pin="VCC"/>
<pinref part="C-30" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="P+20" gate="VCC" pin="VCC"/>
<pinref part="U$10" gate="G$1" pin="TXD"/>
</segment>
<segment>
<pinref part="P+21" gate="VCC" pin="VCC"/>
<pinref part="U$3" gate="G$1" pin="TXD"/>
</segment>
<segment>
<pinref part="P+22" gate="VCC" pin="VCC"/>
<pinref part="U$2" gate="G$1" pin="TXD"/>
</segment>
<segment>
<pinref part="P+23" gate="VCC" pin="VCC"/>
<pinref part="U$8" gate="G$1" pin="TXD"/>
</segment>
<segment>
<pinref part="P+24" gate="VCC" pin="VCC"/>
<pinref part="U$9" gate="G$1" pin="TXD"/>
</segment>
<segment>
<pinref part="P+25" gate="VCC" pin="VCC"/>
<pinref part="U$7" gate="G$1" pin="TXD"/>
</segment>
<segment>
<pinref part="P+26" gate="VCC" pin="VCC"/>
<pinref part="U$6" gate="G$1" pin="TXD"/>
</segment>
<segment>
<pinref part="P+27" gate="VCC" pin="VCC"/>
<pinref part="U$5" gate="G$1" pin="TXD"/>
</segment>
<segment>
<pinref part="P+28" gate="VCC" pin="VCC"/>
<pinref part="U$4" gate="G$1" pin="TXD"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="LED-4" gate="G$1" pin="DI"/>
<pinref part="U$5" gate="G$1" pin="VCC"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="LED-4" gate="G$1" pin="DO"/>
<pinref part="LED-5" gate="G$1" pin="DI"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="LED-6" gate="G$1" pin="DI"/>
<pinref part="U$7" gate="G$1" pin="VCC"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="LED-2" gate="G$1" pin="DO"/>
<pinref part="LED-3" gate="G$1" pin="DI"/>
</segment>
</net>
<net name="N$5">
<segment>
<pinref part="LED-6" gate="G$1" pin="DO"/>
<pinref part="LED-7" gate="G$1" pin="DI"/>
</segment>
</net>
<net name="N$6">
<segment>
<pinref part="LED-7" gate="G$1" pin="DO"/>
<pinref part="U$9" gate="G$1" pin="VCC"/>
</segment>
</net>
<net name="N$7">
<segment>
<pinref part="LED-8" gate="G$1" pin="DO"/>
<pinref part="LED-9" gate="G$1" pin="DI"/>
</segment>
</net>
<net name="N$15">
<segment>
<pinref part="LED-0" gate="G$1" pin="DO"/>
<pinref part="LED-1" gate="G$1" pin="DI"/>
</segment>
</net>
<net name="N$16">
<segment>
<pinref part="LED-2" gate="G$1" pin="DI"/>
<pinref part="U$2" gate="G$1" pin="VCC"/>
</segment>
</net>
<net name="N$32">
<segment>
<pinref part="U$1" gate="G$1" pin="1"/>
<pinref part="R1" gate="G$1" pin="2"/>
<pinref part="U$10" gate="G$1" pin="VCC"/>
</segment>
</net>
<net name="N$31">
<segment>
<pinref part="LED-0" gate="G$1" pin="DI"/>
<pinref part="R1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$9">
<segment>
<pinref part="LED-1" gate="G$1" pin="DO"/>
<pinref part="U$3" gate="G$1" pin="VCC"/>
</segment>
</net>
<net name="N$10">
<segment>
<pinref part="LED-3" gate="G$1" pin="DO"/>
<pinref part="U$4" gate="G$1" pin="VCC"/>
</segment>
</net>
<net name="N$11">
<segment>
<pinref part="LED-5" gate="G$1" pin="DO"/>
<pinref part="U$6" gate="G$1" pin="VCC"/>
</segment>
</net>
<net name="N$12">
<segment>
<pinref part="LED-8" gate="G$1" pin="DI"/>
<pinref part="U$8" gate="G$1" pin="VCC"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
