<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="37.592" y1="23.241" x2="108.204" y2="23.094" width="0" layer="20"/>
<wire x1="108.204" y1="23.094" x2="108.184" y2="80.569" width="0" layer="20"/>
<wire x1="108.184" y1="80.569" x2="37.973" y2="80.696" width="0" layer="20"/>
<wire x1="37.338" y1="80.95" x2="37.465" y2="23.495" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="C1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="R1206FAB">
</package>
<package name="1X06SMD">
</package>
<package name="2X03SMD">
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SM49">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="QFP80P900X900X120-32N">
</package>
</packages>
</library>
<library name="new-pinhead-2">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de, Modified by Cougar@CasaDelGato.Com&lt;/author&gt;</description>
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X09">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BUTTON" library="fab" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="fab" package="C1206FAB" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="fab" package="C1206FAB" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="fab" package="C1206FAB" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CRYSTAL" library="crystal" package="SM49" value="16Mhz">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="LEDGREEN" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="10kOhm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206FAB" value="499ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="QFP80P900X900X120-32N" value="ATMEGA328P-AU">
<attribute name="MPN" value="ATMEGA328P-AU"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1715486"/>
<attribute name="OC_NEWARK" value="14R4631"/>
<attribute name="PACKAGE" value="TQFP-32"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="VALUE"/>
</element>
<element name="PINHEAD-2" library="pinhead" package="1X09" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PINHEAD-1" library="pinhead" package="1X07" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="fab" package="C1206FAB" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FTDI-CABLE" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="PINHEAD-3" library="new-pinhead-2" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JUMPER-RESISTOR" library="fab" package="R1206FAB" value="0Ohm resistor">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JUMPER-RESISTOR-2" library="fab" package="R1206FAB" value="0Ohm resistor">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VCC-GND-PINHEAD" library="fab" package="2X03SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD1" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="20"/>
<contactref element="C5" pad="2"/>
<contactref element="JUMPER-RESISTOR" pad="1"/>
<contactref element="VCC-GND-PINHEAD" pad="3"/>
<contactref element="VCC-GND-PINHEAD" pad="4"/>
<contactref element="PAD2" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="15"/>
<contactref element="PINHEAD-2" pad="7"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="16"/>
<contactref element="PINHEAD-2" pad="8"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="17"/>
<contactref element="R2" pad="1"/>
<contactref element="PINHEAD-2" pad="9"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="7"/>
<contactref element="CRYSTAL" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="CRYSTAL" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="BUTTON" pad="1"/>
<contactref element="LEDGREEN" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="JUMPER-RESISTOR-2" pad="1"/>
<contactref element="VCC-GND-PINHEAD" pad="1"/>
<contactref element="VCC-GND-PINHEAD" pad="2"/>
<contactref element="PAD1" pad="1"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="30"/>
<contactref element="PINHEAD-3" pad="1"/>
<contactref element="FTDI-CABLE" pad="5"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="31"/>
<contactref element="PINHEAD-3" pad="2"/>
<contactref element="FTDI-CABLE" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="2"/>
<contactref element="LEDGREEN" pad="1"/>
</signal>
<signal name="PC0">
<contactref element="U1" pad="23"/>
<contactref element="PINHEAD-1" pad="2"/>
</signal>
<signal name="PC2">
<contactref element="U1" pad="25"/>
<contactref element="PINHEAD-1" pad="4"/>
</signal>
<signal name="PC3">
<contactref element="U1" pad="26"/>
<contactref element="PINHEAD-1" pad="5"/>
</signal>
<signal name="PC4">
<contactref element="U1" pad="27"/>
<contactref element="PINHEAD-1" pad="6"/>
</signal>
<signal name="PC5">
<contactref element="U1" pad="28"/>
<contactref element="PINHEAD-1" pad="7"/>
</signal>
<signal name="PB2">
<contactref element="U1" pad="14"/>
<contactref element="PINHEAD-2" pad="6"/>
</signal>
<signal name="PB1">
<contactref element="U1" pad="13"/>
<contactref element="PINHEAD-2" pad="5"/>
</signal>
<signal name="PB0">
<contactref element="U1" pad="12"/>
<contactref element="PINHEAD-2" pad="4"/>
</signal>
<signal name="ADC6">
<contactref element="U1" pad="19"/>
<contactref element="PAD3" pad="1"/>
</signal>
<signal name="ADC7">
<contactref element="U1" pad="22"/>
<contactref element="PINHEAD-1" pad="1"/>
</signal>
<signal name="PD2">
<contactref element="U1" pad="32"/>
<contactref element="PINHEAD-3" pad="3"/>
</signal>
<signal name="PD3">
<contactref element="U1" pad="1"/>
<contactref element="PINHEAD-3" pad="4"/>
</signal>
<signal name="PD5">
<contactref element="U1" pad="9"/>
<contactref element="PINHEAD-2" pad="1"/>
</signal>
<signal name="PD6">
<contactref element="U1" pad="10"/>
<contactref element="PINHEAD-2" pad="2"/>
</signal>
<signal name="PD7">
<contactref element="U1" pad="11"/>
<contactref element="PINHEAD-2" pad="3"/>
</signal>
<signal name="PD4">
<contactref element="U1" pad="2"/>
<contactref element="PINHEAD-3" pad="5"/>
</signal>
<signal name="PC1">
<contactref element="U1" pad="24"/>
<contactref element="PINHEAD-1" pad="3"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="29"/>
<contactref element="C3" pad="1"/>
<contactref element="BUTTON" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="PINHEAD-3" pad="6"/>
</signal>
<signal name="RTS">
<contactref element="C3" pad="2"/>
<contactref element="FTDI-CABLE" pad="6"/>
</signal>
<signal name="CTS">
<contactref element="FTDI-CABLE" pad="2"/>
</signal>
<signal name="VCC(JUMPER)">
<contactref element="FTDI-CABLE" pad="3"/>
<contactref element="JUMPER-RESISTOR" pad="2"/>
</signal>
<signal name="GND(JUMPER)">
<contactref element="FTDI-CABLE" pad="1"/>
<contactref element="JUMPER-RESISTOR-2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
