<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<schematic>
<libraries>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="QFP80P900X900X120-32N">
</package>
</packages>
<symbols>
<symbol name="ATMEGA328P-AU">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="ADC6" direction="in"/>
<pin name="ADC7" direction="in"/>
<pin name="AREF" direction="in"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATMEGA328P-AU" prefix="U">
<description>8-bit Microcontroller with In-System Programmable Flash</description>
<gates>
<gate name="A" symbol="ATMEGA328P-AU"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X120-32N">
<connects>
<connect gate="A" pin="ADC6" pad="19"/>
<connect gate="A" pin="ADC7" pad="22"/>
<connect gate="A" pin="AREF" pad="20"/>
<connect gate="A" pin="AVCC" pad="18"/>
<connect gate="A" pin="GND" pad="21"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="GND_3" pad="5"/>
<connect gate="A" pin="PB0" pad="12"/>
<connect gate="A" pin="PB1" pad="13"/>
<connect gate="A" pin="PB2" pad="14"/>
<connect gate="A" pin="PB3" pad="15"/>
<connect gate="A" pin="PB4" pad="16"/>
<connect gate="A" pin="PB5" pad="17"/>
<connect gate="A" pin="PB6" pad="7"/>
<connect gate="A" pin="PB7" pad="8"/>
<connect gate="A" pin="PC0" pad="23"/>
<connect gate="A" pin="PC1" pad="24"/>
<connect gate="A" pin="PC2" pad="25"/>
<connect gate="A" pin="PC3" pad="26"/>
<connect gate="A" pin="PC4" pad="27"/>
<connect gate="A" pin="PC5" pad="28"/>
<connect gate="A" pin="PC6" pad="29"/>
<connect gate="A" pin="PD0" pad="30"/>
<connect gate="A" pin="PD1" pad="31"/>
<connect gate="A" pin="PD2" pad="32"/>
<connect gate="A" pin="PD3" pad="1"/>
<connect gate="A" pin="PD4" pad="2"/>
<connect gate="A" pin="PD5" pad="9"/>
<connect gate="A" pin="PD6" pad="10"/>
<connect gate="A" pin="PD7" pad="11"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VCC_2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATMEGA328P-AU"/>
<attribute name="OC_FARNELL" value="1715486"/>
<attribute name="OC_NEWARK" value="14R4631"/>
<attribute name="PACKAGE" value="TQFP-32"/>
<attribute name="SUPPLIER" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="VCC">
<pin name="VCC" direction="sup"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="VCC" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="VCC" symbol="VCC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="fab">
<packages>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="1X06SMD">
</package>
<package name="2X02SMD">
</package>
</packages>
<symbols>
<symbol name="LED">
<description>LED</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CAP-NONPOLARIZED">
<description>non-polarized capacitor</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="TS2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
<symbol name="FTDI">
<pin name="GND"/>
<pin name="CTS"/>
<pin name="VCC"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="RTS"/>
</symbol>
<symbol name="PINH2X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LED">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB1206" package="LED1206FAB">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-UNPOLARIZED" prefix="C" uservalue="yes">
<gates>
<gate name="&gt;NAME" symbol="CAP-NONPOLARIZED"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB" package="C1206FAB">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6MM_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
<gates>
<gate name="2" symbol="TS2"/>
</gates>
<devices>
<device name="6MM_SWITCH" package="6MM_SWITCH">
<connects>
<connect gate="2" pin="P" pad="1"/>
<connect gate="2" pin="P1" pad="2"/>
<connect gate="2" pin="S" pad="3"/>
<connect gate="2" pin="S1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTDI-SMD-HEADER">
<gates>
<gate name="G$1" symbol="FTDI"/>
</gates>
<devices>
<device name="" package="1X06SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RTS" pad="6"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TXD" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X2-SMD">
<gates>
<gate name="G$1" symbol="PINH2X2"/>
</gates>
<devices>
<device name="" package="2X02SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CSM-7X-DU">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;&lt;p&gt;
Source: www.ecsxtal.com .. Crystal 3.6864MHz CSM_7X_DU.PDF</description>
</package>
</packages>
<symbols>
<symbol name="Q">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CSM-7X-DU" prefix="Q">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;&lt;p&gt;
Source: www.ecsxtal.com .. Crystal 3.6864MHz CSM_7X_DU.PDF</description>
<gates>
<gate name="P" symbol="Q"/>
</gates>
<devices>
<device name="" package="CSM-7X-DU">
<connects>
<connect gate="P" pin="1" pad="1"/>
<connect gate="P" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X07/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X09">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X09/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PINHD7">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD9">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X7" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD7"/>
</gates>
<devices>
<device name="" package="1X07">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X07/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X9" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD9"/>
</gates>
<devices>
<device name="" package="1X09">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X09/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PAD">
<pin name="P" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SMD2" prefix="PAD" uservalue="yes">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="PAD"/>
</gates>
<devices>
<device name="" package="SMD1,27-2,54">
<connects>
<connect gate="1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="U1" library="Atmel_By_element14_Batch_1-00" deviceset="ATMEGA328P-AU" device=""/>
<part name="P+1" library="supply1" deviceset="VCC" device=""/>
<part name="CRYSTAL" library="crystal" deviceset="CSM-7X-DU" device="" value="16MHz"/>
<part name="C1" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="22pF"/>
<part name="C2" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="22pF"/>
<part name="GND2" library="supply1" deviceset="GND" device=""/>
<part name="GND4" library="supply1" deviceset="GND" device=""/>
<part name="R2" library="fab" deviceset="RES-US" device="1206FAB" value="10KOhm"/>
<part name="C3" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="0.1uF"/>
<part name="S1" library="fab" deviceset="6MM_SWITCH" device="6MM_SWITCH"/>
<part name="R3" library="fab" deviceset="RES-US" device="1206FAB" value="499Ohm"/>
<part name="GND3" library="supply1" deviceset="GND" device=""/>
<part name="U$2" library="fab" deviceset="LED" device="FAB1206"/>
<part name="GND5" library="supply1" deviceset="GND" device=""/>
<part name="C4" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="10uF"/>
<part name="FTDI" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="JP2" library="pinhead" deviceset="PINHD-1X7" device=""/>
<part name="JP3" library="pinhead" deviceset="PINHD-1X9" device=""/>
<part name="VCC/GND" library="fab" deviceset="PINHD-2X2-SMD" device=""/>
<part name="GND" library="wirepad" deviceset="SMD2" device=""/>
<part name="VCC" library="wirepad" deviceset="SMD2" device=""/>
<part name="ADC6" library="wirepad" deviceset="SMD2" device=""/>
<part name="R1" library="fab" deviceset="RES-US" device="1206FAB" value="0Ohm">
<attribute name="SPICEPREFIX" value="R"/>
</part>
<part name="R4" library="fab" deviceset="RES-US" device="1206FAB" value="0ohm"/>
<part name="EXTRAPINHEADER" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
</parts>
<sheets>
<sheet>
<plain>
<text>FTDI CABLE</text>
<text>EXTRA PIN HEADERS</text>
<text>EXTRA PIN  HEADERS</text>
<text>VCC &amp; GND</text>
</plain>
<busses>
</busses>
<nets>
<net name="VCC">
<segment>
<pinref part="U1" gate="A" pin="VCC_2"/>
<pinref part="P+1" gate="VCC" pin="VCC"/>
<pinref part="U1" gate="A" pin="VCC"/>
<pinref part="U1" gate="A" pin="AVCC"/>
</segment>
<segment>
<pinref part="U1" gate="A" pin="AREF"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="C4" gate="&gt;NAME" pin="2"/>
</segment>
<segment>
<pinref part="VCC/GND" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="VCC/GND" gate="G$1" pin="4"/>
</segment>
<segment>
<pinref part="VCC" gate="1" pin="P"/>
</segment>
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="ADC6">
<segment>
<pinref part="U1" gate="A" pin="ADC6"/>
</segment>
<segment>
<pinref part="ADC6" gate="1" pin="P"/>
</segment>
</net>
<net name="ADC7">
<segment>
<pinref part="U1" gate="A" pin="ADC7"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="1"/>
</segment>
</net>
<net name="PB0">
<segment>
<pinref part="U1" gate="A" pin="PB0"/>
</segment>
<segment>
<pinref part="JP3" gate="A" pin="4"/>
</segment>
</net>
<net name="PB1">
<segment>
<pinref part="U1" gate="A" pin="PB1"/>
</segment>
<segment>
<pinref part="JP3" gate="A" pin="5"/>
</segment>
</net>
<net name="PB2">
<segment>
<pinref part="U1" gate="A" pin="PB2"/>
</segment>
<segment>
<pinref part="JP3" gate="A" pin="6"/>
</segment>
</net>
<net name="MOSI">
<segment>
<pinref part="U1" gate="A" pin="PB3"/>
</segment>
<segment>
<pinref part="JP3" gate="A" pin="7"/>
</segment>
</net>
<net name="MISO">
<segment>
<pinref part="U1" gate="A" pin="PB4"/>
</segment>
<segment>
<pinref part="JP3" gate="A" pin="8"/>
</segment>
</net>
<net name="SCK">
<segment>
<pinref part="U1" gate="A" pin="PB5"/>
</segment>
<segment>
<pinref part="R3" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="JP3" gate="A" pin="9"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="U1" gate="A" pin="GND_2"/>
<pinref part="U1" gate="A" pin="GND_3"/>
<pinref part="U1" gate="A" pin="GND"/>
<pinref part="GND2" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="S1" gate="2" pin="S1"/>
</segment>
<segment>
<pinref part="GND4" gate="1" pin="GND"/>
<pinref part="C2" gate="&gt;NAME" pin="1"/>
<pinref part="C1" gate="&gt;NAME" pin="1"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="C"/>
<pinref part="GND3" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C4" gate="&gt;NAME" pin="1"/>
<pinref part="GND5" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="VCC/GND" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="VCC/GND" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND" gate="1" pin="P"/>
</segment>
<segment>
<pinref part="R4" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="CRYSTAL" gate="P" pin="2"/>
<pinref part="U1" gate="A" pin="PB6"/>
<pinref part="C2" gate="&gt;NAME" pin="2"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="U1" gate="A" pin="PB7"/>
<pinref part="CRYSTAL" gate="P" pin="1"/>
<pinref part="C1" gate="&gt;NAME" pin="2"/>
</segment>
</net>
<net name="PC0">
<segment>
<pinref part="U1" gate="A" pin="PC0"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="2"/>
</segment>
</net>
<net name="PC1">
<segment>
<pinref part="U1" gate="A" pin="PC1"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="3"/>
</segment>
</net>
<net name="PC2">
<segment>
<pinref part="U1" gate="A" pin="PC2"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="4"/>
</segment>
</net>
<net name="PC3">
<segment>
<pinref part="U1" gate="A" pin="PC3"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="5"/>
</segment>
</net>
<net name="PC4">
<segment>
<pinref part="U1" gate="A" pin="PC4"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="6"/>
</segment>
</net>
<net name="PC5">
<segment>
<pinref part="U1" gate="A" pin="PC5"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="7"/>
</segment>
</net>
<net name="RST">
<segment>
<pinref part="U1" gate="A" pin="PC6"/>
<pinref part="C3" gate="&gt;NAME" pin="1"/>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="S1" gate="2" pin="P1"/>
</segment>
<segment>
<pinref part="EXTRAPINHEADER" gate="G$1" pin="RTS"/>
</segment>
</net>
<net name="RX">
<segment>
<pinref part="U1" gate="A" pin="PD0"/>
</segment>
<segment>
<pinref part="FTDI" gate="G$1" pin="RXD"/>
</segment>
<segment>
<pinref part="EXTRAPINHEADER" gate="G$1" pin="GND"/>
</segment>
</net>
<net name="TX">
<segment>
<pinref part="U1" gate="A" pin="PD1"/>
</segment>
<segment>
<pinref part="FTDI" gate="G$1" pin="TXD"/>
</segment>
<segment>
<pinref part="EXTRAPINHEADER" gate="G$1" pin="CTS"/>
</segment>
</net>
<net name="PD2">
<segment>
<pinref part="U1" gate="A" pin="PD2"/>
</segment>
<segment>
<pinref part="EXTRAPINHEADER" gate="G$1" pin="VCC"/>
</segment>
</net>
<net name="PD3">
<segment>
<pinref part="U1" gate="A" pin="PD3"/>
</segment>
<segment>
<pinref part="EXTRAPINHEADER" gate="G$1" pin="TXD"/>
</segment>
</net>
<net name="PD4">
<segment>
<pinref part="U1" gate="A" pin="PD4"/>
</segment>
<segment>
<pinref part="EXTRAPINHEADER" gate="G$1" pin="RXD"/>
</segment>
</net>
<net name="PD5">
<segment>
<pinref part="U1" gate="A" pin="PD5"/>
</segment>
<segment>
<pinref part="JP3" gate="A" pin="1"/>
</segment>
</net>
<net name="PD6">
<segment>
<pinref part="U1" gate="A" pin="PD6"/>
</segment>
<segment>
<pinref part="JP3" gate="A" pin="2"/>
</segment>
</net>
<net name="PD7">
<segment>
<pinref part="U1" gate="A" pin="PD7"/>
</segment>
<segment>
<pinref part="JP3" gate="A" pin="3"/>
</segment>
</net>
<net name="RTS">
<segment>
<pinref part="C3" gate="&gt;NAME" pin="2"/>
</segment>
<segment>
<pinref part="FTDI" gate="G$1" pin="RTS"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="U$2" gate="G$1" pin="A"/>
<pinref part="R3" gate="G$1" pin="2"/>
</segment>
</net>
<net name="CTS">
<segment>
<pinref part="FTDI" gate="G$1" pin="CTS"/>
</segment>
</net>
<net name="VCC-JUMPER">
<segment>
<pinref part="R1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="FTDI" gate="G$1" pin="VCC"/>
</segment>
</net>
<net name="GND-JUMPER">
<segment>
<pinref part="R4" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="FTDI" gate="G$1" pin="GND"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
