<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<schematic>
<libraries>
<library name="RepRapjr">
<packages>
<package name="A4988BREAKOUT">
</package>
</packages>
<symbols>
<symbol name="A4988BREAKOUT">
<pin name="EN" direction="in"/>
<pin name="MS1" direction="in"/>
<pin name="MS2" direction="in"/>
<pin name="MS3" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="SLEEP" direction="in"/>
<pin name="STEP" direction="in"/>
<pin name="DIR" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="1B" direction="out"/>
<pin name="1A" direction="out"/>
<pin name="2A" direction="out"/>
<pin name="2B" direction="out"/>
<pin name="GND@0" direction="pwr"/>
<pin name="VMOT" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="A4988BREAKOUT">
<gates>
<gate name="G$1" symbol="A4988BREAKOUT"/>
</gates>
<devices>
<device name="" package="A4988BREAKOUT">
<connects>
<connect gate="G$1" pin="1A" pad="1A"/>
<connect gate="G$1" pin="1B" pad="1B"/>
<connect gate="G$1" pin="2A" pad="2A"/>
<connect gate="G$1" pin="2B" pad="2B"/>
<connect gate="G$1" pin="DIR" pad="DIR"/>
<connect gate="G$1" pin="EN" pad="EN"/>
<connect gate="G$1" pin="GND@0" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@0"/>
<connect gate="G$1" pin="MS1" pad="MS1"/>
<connect gate="G$1" pin="MS2" pad="MS2"/>
<connect gate="G$1" pin="MS3" pad="MS3"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="SLEEP" pad="SLP"/>
<connect gate="G$1" pin="STEP" pad="STEP"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
<connect gate="G$1" pin="VMOT" pad="VMOT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="adafruit">
<packages>
<package name="CT3216">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip
tantalum</description>
</package>
<package name="CT3528">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip
tantalum</description>
</package>
<package name="CT6032">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip
tantalum</description>
</package>
<package name="CT7343">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip
tantalum</description>
</package>
<package name="B45181A">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 5 x 5 mm, rectangle, grid 2.54 mm</description>
</package>
<package name="B45181B">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 7.6 x 5 mm, rectangle, grid 5.08 mm</description>
</package>
<package name="B45181C">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 12.7 x 7.6 mm, rectangle, grid 10.16 mm</description>
</package>
<package name="B45181D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 12.5 x 12.5 mm, rectangle, grid 10.16 mm</description>
</package>
<package name="TT2D4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4 mm, grid 2.54 mm</description>
</package>
<package name="TT2D4L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4 mm, grid 2.54 mm</description>
</package>
<package name="TT2D5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5 mm, grid 2.54 mm</description>
</package>
<package name="TT2D6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 2.54 mm</description>
</package>
<package name="TT2D6L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 2.54 mm</description>
</package>
<package name="TT2D7L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 2.54 mm</description>
</package>
<package name="TT2D7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 2.54 mm</description>
</package>
<package name="TT5D10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 10 mm, grid 5.08 mm</description>
</package>
<package name="TT5D11">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 11 mm, grid 5.08 mm</description>
</package>
<package name="TT5D11L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 11 mm, grid 5.08 mm</description>
</package>
<package name="TT5D6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 5.08 mm</description>
</package>
<package name="TT5D6L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 5.08 mm</description>
</package>
<package name="TT5D7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 5.08 mm</description>
</package>
<package name="TT5D7L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 5.08 mm</description>
</package>
<package name="TT5D9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 9 mm, grid 5.08 mm</description>
</package>
<package name="TT5D9L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 9 mm, grid 5.08 mm</description>
</package>
<package name="ETR1">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 2.54 mm</description>
</package>
<package name="ETR2">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 5.08 mm</description>
</package>
<package name="ETR3">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 5.08 mm</description>
</package>
<package name="ETR4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 10.16 mm</description>
</package>
<package name="ETR5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 10.16 mm</description>
</package>
<package name="P128-35">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-40">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-50">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-60">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="TAP5-45">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4.5 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-50">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-70">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-60">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-80">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 8.0 mm, grid 5.08 mm</description>
</package>
<package name="085CS_1R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1AR">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1AW">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-2R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-2W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-3R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-3W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0405">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0505">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0605">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0807">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1012">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="175TMP-0808">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
High Temperature solid electrolytic SMD 175 TMP&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="175TMP-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
High Temperature solid electrolytic SMD 175 TMP&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="A/3216-18R">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="A/3216-18W">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="B/3528-21R">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET T / EIA 3528-12</description>
</package>
<package name="B/3528-21W">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET T / EIA 3528-12</description>
</package>
<package name="C/6032-28R">
<description>&lt;b&gt;Chip Capacitor Type KEMET C / EIA 6032-28 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET U / EIA 6032-15</description>
</package>
<package name="C/6032-28W">
<description>&lt;b&gt;Chip Capacitor Type KEMET C / EIA 6032-28 Wafe solder&lt;/b&gt;&lt;p&gt;
KEMET U / EIA 6032-15</description>
</package>
<package name="D/7343-31R">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21&lt;/b&gt;&lt;p&gt;
KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 Reflow solder</description>
</package>
<package name="D/7343-31W">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21&lt;/b&gt;&lt;p&gt;
KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 Wafe solder</description>
</package>
<package name="E/7260-38R">
<description>&lt;b&gt;Chip Capacitor Type KEMET E / EIA 7260-38 Reflow solder&lt;/b&gt;</description>
</package>
<package name="E/7260-38W">
<description>&lt;b&gt;Chip Capacitor Type KEMET E / EIA 7260-38 Wafe solder&lt;/b&gt;</description>
</package>
<package name="R/2012-12R">
<description>&lt;b&gt;Chip Capacitor Type KEMET R/EIA 2012-12 Reflow solder&lt;/b&gt;</description>
</package>
<package name="R/2012-12W">
<description>&lt;b&gt;Chip Capacitor Type KEMET R/EIA 2012-12 Wafe solder&lt;/b&gt;</description>
</package>
<package name="PANASONIC_A">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package A&lt;/b&gt;</description>
</package>
<package name="PANASONIC_B">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B&lt;/b&gt;</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C&lt;/b&gt;</description>
</package>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="PANASONIC_F">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package F&lt;/b&gt;</description>
</package>
<package name="PANASONIC_G">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package G&lt;/b&gt;</description>
</package>
<package name="E1,8-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 1.8 mm, diameter 4 mm</description>
</package>
<package name="EB20D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 20 mm</description>
</package>
<package name="EB22,5D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 22.5 mm</description>
</package>
<package name="EB25D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 25 mm</description>
</package>
<package name="EB30D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 30 mm</description>
</package>
<package name="EB35D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 35 mm</description>
</package>
<package name="E15-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 5 mm</description>
</package>
<package name="E15-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 6 mm</description>
</package>
<package name="E15-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 9 mm</description>
</package>
<package name="E2,5-6E">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="E2-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2 mm, diameter 4 mm</description>
</package>
<package name="E2-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.032 mm, diameter 5 mm</description>
</package>
<package name="E2,5RE">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 4 mm,</description>
</package>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="E2,5-4R">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 4 mm</description>
</package>
<package name="E2,5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="E2,5-7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 7 mm</description>
</package>
<package name="E22-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 10 mm</description>
</package>
<package name="E22-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 6 mm</description>
</package>
<package name="E22-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 9 mm</description>
</package>
<package name="E25-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 25.4 mm, diameter 10 mm</description>
</package>
<package name="E25-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 25.4 mm, diameter 9 mm</description>
</package>
<package name="E3,5-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 10 mm</description>
</package>
<package name="E3,5-8">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 8 mm</description>
</package>
<package name="E30-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 10 mm</description>
</package>
<package name="E30-12">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 12 mm</description>
</package>
<package name="E30-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 16 mm</description>
</package>
<package name="E35-12">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 35.56 mm, diameter 12 mm</description>
</package>
<package name="E35-14">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 14 mm</description>
</package>
<package name="E35-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 16 mm</description>
</package>
<package name="E35-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 18 mm</description>
</package>
<package name="E45-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 16 mm</description>
</package>
<package name="E45-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 18 mm</description>
</package>
<package name="E45-21">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 21 mm</description>
</package>
<package name="E45-22">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 22 mm</description>
</package>
<package name="E45-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 25 mm</description>
</package>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
<package name="E5-13">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 13 mm</description>
</package>
<package name="E5-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.05 mm, diameter 4 mm</description>
</package>
<package name="E5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 5 mm</description>
</package>
<package name="E5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 6 mm</description>
</package>
<package name="E5-8,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 8.5 mm</description>
</package>
<package name="E5R">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 9 mm</description>
</package>
<package name="E50-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 50 mm, diameter 25 mm</description>
</package>
<package name="E50-30">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 50 mm, diameter 30 mm</description>
</package>
<package name="E55-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 55 mm, diameter 25 mm</description>
</package>
<package name="E55-30">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 55 mm, diameter 30 mm</description>
</package>
<package name="E7,5-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.62 mm, diameter 16 mm</description>
</package>
<package name="E7,5-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.62 mm, diameter 18 mm</description>
</package>
<package name="TT2D5L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5 mm, grid 2.54 mm</description>
</package>
</packages>
<symbols>
<symbol name="CPOL-US">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CPOL-US" prefix="C" uservalue="yes">
<description>&lt;B&gt;POLARIZED CAPACITOR&lt;/B&gt;, American symbol</description>
<gates>
<gate name="G$1" symbol="CPOL-US"/>
</gates>
<devices>
<device name="CT3216" package="CT3216">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT3528" package="CT3528">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT6032" package="CT6032">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT7343" package="CT7343">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181A" package="B45181A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181B" package="B45181B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181C" package="B45181C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181D" package="B45181D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D4" package="TT2D4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D4L" package="TT2D4L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D5" package="TT2D5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D6" package="TT2D6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D6L" package="TT2D6L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D7L" package="TT2D7L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D7" package="TT2D7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D10" package="TT5D10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D11" package="TT5D11">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D11L" package="TT5D11L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT6D6" package="TT5D6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D6L" package="TT5D6L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D7" package="TT5D7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D7L" package="TT5D7L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D9" package="TT5D9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D9L" package="TT5D9L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR1" package="ETR1">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR2" package="ETR2">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR3" package="ETR3">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR4" package="ETR4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR5" package="ETR5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-35" package="P128-35">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-40" package="P128-40">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-50" package="P128-50">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-60" package="P128-60">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-45" package="TAP5-45">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-50" package="TAP5-50">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-70" package="TAP5-70">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-60" package="TAP5-60">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-80" package="TAP5-80">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1R" package="085CS_1R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1W" package="085CS_1W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1AR" package="085CS_1AR">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1AW" package="085CS_1AW">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-2R" package="139CLL-2R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-2W" package="139CLL-2W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-3R" package="139CLL-3R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-3W" package="139CLL-3W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="140CLH-0810" package="140CLH-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="140CLH-1010" package="140CLH-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="140CLH-1014" package="140CLH-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150CLZ-0810" package="150CLZ-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150CLZ-1010" package="150CLZ-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150CLZ-1014" package="150CLZ-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0405" package="153CLV-0405">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0505" package="153CLV-0505">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0605" package="153CLV-0605">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0807" package="153CLV-0807">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0810" package="153CLV-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-1010" package="153CLV-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-1012" package="153CLV-1012">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-1014" package="153CLV-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="175TMP-0808" package="175TMP-0808">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="175TMP-0810" package="175TMP-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A/3216-18R" package="A/3216-18R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A/3216-18W" package="A/3216-18W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B/3528-21R" package="B/3528-21R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B/3528-21W" package="B/3528-21W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C/6032-28R" package="C/6032-28R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C/6032-28W" package="C/6032-28W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D/7343-31R" package="D/7343-31R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D/7343-31W" package="D/7343-31W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E/7260-38R" package="E/7260-38R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E/7260-38W" package="E/7260-38W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R/2012-12R" package="R/2012-12R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R/2012-12W" package="R/2012-12W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A" package="PANASONIC_A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B" package="PANASONIC_B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C" package="PANASONIC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="PANASONIC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E" package="PANASONIC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="F" package="PANASONIC_F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="G" package="PANASONIC_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E1.8-4" package="E1,8-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-20" package="EB20D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-22.5" package="EB22,5D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-25" package="EB25D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-30" package="EB30D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-35" package="EB35D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E15-5AXIAL" package="E15-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E15-6AXIAL" package="E15-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E15-9AXIAL" package="E15-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2,5-6E" package="E2,5-6E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2-4" package="E2-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2-5" package="E2-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-4V" package="E2,5RE">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-5" package="E2,5-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-5V" package="E2,5-4R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-6" package="E2,5-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-7" package="E2,5-7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E22-10AXIAL" package="E22-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E22-6AXIAL" package="E22-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E22-9AXIAL" package="E22-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E25-10AXIAL" package="E25-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E25-9AXIAL" package="E25-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E3.5-10" package="E3,5-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E3.5-8" package="E3,5-8">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E30-10AXIAL" package="E30-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E30-12AXIAL" package="E30-12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E30-16AXIAL" package="E30-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-12AXIAL" package="E35-12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-14AXIAL" package="E35-14">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-16AXIAL" package="E35-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-18AXIAL" package="E35-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-16AXIAL" package="E45-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-18AXIAL" package="E45-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-21AXIAL" package="E45-21">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-22AXIAL" package="E45-22">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-25AXIAL" package="E45-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-10.5" package="E5-10,5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-13" package="E5-13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-4" package="E5-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-5" package="E5-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-6" package="E5-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-8.5" package="E5-8,5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-9VAXIAL" package="E5R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E50-25AXIAL" package="E50-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E50-30AXIAL" package="E50-30">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E55-25AXIAL" package="E55-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E55-30AXIAL" package="E55-30">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E7.5-16" package="E7,5-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E7.5-18" package="E7,5-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D5L" package="TT2D5L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PINHD4">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X4" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD4"/>
</gates>
<devices>
<device name="" package="1X04">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X04/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Seeed-OPL-Connector">
<packages>
<package name="DCJ3P-14.2X11.0X9.0MM">
</package>
</packages>
<symbols>
<symbol name="POWER-JACK-DC">
<pin name="+"/>
<pin name="-"/>
<pin name="CDN"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CONN-POWER-JACK-2.1MM(DC-005)" prefix="J" uservalue="yes">
<description>320120003</description>
<gates>
<gate name="JACK" symbol="POWER-JACK-DC"/>
</gates>
<devices>
<device name="" package="DCJ3P-14.2X11.0X9.0MM">
<connects>
<connect gate="JACK" pin="+" pad="+"/>
<connect gate="JACK" pin="-" pad="-1"/>
<connect gate="JACK" pin="CDN" pad="-2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DC-005"/>
<attribute name="VALUE" value="DC-005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="fab">
<packages>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206FAB">
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="LED">
<description>LED</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="CAP-NONPOLARIZED">
<description>non-polarized capacitor</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="TS2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LED">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB1206" package="LED1206FAB">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-UNPOLARIZED" prefix="C" uservalue="yes">
<gates>
<gate name="&gt;NAME" symbol="CAP-NONPOLARIZED"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB" package="C1206FAB">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6MM_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
<gates>
<gate name="2" symbol="TS2"/>
</gates>
<devices>
<device name="6MM_SWITCH" package="6MM_SWITCH">
<connects>
<connect gate="2" pin="P" pad="1"/>
<connect gate="2" pin="P1" pad="2"/>
<connect gate="2" pin="S" pad="3"/>
<connect gate="2" pin="S1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCC" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="VCC" symbol="VCC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
<symbols>
<symbol name="ATMEGAXX8-32PIN_NOPAD">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATMEGA328P_TQFP" prefix="U">
<description>&lt;h3&gt;Popular 328P in QFP&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/13448"&gt;Storefront component: ATmega328 - TQFP&lt;/a&gt; (COM-13448)&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/SMD/ATMega328.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12757"&gt;SparkFun RedBoard - Programmed with Arduino&lt;/a&gt; (DEV-12757)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11113"&gt;Arduino Pro Mini 328 - 5V/16MHz&lt;/a&gt; (DEV-11113)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11114"&gt;Arduino Pro Mini 328 - 3.3V/8MHz&lt;/a&gt; (DEV-11114)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13712"&gt;SparkFun OpenLog&lt;/a&gt; (DEV-13712)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12923"&gt;SparkFun MicroView - OLED Arduino Module&lt;/a&gt; (DEV-12923)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12651"&gt;SparkFun Digital Sandbox&lt;/a&gt; (DEV-12651)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11888"&gt;SparkFun PicoBoard&lt;/a&gt; (WIG-11888)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10116"&gt;Arduino Fio&lt;/a&gt; (DEV-10116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13342"&gt;LilyPad Arduino 328 Main Board&lt;/a&gt; (DEV-13342)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13741"&gt;SparkFun RedStick&lt;/a&gt; (DEV-13741)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11013"&gt;LilyPad MP3&lt;/a&gt; (DEV-11013)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10941"&gt;LilyPad Arduino SimpleSnap&lt;/a&gt; (DEV-10941)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13899"&gt;SparkFun Stepoko&lt;/a&gt; (ROB-13899)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11345"&gt;SparkFun Geiger Counter&lt;/a&gt; (SEN-11345)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12781"&gt;SparkFun EL Sequencer&lt;/a&gt; (COM-12781)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10915"&gt;Arduino Pro 328 - 5V/16MHz&lt;/a&gt; (DEV-10915)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12773"&gt;CryptoCape&lt;/a&gt; (DEV-12773)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10740"&gt;SparkFun IR Thermometer Evaluation Board - MLX90614&lt;/a&gt; (SEN-10740)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12097"&gt;SparkFun RedBot Mainboard&lt;/a&gt; (ROB-12097)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10914"&gt;Arduino Pro 328 - 3.3V/8MHz&lt;/a&gt; (DEV-10914)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13036"&gt;SparkFun Block for Intel® Edison - Arduino&lt;/a&gt; (DEV-13036)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10935"&gt;SparkFun Simon Says - Surface Mount Soldering Kit&lt;/a&gt; (KIT-10935)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11441"&gt;SparkFun 7-Segment Serial Display - Red&lt;/a&gt; (COM-11441)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11629"&gt;SparkFun 7-Segment Serial Display - White&lt;/a&gt; (COM-11629)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11443"&gt;SparkFun 7-Segment Serial Display - Yellow&lt;/a&gt; (COM-11443)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11440"&gt;SparkFun 7-Segment Serial Display - Kelly Green&lt;/a&gt; (COM-11440)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11442"&gt;SparkFun 7-Segment Serial Display - Blue&lt;/a&gt; (COM-11442)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11647"&gt;SparkFun OpenSegment Serial Display - 20mm (Blue)&lt;/a&gt; (COM-11647)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11646"&gt;SparkFun OpenSegment Serial Display - 20mm (Green)&lt;/a&gt; (COM-11646)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11648"&gt;SparkFun OpenSegment Serial Display - 20mm (White)&lt;/a&gt; (COM-11648)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11644"&gt;SparkFun OpenSegment Serial Display - 20mm (Red)&lt;/a&gt; (COM-11644)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11645"&gt;SparkFun OpenSegment Serial Display - 20mm (Yellow)&lt;/a&gt; (COM-11645)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13190"&gt;SparkFun OpenSegment Shield&lt;/a&gt; (DEV-13190)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="U1" symbol="ATMEGAXX8-32PIN_NOPAD"/>
</gates>
<devices>
<device name="" package="TQFP32-08">
<connects>
<connect gate="U1" pin="ADC6" pad="19"/>
<connect gate="U1" pin="ADC7" pad="22"/>
<connect gate="U1" pin="AGND" pad="21"/>
<connect gate="U1" pin="AREF" pad="20"/>
<connect gate="U1" pin="AVCC" pad="18"/>
<connect gate="U1" pin="GND" pad="3 5"/>
<connect gate="U1" pin="PB0(ICP)" pad="12"/>
<connect gate="U1" pin="PB1(OC1A)" pad="13"/>
<connect gate="U1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="U1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="U1" pin="PB4(MISO)" pad="16"/>
<connect gate="U1" pin="PB5(SCK)" pad="17"/>
<connect gate="U1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="U1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="U1" pin="PC0(ADC0)" pad="23"/>
<connect gate="U1" pin="PC1(ADC1)" pad="24"/>
<connect gate="U1" pin="PC2(ADC2)" pad="25"/>
<connect gate="U1" pin="PC3(ADC3)" pad="26"/>
<connect gate="U1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="U1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="U1" pin="PC6(/RESET)" pad="29"/>
<connect gate="U1" pin="PD0(RXD)" pad="30"/>
<connect gate="U1" pin="PD1(TXD)" pad="31"/>
<connect gate="U1" pin="PD2(INT0)" pad="32"/>
<connect gate="U1" pin="PD3(INT1)" pad="1"/>
<connect gate="U1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="U1" pin="PD5(T1)" pad="9"/>
<connect gate="U1" pin="PD6(AIN0)" pad="10"/>
<connect gate="U1" pin="PD7(AIN1)" pad="11"/>
<connect gate="U1" pin="VCC" pad="4 6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09069"/>
<attribute name="VALUE" value="ATMEGA328P_TQFP"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CSM-7X-DU">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;&lt;p&gt;
Source: www.ecsxtal.com .. Crystal 3.6864MHz CSM_7X_DU.PDF</description>
</package>
</packages>
<symbols>
<symbol name="Q">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CSM-7X-DU" prefix="Q">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;&lt;p&gt;
Source: www.ecsxtal.com .. Crystal 3.6864MHz CSM_7X_DU.PDF</description>
<gates>
<gate name="P" symbol="Q"/>
</gates>
<devices>
<device name="" package="CSM-7X-DU">
<connects>
<connect gate="P" pin="1" pad="1"/>
<connect gate="P" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X07/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PINHD6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD7">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD1">
<pin name="1" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD6"/>
</gates>
<devices>
<device name="" package="1X06">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X06/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X7" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD7"/>
</gates>
<devices>
<device name="" package="1X07">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X07/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD2"/>
</gates>
<devices>
<device name="" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X02/90">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="1X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X03/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X1" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD1"/>
</gates>
<devices>
<device name="" package="1X01">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="tango">
<packages>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="78XX">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="L7805" prefix="IC" uservalue="yes">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="78XX"/>
</gates>
<devices>
<device name="" package="78XXL">
<connects>
<connect gate="A" pin="GND" pad="GND"/>
<connect gate="A" pin="IN" pad="IN"/>
<connect gate="A" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJW">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="SJ">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SJ" prefix="SJ" uservalue="yes">
<description>SMD solder &lt;b&gt;JUMPER&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="SJ"/>
</gates>
<devices>
<device name="" package="SJ">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W" package="SJW">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="U$1" library="RepRapjr" deviceset="A4988BREAKOUT" device=""/>
<part name="C1" library="adafruit" deviceset="CPOL-US" device="E2,5-6E"/>
<part name="J1" library="Seeed-OPL-Connector" deviceset="CONN-POWER-JACK-2.1MM(DC-005)" device="" value="DC-005"/>
<part name="JP5" library="pinhead" deviceset="PINHD-1X4" device=""/>
<part name="GREELED" library="fab" deviceset="LED" device="FAB1206" value="POWER"/>
<part name="U2" library="SparkFun-IC-Microcontroller" deviceset="ATMEGA328P_TQFP" device="" value="ATMEGA328P_TQFP"/>
<part name="S1" library="fab" deviceset="6MM_SWITCH" device="6MM_SWITCH"/>
<part name="GND2" library="supply1" deviceset="GND" device=""/>
<part name="R2" library="fab" deviceset="RES-US" device="1206FAB" value="10k"/>
<part name="P+1" library="supply1" deviceset="VCC" device=""/>
<part name="C2" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="22pF"/>
<part name="C3" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="22pF"/>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
<part name="GND3" library="supply1" deviceset="GND" device=""/>
<part name="R3" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="GND6" library="supply1" deviceset="GND" device=""/>
<part name="P+3" library="supply1" deviceset="VCC" device=""/>
<part name="C5" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="10uP"/>
<part name="GND7" library="supply1" deviceset="GND" device=""/>
<part name="P+4" library="supply1" deviceset="VCC" device=""/>
<part name="C6" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="100uF"/>
<part name="Q1" library="crystal" deviceset="CSM-7X-DU" device="" value="16MHz Clock"/>
<part name="P+5" library="supply1" deviceset="VCC" device=""/>
<part name="P+6" library="supply1" deviceset="VCC" device=""/>
<part name="P+7" library="supply1" deviceset="VCC" device=""/>
<part name="GND8" library="supply1" deviceset="GND" device=""/>
<part name="GND9" library="supply1" deviceset="GND" device=""/>
<part name="JP2" library="pinhead" deviceset="PINHD-1X6" device=""/>
<part name="P+8" library="supply1" deviceset="VCC" device=""/>
<part name="GND10" library="supply1" deviceset="GND" device=""/>
<part name="JP6" library="pinhead" deviceset="PINHD-1X7" device=""/>
<part name="12VTOLED" library="tango" deviceset="L7805" device=""/>
<part name="12VTOSIYUNO" library="tango" deviceset="L7805" device=""/>
<part name="GND5" library="supply1" deviceset="GND" device=""/>
<part name="GND11" library="supply1" deviceset="GND" device=""/>
<part name="GND12" library="supply1" deviceset="GND" device=""/>
<part name="P+10" library="supply1" deviceset="VCC" device=""/>
<part name="GND14" library="supply1" deviceset="GND" device=""/>
<part name="P+12" library="supply1" deviceset="VCC" device=""/>
<part name="JP3" library="pinhead" deviceset="PINHD-1X2" device=""/>
<part name="P+13" library="supply1" deviceset="VCC" device=""/>
<part name="GND16" library="supply1" deviceset="GND" device=""/>
<part name="LED+-" library="pinhead" deviceset="PINHD-1X2" device=""/>
<part name="SWITCH12V" library="pinhead" deviceset="PINHD-1X2" device=""/>
<part name="JP7" library="pinhead" deviceset="PINHD-1X6" device=""/>
<part name="JP1" library="pinhead" deviceset="PINHD-1X2" device=""/>
<part name="JP8" library="pinhead" deviceset="PINHD-1X3" device=""/>
<part name="JP4" library="pinhead" deviceset="PINHD-1X1" device="" value="FTDIRESET"/>
<part name="JP9" library="pinhead" deviceset="PINHD-1X2" device="" value="FTDIVCCGND"/>
<part name="SJ1" library="jumper" deviceset="SJ" device=""/>
<part name="SJ2" library="jumper" deviceset="SJ" device=""/>
<part name="SJ3" library="jumper" deviceset="SJ" device=""/>
<part name="SJ4" library="jumper" deviceset="SJ" device=""/>
<part name="SWITCHSTEPPER" library="pinhead" deviceset="PINHD-1X2" device=""/>
<part name="SWITCHLED" library="pinhead" deviceset="PINHD-1X2" device=""/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="VIN">
<segment>
<pinref part="12VTOSIYUNO" gate="A" pin="IN"/>
</segment>
<segment>
<pinref part="12VTOLED" gate="A" pin="IN"/>
</segment>
<segment>
<pinref part="SWITCHSTEPPER" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SWITCH12V" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="J1" gate="JACK" pin="+"/>
</segment>
<segment>
<pinref part="SWITCHLED" gate="G$1" pin="1"/>
</segment>
</net>
<net name="DIR">
<segment>
<pinref part="U$1" gate="G$1" pin="DIR"/>
</segment>
<segment>
<pinref part="U2" gate="U1" pin="PB0(ICP)"/>
</segment>
<segment>
<pinref part="JP7" gate="A" pin="4"/>
</segment>
</net>
<net name="STEP">
<segment>
<pinref part="U$1" gate="G$1" pin="STEP"/>
</segment>
<segment>
<pinref part="U2" gate="U1" pin="PB1(OC1A)"/>
</segment>
<segment>
<pinref part="JP7" gate="A" pin="5"/>
</segment>
</net>
<net name="N$7">
<segment>
<pinref part="U$1" gate="G$1" pin="SLEEP"/>
<pinref part="U$1" gate="G$1" pin="RST"/>
</segment>
</net>
<net name="N$34">
<segment>
<pinref part="U$1" gate="G$1" pin="2B"/>
<pinref part="JP5" gate="A" pin="1"/>
</segment>
</net>
<net name="N$35">
<segment>
<pinref part="U$1" gate="G$1" pin="2A"/>
<pinref part="JP5" gate="A" pin="2"/>
</segment>
</net>
<net name="N$36">
<segment>
<pinref part="U$1" gate="G$1" pin="1A"/>
<pinref part="JP5" gate="A" pin="3"/>
</segment>
</net>
<net name="N$37">
<segment>
<pinref part="U$1" gate="G$1" pin="1B"/>
<pinref part="JP5" gate="A" pin="4"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="S1" gate="2" pin="S"/>
<pinref part="S1" gate="2" pin="S1"/>
<pinref part="GND2" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C2" gate="&gt;NAME" pin="2"/>
<pinref part="GND1" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C3" gate="&gt;NAME" pin="2"/>
<pinref part="GND3" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND6" gate="1" pin="GND"/>
<pinref part="R3" gate="G$1" pin="1"/>
<pinref part="JP9" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="C5" gate="&gt;NAME" pin="2"/>
<pinref part="GND7" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="U2" gate="U1" pin="AGND"/>
<pinref part="GND8" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="U2" gate="U1" pin="GND"/>
<pinref part="GND9" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="2"/>
<pinref part="GND10" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="J1" gate="JACK" pin="-"/>
<pinref part="J1" gate="JACK" pin="CDN"/>
<pinref part="GND5" gate="1" pin="GND"/>
<pinref part="C1" gate="G$1" pin="-"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="GND@0"/>
<pinref part="GND11" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="GND@1"/>
<pinref part="GND12" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="12VTOSIYUNO" gate="A" pin="GND"/>
<pinref part="GND14" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="JP3" gate="G$1" pin="2"/>
<pinref part="GND16" gate="1" pin="GND"/>
</segment>
</net>
<net name="VCC">
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="P+1" gate="VCC" pin="VCC"/>
</segment>
<segment>
<pinref part="P+3" gate="VCC" pin="VCC"/>
<pinref part="GREELED" gate="G$1" pin="A"/>
<pinref part="JP9" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C5" gate="&gt;NAME" pin="1"/>
<pinref part="P+4" gate="VCC" pin="VCC"/>
</segment>
<segment>
<pinref part="U2" gate="U1" pin="VCC"/>
<pinref part="P+5" gate="VCC" pin="VCC"/>
</segment>
<segment>
<pinref part="U2" gate="U1" pin="AVCC"/>
<pinref part="P+6" gate="VCC" pin="VCC"/>
</segment>
<segment>
<pinref part="U2" gate="U1" pin="AREF"/>
<pinref part="P+7" gate="VCC" pin="VCC"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="5"/>
<pinref part="P+8" gate="VCC" pin="VCC"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="VDD"/>
<pinref part="P+10" gate="VCC" pin="VCC"/>
</segment>
<segment>
<pinref part="12VTOSIYUNO" gate="A" pin="OUT"/>
<pinref part="P+12" gate="VCC" pin="VCC"/>
</segment>
<segment>
<pinref part="JP3" gate="G$1" pin="1"/>
<pinref part="P+13" gate="VCC" pin="VCC"/>
</segment>
</net>
<net name="XTAL1">
<segment>
<pinref part="U2" gate="U1" pin="PB6(XTAL1/TOSC1)"/>
<pinref part="C2" gate="&gt;NAME" pin="1"/>
<pinref part="Q1" gate="P" pin="2"/>
</segment>
</net>
<net name="XTAL2">
<segment>
<pinref part="U2" gate="U1" pin="PB7(XTAL2/TOSC2)"/>
<pinref part="C3" gate="&gt;NAME" pin="1"/>
<pinref part="Q1" gate="P" pin="1"/>
</segment>
</net>
<net name="N$38">
<segment>
<pinref part="GREELED" gate="G$1" pin="C"/>
<pinref part="R3" gate="G$1" pin="2"/>
</segment>
</net>
<net name="RST">
<segment>
<pinref part="U2" gate="U1" pin="PC6(/RESET)"/>
<pinref part="S1" gate="2" pin="P1"/>
<pinref part="S1" gate="2" pin="P"/>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="C6" gate="&gt;NAME" pin="1"/>
<pinref part="JP2" gate="A" pin="1"/>
</segment>
</net>
<net name="A0">
<segment>
<pinref part="U2" gate="U1" pin="PC0(ADC0)"/>
</segment>
<segment>
<pinref part="JP6" gate="A" pin="2"/>
</segment>
</net>
<net name="A1">
<segment>
<pinref part="U2" gate="U1" pin="PC1(ADC1)"/>
</segment>
<segment>
<pinref part="JP6" gate="A" pin="3"/>
</segment>
</net>
<net name="A2">
<segment>
<pinref part="U2" gate="U1" pin="PC2(ADC2)"/>
</segment>
<segment>
<pinref part="JP6" gate="A" pin="4"/>
</segment>
</net>
<net name="A3">
<segment>
<pinref part="U2" gate="U1" pin="PC3(ADC3)"/>
</segment>
<segment>
<pinref part="JP6" gate="A" pin="5"/>
</segment>
</net>
<net name="A4">
<segment>
<pinref part="U2" gate="U1" pin="PC4(ADC4/SDA)"/>
</segment>
<segment>
<pinref part="JP6" gate="A" pin="6"/>
</segment>
</net>
<net name="A5">
<segment>
<pinref part="U2" gate="U1" pin="PC5(ADC5/SCL)"/>
</segment>
<segment>
<pinref part="JP6" gate="A" pin="7"/>
</segment>
</net>
<net name="ADC6">
<segment>
<pinref part="U2" gate="U1" pin="ADC6"/>
</segment>
</net>
<net name="SCK13">
<segment>
<pinref part="U2" gate="U1" pin="PB5(SCK)"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="3"/>
</segment>
</net>
<net name="ADC7">
<segment>
<pinref part="U2" gate="U1" pin="ADC7"/>
</segment>
<segment>
<pinref part="JP6" gate="A" pin="1"/>
</segment>
</net>
<net name="RX">
<segment>
<pinref part="U2" gate="U1" pin="PD1(TXD)"/>
</segment>
<segment>
<pinref part="JP1" gate="G$1" pin="2"/>
</segment>
</net>
<net name="TX">
<segment>
<pinref part="U2" gate="U1" pin="PD0(RXD)"/>
</segment>
<segment>
<pinref part="JP1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="2">
<segment>
<pinref part="U2" gate="U1" pin="PD2(INT0)"/>
</segment>
<segment>
<pinref part="JP8" gate="A" pin="1"/>
</segment>
</net>
<net name="3">
<segment>
<pinref part="U2" gate="U1" pin="PD3(INT1)"/>
</segment>
<segment>
<pinref part="JP8" gate="A" pin="2"/>
</segment>
</net>
<net name="4">
<segment>
<pinref part="U2" gate="U1" pin="PD4(XCK/T0)"/>
</segment>
<segment>
<pinref part="JP8" gate="A" pin="3"/>
</segment>
</net>
<net name="5">
<segment>
<pinref part="U2" gate="U1" pin="PD5(T1)"/>
</segment>
<segment>
<pinref part="JP7" gate="A" pin="1"/>
</segment>
</net>
<net name="6">
<segment>
<pinref part="U2" gate="U1" pin="PD6(AIN0)"/>
</segment>
<segment>
<pinref part="JP7" gate="A" pin="2"/>
</segment>
</net>
<net name="7">
<segment>
<pinref part="U2" gate="U1" pin="PD7(AIN1)"/>
</segment>
<segment>
<pinref part="JP7" gate="A" pin="3"/>
</segment>
</net>
<net name="10">
<segment>
<pinref part="U2" gate="U1" pin="PB2(SS/OC1B)"/>
</segment>
<segment>
<pinref part="JP7" gate="A" pin="6"/>
</segment>
</net>
<net name="MISO12">
<segment>
<pinref part="U2" gate="U1" pin="PB4(MISO)"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="4"/>
</segment>
</net>
<net name="MOSI11">
<segment>
<pinref part="U2" gate="U1" pin="PB3(MOSI/OC2)"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="6"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="C6" gate="&gt;NAME" pin="2"/>
<pinref part="JP4" gate="G$1" pin="1"/>
</segment>
</net>
<net name="VLED">
<segment>
<pinref part="LED+-" gate="G$1" pin="1"/>
<pinref part="12VTOLED" gate="A" pin="OUT"/>
</segment>
<segment>
<pinref part="SWITCHLED" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="12VTOLED" gate="A" pin="GND"/>
<pinref part="LED+-" gate="G$1" pin="2"/>
</segment>
</net>
<net name="VMOT">
<segment>
<pinref part="C1" gate="G$1" pin="+"/>
<pinref part="SWITCH12V" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="VMOT"/>
</segment>
<segment>
<pinref part="SWITCHSTEPPER" gate="G$1" pin="2"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
