<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="14.478" y1="5.588" x2="66.98" y2="5.588" width="0" layer="20"/>
<wire x1="66.98" y1="5.588" x2="68.25" y2="71.872" width="0" layer="20"/>
<wire x1="68.25" y1="71.872" x2="15.494" y2="71.618" width="0" layer="20"/>
<wire x1="15.494" y1="71.618" x2="14.478" y2="5.588" width="0" layer="20"/>
<text>Graceplexing</text>
<polygon width="0.3048" layer="46">
<vertex x="33.528" y="67.818"/>
<vertex x="33.528" y="43.688"/>
<vertex x="18.796" y="43.688"/>
<vertex x="18.796" y="13.208"/>
<vertex x="24.13" y="7.874"/>
<vertex x="59.436" y="7.874"/>
<vertex x="64.262" y="12.7"/>
<vertex x="64.262" y="43.688"/>
<vertex x="57.658" y="43.688"/>
<vertex x="57.658" y="56.896"/>
<vertex x="50.546" y="56.896"/>
<vertex x="50.546" y="68.072"/>
<vertex x="50.292" y="67.818"/>
</polygon>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="2X03SMD">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' Retired foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are &lt;b&gt; no longer used&lt;/b&gt; in our catalog.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LIPO-110-TABS">
</package>
</packages>
</library>
<library name="_hhn_78xx_79xx_NCV78xx_d2pak_dpak">
<description>&lt;h2&gt;78xx 79xx NCV78xx SMD (D2PAK, DPAK)&lt;/h2&gt;
&lt;p&gt;&lt;b&gt;Linear Voltage Regulators&lt;/b&gt;&lt;/p&gt;
Source: ONSEMI (http://onsemi.com)&lt;br /&gt;
&lt;hr&gt;
&lt;p&gt;&lt;i&gt;Author: Dipl.-Ing. FH Rainer Bayer&lt;br /&gt;
HHN Hochschule Heilbronn, rainer.bayer@hs-heilbronn.de&lt;br /&gt;
Ingenieurbüro ing-rb, mail@ing-rb.de&lt;/p&gt;</description>
<packages>
<package name="DPAK-3">
<description>&lt;b&gt;DPAK-3&lt;/b&gt; (acc. to. ON Semiconductor specs)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="fab" package="SOIC14" value="ATTINY44-SSU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206FAB" value="row1 : 470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="fab" package="R1206FAB" value="row2 : 470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="fab" package="R1206FAB" value="row3 : 470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="fab" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fab" package="2X03SMD" value="AVRISPSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BT1" library="SparkFun-Retired" package="LIPO-110-TABS" value=""/>
<element name="U1" library="_hhn_78xx_79xx_NCV78xx_d2pak_dpak" package="DPAK-3" value="MC78GENERICDT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="12"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="11"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="10"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="LED1" pad="2"/>
<contactref element="LED2" pad="1"/>
<contactref element="LED6" pad="1"/>
<contactref element="LED5" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="LED1" pad="1"/>
<contactref element="LED3" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="LED2" pad="2"/>
<contactref element="LED4" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="LED3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="LED4" pad="2"/>
<contactref element="LED6" pad="2"/>
<contactref element="LED5" pad="1"/>
</signal>
<signal name="BUTTON">
<contactref element="IC1" pad="5"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="GND">
<contactref element="S1" pad="1"/>
<contactref element="U$1" pad="6"/>
<contactref element="IC1" pad="14"/>
<contactref element="BT1" pad="-"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="3"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="5"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="TX">
<contactref element="IC1" pad="13"/>
</signal>
<signal name="5V">
<contactref element="IC1" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="6V">
<contactref element="U1" pad="1"/>
<contactref element="BT1" pad="+"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
