<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.1">
<drawing>
<board>
<plain>
<wire x1="16.764" y1="56.896" x2="59.416" y2="56.388" width="0" layer="20"/>
<wire x1="59.416" y1="56.388" x2="58.908" y2="95.682" width="0" layer="20"/>
<wire x1="58.908" y1="95.682" x2="16.256" y2="96.19" width="0" layer="20"/>
<wire x1="16.256" y1="96.19" x2="16.764" y2="56.896" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
<package name="EFOBM">
</package>
</packages>
</library>
<library name="myFab">
<packages>
<package name="SOIC14_ATTTINY44">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="2X3PINHEADER">
</package>
</packages>
</library>
<library name="pinhead-1">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X06SMD/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 90°</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="FKIT-LED-1206">
<description>&lt;B&gt;LED 1206 SMT&lt;/B&gt;&lt;p&gt;
1206, surface mount
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Area: 0.125"x 0.06" &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="myFab" package="SOIC14_ATTTINY44" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="myFab" package="2X3PINHEADER" value=""/>
<element name="JP2" library="pinhead-1" package="1X06SMD/90" value="Pines">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R0" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fab" package="EFOBM" value="RESONATOR"/>
<element name="R1" library="fab" package="R1206FAB" value="10kohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PHOTO" library="SparkFun-Resistors" package="AXIAL-0.3" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-12184"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="FKIT-LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206FAB" value="300ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="R4">
<contactref element="R0" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="VCC"/>
<contactref element="JP2" pad="3"/>
<contactref element="PHOTO" pad="P$2"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="GND"/>
<contactref element="IC1" pad="14"/>
<contactref element="C1" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="13"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="9"/>
<contactref element="JP1" pad="SCK"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="7"/>
<contactref element="JP1" pad="MOSI"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="8"/>
<contactref element="JP1" pad="MISO"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="RST"/>
<contactref element="R0" pad="2"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="12"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="3"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="10"/>
<contactref element="PHOTO" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="D1" pad="A"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$10">
<contactref element="D1" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
