<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.1">
<drawing>
<schematic>
<libraries>
<library name="fab">
<packages>
<package name="EFOBM">
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206FAB">
</package>
</packages>
<symbols>
<symbol name="CERAMIC_RESONATOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CAP-NONPOLARIZED">
<description>non-polarized capacitor</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RESONATOR">
<gates>
<gate name="G$1" symbol="CERAMIC_RESONATOR"/>
</gates>
<devices>
<device name="" package="EFOBM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-UNPOLARIZED" prefix="C">
<gates>
<gate name="&gt;NAME" symbol="CAP-NONPOLARIZED"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB" package="C1206FAB">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="myFab">
<packages>
<package name="2X3PINHEADER">
</package>
<package name="SOIC14_ATTTINY44">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="2X3PINHEADER">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="ATTINY24/44/84">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PA7(ICP/OC0B/ADC7)"/>
<pin name="PA6(OC1A/SDA/MOSI/ADC6)"/>
<pin name="(OC1B/MISO/DO/ADC5)PA5"/>
<pin name="(T1/SCL/USCK/ADC4)PA4"/>
<pin name="(T0/ADC3)PA3"/>
<pin name="(AIN1/ADC2)PA2"/>
<pin name="(AIN0/ADC1)PA1"/>
<pin name="(AREF/ADC0)PA0"/>
<pin name="RESET"/>
<pin name="PB2(INT0/OC0A/CKOUT)"/>
<pin name="PB1(XTAL2)"/>
<pin name="PB0(XTAL1/CLKI)"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="2X3PINHEADER" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2X3PINHEADER"/>
</gates>
<devices>
<device name="" package="2X3PINHEADER">
<connects>
<connect gate="A" pin="1" pad="GND"/>
<connect gate="A" pin="2" pad="RST"/>
<connect gate="A" pin="3" pad="MOSI"/>
<connect gate="A" pin="4" pad="SCK"/>
<connect gate="A" pin="5" pad="VCC"/>
<connect gate="A" pin="6" pad="MISO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY44" prefix="IC" uservalue="yes">
<gates>
<gate name="1" symbol="ATTINY24/44/84"/>
</gates>
<devices>
<device name="-SSU" package="SOIC14_ATTTINY44">
<connects>
<connect gate="1" pin="(AIN0/ADC1)PA1" pad="12"/>
<connect gate="1" pin="(AIN1/ADC2)PA2" pad="11"/>
<connect gate="1" pin="(AREF/ADC0)PA0" pad="13"/>
<connect gate="1" pin="(OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="1" pin="(T0/ADC3)PA3" pad="10"/>
<connect gate="1" pin="(T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="1" pin="GND" pad="14"/>
<connect gate="1" pin="PA6(OC1A/SDA/MOSI/ADC6)" pad="7"/>
<connect gate="1" pin="PA7(ICP/OC0B/ADC7)" pad="6"/>
<connect gate="1" pin="PB0(XTAL1/CLKI)" pad="2"/>
<connect gate="1" pin="PB1(XTAL2)" pad="3"/>
<connect gate="1" pin="PB2(INT0/OC0A/CKOUT)" pad="5"/>
<connect gate="1" pin="RESET" pad="4"/>
<connect gate="1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND">
<gates>
<gate name="G$1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead-1">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="1X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 90°</description>
</package>
<package name="1X06M">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2</description>
</package>
<package name="1X06SMD">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 SMD</description>
</package>
<package name="1X06SMD/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 90°</description>
</package>
</packages>
<symbols>
<symbol name="PINHD6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD6"/>
</gates>
<devices>
<device name="_2.54" package="1X06">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.54-90°" package="1X06/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.00" package="1X06M">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.54-SMD" package="1X06SMD">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.54-SMD-90°" package="1X06SMD/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
<package name="AXIAL-0.1">
<description>&lt;h3&gt;AXIAL-0.1&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.1" pitch between holes.&lt;/p&gt;</description>
</package>
<package name="AXIAL-0.1-KIT">
<description>&lt;h3&gt;AXIAL-0.1-KIT&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.1" pitch between holes.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of the AXIAL-0.1 package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;</description>
</package>
<package name="AXIAL-0.3-KIT">
<description>&lt;h3&gt;AXIAL-0.3-KIT&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of the AXIAL-0.3 package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;</description>
</package>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0402">
<description>&lt;p&gt;&lt;b&gt;Generic 1005 (0402) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="RESISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="100KOHM" prefix="R">
<description>&lt;h3&gt;100kΩ resistor&lt;/h3&gt;
&lt;p&gt;A resistor is a passive two-terminal electrical component that implements electrical resistance as a circuit element. Resistors act to reduce current flow, and, at the same time, act to lower voltage levels within circuits. - Wikipedia&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="-HORIZ-1/4W-1%" package="AXIAL-0.3">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-12184"/>
<attribute name="VALUE" value="100k"/>
</technology>
</technologies>
</device>
<device name="-VERT-1/4W-1%" package="AXIAL-0.1">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-12184"/>
<attribute name="VALUE" value="100k"/>
</technology>
</technologies>
</device>
<device name="-VERT_KIT-1/4W-1%" package="AXIAL-0.1-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-12184"/>
<attribute name="VALUE" value="100k"/>
</technology>
</technologies>
</device>
<device name="-HORIZ_KIT-1/4W-1%" package="AXIAL-0.3-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-12184"/>
<attribute name="VALUE" value="100k"/>
</technology>
</technologies>
</device>
<device name="-VERT-1/4W-5%" package="AXIAL-0.1">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-10686"/>
<attribute name="VALUE" value="100k"/>
</technology>
</technologies>
</device>
<device name="-VERT_KIT-1/4W-5%" package="AXIAL-0.1-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-10686"/>
<attribute name="VALUE" value="100k"/>
</technology>
</technologies>
</device>
<device name="-HORIZ-1/4W-5%" package="AXIAL-0.3">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-10686"/>
<attribute name="VALUE" value="100k"/>
</technology>
</technologies>
</device>
<device name="-HORIZ_KIT-1/4W-5%" package="AXIAL-0.3-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-10686"/>
<attribute name="VALUE" value="100k"/>
</technology>
</technologies>
</device>
<device name="-0603-1/10W-1%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE" value="100k"/>
</technology>
</technologies>
</device>
<device name="-0402-1/16W-1%" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-13495"/>
<attribute name="VALUE" value="100K"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_5MM">
<description>&lt;B&gt;LED 5mm PTH&lt;/B&gt;&lt;p&gt;
5 mm, round
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED-IR-THRU&lt;/li&gt;</description>
</package>
<package name="LED_3MM">
<description>&lt;h3&gt;LED 3MM PTH&lt;/h3&gt;

3 mm, round.

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 3mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="LED-1206">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="LED-0603">
<description>&lt;B&gt;LED 0603 SMT&lt;/B&gt;&lt;p&gt;
0603, surface mount.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.075inch &lt;/li&gt;
&lt;li&gt;Area: 0.06" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED - BLUE&lt;/li&gt;</description>
</package>
<package name="LED_10MM">
<description>&lt;B&gt;LED 10mm PTH&lt;/B&gt;&lt;p&gt;
10 mm, round
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.2inch&lt;/li&gt;
&lt;li&gt;Diameter: 10mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;</description>
</package>
<package name="FKIT-LED-1206">
<description>&lt;B&gt;LED 1206 SMT&lt;/B&gt;&lt;p&gt;
1206, surface mount
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Area: 0.125"x 0.06" &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;</description>
</package>
<package name="LED_3MM-NS">
<description>&lt;h3&gt;LED 3MM PTH- No Silk&lt;/h3&gt;

3 mm, round, no silk outline of package

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 3mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="LED_5MM-KIT">
<description>&lt;h3&gt;LED 5mm KIT PTH&lt;/h3&gt;
&lt;p&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example Device:
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="LED-1206-BOTTOM">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
<symbols>
<symbol name="LED">
<description>&lt;h3&gt;LED&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LED" prefix="D" uservalue="yes">
<description>&lt;b&gt;LED (Generic)&lt;/b&gt;
&lt;p&gt;Standard schematic elements and footprints for 5mm, 3mm, 1206, and 0603 sized LEDs. Generic LEDs with no color specified.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="5MM" package="LED_5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM" package="LED_3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08794"/>
</technology>
</technologies>
</device>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10MM" package="LED_10MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-FKIT-1206" package="FKIT-LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3MM-NO_SILK" package="LED_3MM-NS">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM-KIT" package="LED_5MM-KIT">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206-BOTTOM" package="LED-1206-BOTTOM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="U$1" library="fab" deviceset="RESONATOR" device=""/>
<part name="R0" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="C1" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="1uF"/>
<part name="IC1" library="myFab" deviceset="ATTINY44" device="-SSU"/>
<part name="U$7" library="myFab" deviceset="GND" device=""/>
<part name="JP1" library="myFab" deviceset="2X3PINHEADER" device=""/>
<part name="U$9" library="myFab" deviceset="GND" device=""/>
<part name="JP2" library="pinhead-1" deviceset="PINHD-1X6" device="_2.54-SMD-90°" value="Pines"/>
<part name="U$2" library="myFab" deviceset="GND" device=""/>
<part name="R1" library="fab" deviceset="RES-US" device="1206FAB" value="10kohm"/>
<part name="PHOTO" library="SparkFun-Resistors" deviceset="100KOHM" device="-HORIZ-1/4W-1%" value=""/>
<part name="U$3" library="myFab" deviceset="GND" device=""/>
<part name="D1" library="SparkFun-LED" deviceset="LED" device="-FKIT-1206"/>
<part name="R2" library="fab" deviceset="RES-US" device="1206FAB" value="300ohm"/>
<part name="U$4" library="myFab" deviceset="GND" device=""/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="R4">
<segment>
<pinref part="R0" gate="G$1" pin="1"/>
<pinref part="IC1" gate="1" pin="VCC"/>
<pinref part="C1" gate="&gt;NAME" pin="1"/>
<pinref part="JP1" gate="A" pin="5"/>
<pinref part="JP2" gate="A" pin="3"/>
<pinref part="PHOTO" gate="G$1" pin="2"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="JP1" gate="A" pin="1"/>
<pinref part="U$7" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="IC1" gate="1" pin="GND"/>
<pinref part="C1" gate="&gt;NAME" pin="2"/>
<pinref part="U$9" gate="G$1" pin="GND"/>
<pinref part="JP2" gate="A" pin="1"/>
</segment>
<segment>
<pinref part="U$1" gate="G$1" pin="2"/>
<pinref part="U$2" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="R1" gate="G$1" pin="2"/>
<pinref part="U$3" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="U$4" gate="G$1" pin="GND"/>
</segment>
</net>
<net name="N$8">
<segment>
<pinref part="IC1" gate="1" pin="(AREF/ADC0)PA0"/>
<pinref part="JP2" gate="A" pin="4"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="IC1" gate="1" pin="(T1/SCL/USCK/ADC4)PA4"/>
<pinref part="JP1" gate="A" pin="4"/>
</segment>
</net>
<net name="N$5">
<segment>
<pinref part="IC1" gate="1" pin="PA6(OC1A/SDA/MOSI/ADC6)"/>
<pinref part="JP1" gate="A" pin="3"/>
</segment>
</net>
<net name="N$17">
<segment>
<pinref part="IC1" gate="1" pin="(OC1B/MISO/DO/ADC5)PA5"/>
<pinref part="JP1" gate="A" pin="6"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="JP1" gate="A" pin="2"/>
<pinref part="R0" gate="G$1" pin="2"/>
<pinref part="IC1" gate="1" pin="RESET"/>
</segment>
</net>
<net name="N$9">
<segment>
<pinref part="IC1" gate="1" pin="(AIN0/ADC1)PA1"/>
<pinref part="JP2" gate="A" pin="5"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="U$1" gate="G$1" pin="3"/>
<pinref part="IC1" gate="1" pin="PB0(XTAL1/CLKI)"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="U$1" gate="G$1" pin="1"/>
<pinref part="IC1" gate="1" pin="PB1(XTAL2)"/>
</segment>
</net>
<net name="N$6">
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
<pinref part="IC1" gate="1" pin="(T0/ADC3)PA3"/>
<pinref part="PHOTO" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$7">
<segment>
<pinref part="D1" gate="G$1" pin="A"/>
<pinref part="IC1" gate="1" pin="PA7(ICP/OC0B/ADC7)"/>
</segment>
</net>
<net name="N$10">
<segment>
<pinref part="D1" gate="G$1" pin="C"/>
<pinref part="R2" gate="G$1" pin="2"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
