<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="56.1088" y2="0" width="0" layer="20"/>
<wire x1="56.1088" y1="0" x2="56.1088" y2="55.2096" width="0" layer="20"/>
<wire x1="56.1088" y1="55.2096" x2="0" y2="55.2096" width="0" layer="20"/>
<wire x1="0" y1="55.2096" x2="0" y2="0" width="0" layer="20"/>
<text>5V</text>
<text>G</text>
<text>D0</text>
<text>A0</text>
<text>D8</text>
<text>SQUAREDUINO</text>
<text>v0.2</text>
</plain>
<libraries>
<library name="01_FAB_Hello">
<packages>
<package name="2X03SMD">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06-SMD">
</package>
<package name="1206">
</package>
<package name="1X02_NO_SILK">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X06-CLEANBIG">
</package>
<package name="1X08-CLEANBIG">
</package>
</packages>
</library>
<library name="CEDTv79">
<description>&lt;b&gt;Center for Electronics Design and Technology&lt;/b&gt;&lt;br&gt;
at&lt;br&gt;
Netaji Subhas Institute of Technology&lt;br&gt;
Dwarka,&lt;br&gt;
New Delhi, India&lt;br&gt;
&lt;br&gt;
Data Modified :24-December-2013&lt;br&gt;
&lt;br&gt;
CEDT is Managed by Dhananjay V. Gadre (dvgadre@gmail.com)&lt;br&gt;&lt;br&gt;
&lt;br&gt;
Library Maintained By Rohit Gupta (rohit7gupta@gmail.com)
&lt;br&gt;
&lt;br&gt;
Get the latest version from &lt;a href="https://github.com/IndianTinker/CEDT-EagleLibrary"&gt;here&lt;/a&gt;
&lt;br&gt;&lt;br&gt;
&lt;author&gt;This library was created by Anurag Chugh, Rohit Dureja and Shanjit Singh Jajmann and distinguished members of CEDT,NSIT &lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_adafruit">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="01_ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="01_fab">
<packages>
<package name="EFOBM">
</package>
</packages>
</library>
<library name="01_Arduino-AVR">
<description>&lt;b&gt;Arduino Microcontrollers&lt;/b&gt;
&lt;p&gt;
Atmel ATmega8, ATmega168: 8-bit AVR microcontrollers
&lt;p&gt;&lt;ul&gt;
&lt;li&gt;&lt;i&gt;ATmega8 was used on the original Arduino Serial and USB boards&lt;br&gt;
- 28-pin PDIP (32-lead packages also included)&lt;/i&gt;
&lt;li&gt;ATmega168 for current Arduino Diecimila and NG boards&lt;br&gt;
 - 28-pin PDIP
&lt;li&gt;ATMEGA168 for the Arduino Nano, Mini, LilyPad, Pro and so forth&lt;br&gt;
- 32-lead TQFP and 32-pad QFN/MLF
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;from Rob Faludi: www.faludi.com/projects&lt;/p&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm

Reduced pin width</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="01_FAB_Hello" package="2X03SMD" value=""/>
<element name="JP2" library="01_SparkFun" package="1X06-SMD" value=""/>
<element name="IC1" library="01_Arduino-AVR" package="TQFP32-08" value="ATMEGA168-AU"/>
<element name="JP3" library="adafruit" package="1X06-CLEANBIG" value=""/>
<element name="JP4" library="adafruit" package="1X08-CLEANBIG" value=""/>
<element name="C2" library="01_SparkFun" package="1206" value="0.1uF"/>
<element name="C3" library="01_SparkFun" package="1206" value="0.1uF"/>
<element name="C4" library="01_SparkFun" package="1206" value="0.1uF"/>
<element name="IC2" library="CEDTv79" package="SOT223" value="LM2940IMP"/>
<element name="C1" library="01_SparkFun" package="1206" value="0.1uF"/>
<element name="C5" library="01_SparkFun" package="1206" value="0.1uF"/>
<element name="C6" library="01_SparkFun" package="1206" value="0.1uF"/>
<element name="R1" library="01_adafruit" package="R1206" value="10K"/>
<element name="S1" library="01_FAB_Hello" package="6MM_SWITCH" value=""/>
<element name="JP5" library="adafruit" package="1X06-CLEANBIG" value=""/>
<element name="R2" library="01_adafruit" package="R1206" value="499"/>
<element name="U$5" library="01_ng" package="1206" value=""/>
<element name="U$6" library="01_ng" package="1206" value=""/>
<element name="R3" library="01_adafruit" package="R1206" value="499"/>
<element name="JP6" library="01_SparkFun" package="1X02_NO_SILK" value=""/>
<element name="16MHZ" library="01_fab" package="EFOBM" value="RESONATOR"/>
<element name="R4" library="01_SparkFun" package="1206" value="0K"/>
</elements>
<signals>
<signal name="MOSI">
<contactref element="JP1" pad="4"/>
<contactref element="IC1" pad="15"/>
<contactref element="JP5" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="16"/>
<contactref element="JP5" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="3"/>
<contactref element="IC1" pad="17"/>
<contactref element="JP5" pad="6"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="21"/>
<contactref element="JP1" pad="6"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U$5" pad="2"/>
<contactref element="U$6" pad="2"/>
<contactref element="JP6" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="16MHZ" pad="2"/>
</signal>
<signal name="RX">
<contactref element="JP2" pad="4"/>
<contactref element="IC1" pad="30"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="TX">
<contactref element="JP2" pad="5"/>
<contactref element="IC1" pad="31"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="RTS">
<contactref element="JP2" pad="6"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="UCC">
</signal>
<signal name="A0">
<contactref element="IC1" pad="23"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="24"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="A2">
<contactref element="IC1" pad="25"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="A3">
<contactref element="IC1" pad="26"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="A4">
<contactref element="IC1" pad="27"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="A5">
<contactref element="IC1" pad="28"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="D2">
<contactref element="IC1" pad="32"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="D3">
<contactref element="IC1" pad="1"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="D4">
<contactref element="IC1" pad="2"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="D6">
<contactref element="IC1" pad="10"/>
<contactref element="JP4" pad="7"/>
</signal>
<signal name="D7">
<contactref element="IC1" pad="11"/>
<contactref element="JP4" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="20"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="VBUS">
<contactref element="JP2" pad="3"/>
<contactref element="C5" pad="2"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="5V">
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="18"/>
<contactref element="R2" pad="2"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="IC1" pad="29"/>
<contactref element="C6" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="D8">
<contactref element="IC1" pad="12"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="D9">
<contactref element="IC1" pad="13"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="D10">
<contactref element="IC1" pad="14"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="1"/>
<contactref element="U$5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$6" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="D5">
<contactref element="JP4" pad="6"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="XTAL1">
<contactref element="IC1" pad="7"/>
<contactref element="16MHZ" pad="1"/>
</signal>
<signal name="XTAL2">
<contactref element="IC1" pad="8"/>
<contactref element="16MHZ" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="JP4" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
