(kicad_pcb (version 4) (host pcbnew 4.0.0-rc1-stable)
  (general
    (links 65)
    (no_connects 6)
    (area 122.062999 99.456999 169.656001 134.604001)
    (thickness 1.6)
    (drawings 12)
    (tracks 209)
    (zones 0)
    (modules 20)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.35)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VIN)
  (net 2 GND)
  (net 3 VCC)
  (net 4 XTAL1)
  (net 5 XTAL2)
  (net 6 RST)
  (net 7 MOSI)
  (net 8 MISO)
  (net 9 MOT11)
  (net 10 MOT12)
  (net 11 MOT22)
  (net 12 MOT21)
  (net 13 OUT11)
  (net 14 OUT12)
  (net 15 OUT22)
  (net 16 OUT21)
  (net 17 BTN1)
  (net 18 BTN2)
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net BTN1)
    (add_net BTN2)
    (add_net MISO)
    (add_net MOSI)
    (add_net MOT11)
    (add_net MOT12)
    (add_net MOT21)
    (add_net MOT22)
    (add_net OUT11)
    (add_net OUT12)
    (add_net OUT21)
    (add_net OUT22)
    (add_net RST)
    (add_net VCC)
    (add_net XTAL1)
    (add_net XTAL2)
  )
  (net_class Slim ""
    (clearance 0.4)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class VIN ""
    (clearance 0.4)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net VIN)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 140.81697 120.360628 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value C (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 XTAL2))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 140.81697 112.827628 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value C (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 XTAL1))
    (model "C:/Program Files/KiCad/share/kicad/modules/packages3d/Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 159.131 131.445 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference 0.22u1 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value C (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VIN))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 158.75 116.967 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference 0.22u2 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value C (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VIN))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 147.193 103.378)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference 100n1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value C (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VIN))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 147.173 106.172)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference 100n2 (at 0 -2.1) (layer F.SilkS))
    (fp_text value C (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_4x4.5 (layer F.Cu) (tedit 55725C01)
    (at 158.877 113.03)
    (descr "SMT capacitor, aluminium electrolytic, 4x4.5")
    (attr smd)
    (fp_text reference 100u1 (at 0 -3.175) (layer F.SilkS))
    (fp_text value CP (at 0 3.175) (layer F.Fab))
    (pad 1 smd rect (at 1.80086 0) (size 2.60096 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 VIN))
    (pad 2 smd rect (at -1.80086 0) (size 2.60096 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_4x4.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_4x4.5 (layer F.Cu) (tedit 55725C01)
    (at 159.258 127.508)
    (descr "SMT capacitor, aluminium electrolytic, 4x4.5")
    (attr smd)
    (fp_text reference 100u2 (at 0 -3.175) (layer F.SilkS))
    (fp_text value CP (at 0 3.175) (layer F.Fab))
    (pad 1 smd rect (at 1.80086 0) (size 2.60096 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 VIN))
    (pad 2 smd rect (at -1.80086 0) (size 2.60096 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_4x4.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 137.64197 111.418628 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 1u (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-SOIC14 (layer F.Cu) (tedit 200000)
    (at 149.0345 112.522 270)
    (descr "SMALL OUTLINE PACKAGE")
    (tags "SMALL OUTLINE PACKAGE")
    (attr smd)
    (fp_text reference IC1 (at -5.1435 -1.143 360) (layer B.SilkS))
    (fp_text value ATTINY44-SSU (at 1.27 0.0635 270) (layer B.SilkS))
    (pad 1 smd rect (at -3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at -2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 4 XTAL1))
    (pad 3 smd rect (at -1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 5 XTAL2))
    (pad 4 smd rect (at 0 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 6 RST))
    (pad 5 smd rect (at 1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 17 BTN1))
    (pad 6 smd rect (at 2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 18 BTN2))
    (pad 7 smd rect (at 3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 7 MOSI))
    (pad 8 smd rect (at 3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 8 MISO))
    (pad 9 smd rect (at 2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 9 MOT11))
    (pad 10 smd rect (at 1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 10 MOT12))
    (pad 11 smd rect (at 0 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 12 smd rect (at -1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 12 MOT21))
    (pad 13 smd rect (at -2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 11 MOT22))
    (pad 14 smd rect (at -3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 149.098 123.825 270)
    (attr smd)
    (fp_text reference M2 (at -0.635 -4.445 270) (layer B.SilkS))
    (fp_text value AVRISPSMD (at 0 4.445 270) (layer B.SilkS))
    (pad 1 smd rect (at -2.54 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 MISO))
    (pad 2 smd rect (at 2.91846 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 3 smd rect (at -2.54 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 MOT11))
    (pad 4 smd rect (at 2.91846 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 MOSI))
    (pad 5 smd rect (at -2.54 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 RST))
    (pad 6 smd rect (at 2.91846 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module fablab-inventory:Pin_Header_Angled_SMD_1X04 (layer F.Cu) (tedit 56DAB1D1)
    (at 170.307 115.824 270)
    (fp_text reference P1 (at -6.35 3.81 360) (layer F.SilkS))
    (fp_text value Header_angled_SMT_1X04 (at 0 7.62 270) (layer F.Fab))
    (pad 1 smd rect (at -3.81 5.205 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 15 OUT22))
    (pad 2 smd oval (at -1.27 5.205 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 16 OUT21))
    (pad 3 smd oval (at 1.27 5.205 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 14 OUT12))
    (pad 4 smd oval (at 3.81 5.205 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 13 OUT11))
  )
  (module fablab-inventory:Pin_Header_Angled_SMD_1X02 (layer F.Cu) (tedit 56DAB188)
    (at 156.845 104.648 270)
    (fp_text reference P2 (at -3.81 3.81 360) (layer F.SilkS))
    (fp_text value Header_angled_SMT_1X02 (at 0 7.62 270) (layer F.Fab))
    (pad 1 smd rect (at -1.27 5.205 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 1 VIN))
    (pad 2 smd oval (at 1.27 5.205 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 147.908 118.491 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 RST))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 142.875 104.775 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U1 (at 0 -2.25 90) (layer F.SilkS))
    (fp_text value LM3480-5.0 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 VIN))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 54130A77)
    (at 158.8295 121.7455)
    (descr "8-Lead Thermally Enhanced Plastic Small Outline (SE) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -3.5) (layer F.SilkS))
    (fp_text value A4950E (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 MOT12))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 MOT11))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VIN))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 OUT11))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 OUT12))
    (pad 9 smd rect (at 0.5875 0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.5875 -0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.5875 0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.5875 -0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_SOIC.3dshapes/SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 54130A77)
    (at 158.5755 107.3625)
    (descr "8-Lead Thermally Enhanced Plastic Small Outline (SE) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 -3.5) (layer F.SilkS))
    (fp_text value A4950E (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 MOT22))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 MOT21))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VIN))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 OUT21))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 OUT22))
    (pad 9 smd rect (at 0.5875 0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.5875 -0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.5875 0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.5875 -0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_SOIC.3dshapes/SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-SD_SMD (layer F.Cu) (tedit 0)
    (at 133.57797 116.299488 90)
    (descr "Crystal Quarz HC49-SD SMD")
    (tags "Crystal Quarz HC49-SD SMD")
    (attr smd)
    (fp_text reference X1 (at 0 -5.08 90) (layer F.SilkS))
    (fp_text value CRYSTAL_SMD (at 2.54 5.08 90) (layer F.Fab))
    (pad 1 smd rect (at -4.84886 0 90) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 5 XTAL2))
    (pad 2 smd rect (at 4.84886 0 90) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 4 XTAL1))
  )
  (module fab:fab-6MM_SWITCH (layer F.Cu) (tedit 200000)
    (at 130.429 128.524 180)
    (descr "OMRON SWITCH")
    (tags "OMRON SWITCH")
    (attr smd)
    (fp_text reference S1 (at 0.127 -4.318 180) (layer B.SilkS))
    (fp_text value 6MM_SWITCH6MM_SWITCH (at 0.762 4.445 180) (layer B.SilkS))
    (fp_text user 1 (at -3.683 -2.286 180) (layer B.SilkS))
    (fp_text user 2 (at 4.191 -2.159 180) (layer B.SilkS))
    (fp_text user 3 (at -3.937 2.159 180) (layer B.SilkS))
    (fp_text user 4 (at 4.191 2.159 180) (layer B.SilkS))
    (pad 1 smd rect (at -3.302 -2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.302 -2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.302 2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 17 BTN1))
    (pad 4 smd rect (at 3.302 2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 17 BTN1))
  )
  (module fab:fab-6MM_SWITCH (layer F.Cu) (tedit 200000)
    (at 140.208 128.524 180)
    (descr "OMRON SWITCH")
    (tags "OMRON SWITCH")
    (attr smd)
    (fp_text reference S2 (at 0.127 -4.318 180) (layer B.SilkS))
    (fp_text value 6MM_SWITCH6MM_SWITCH (at 0.762 4.445 180) (layer B.SilkS))
    (fp_text user 1 (at -3.683 -2.286 180) (layer B.SilkS))
    (fp_text user 2 (at 4.191 -2.159 180) (layer B.SilkS))
    (fp_text user 3 (at -3.937 2.159 180) (layer B.SilkS))
    (fp_text user 4 (at 4.191 2.159 180) (layer B.SilkS))
    (pad 1 smd rect (at -3.302 -2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.302 -2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.302 2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 18 BTN2))
    (pad 4 smd rect (at 3.302 2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 18 BTN2))
  )
  (gr_line (start 168.656 107.315) (end 161.798 100.457) (layer Edge.Cuts) (width 2))
  (gr_line (start 168.656 127.127) (end 168.656 107.315) (layer Edge.Cuts) (width 2))
  (gr_line (start 162.179 133.604) (end 168.656 127.127) (layer Edge.Cuts) (width 2))
  (gr_line (start 125.222 133.604) (end 162.179 133.604) (layer Edge.Cuts) (width 2))
  (gr_line (start 123.063 131.445) (end 125.222 133.604) (layer Edge.Cuts) (width 2))
  (gr_line (start 123.063 123.698) (end 123.063 131.445) (layer Edge.Cuts) (width 2))
  (gr_line (start 124.968 123.698) (end 123.063 123.698) (layer Edge.Cuts) (width 2))
  (gr_line (start 127.762 123.698) (end 124.968 123.698) (layer Edge.Cuts) (width 2))
  (gr_line (start 130.302 121.158) (end 127.762 123.698) (layer Edge.Cuts) (width 2))
  (gr_line (start 130.302 107.442) (end 130.302 121.158) (layer Edge.Cuts) (width 2))
  (gr_line (start 137.287 100.457) (end 130.302 107.442) (layer Edge.Cuts) (width 2))
  (gr_line (start 161.798 100.457) (end 137.287 100.457) (layer Edge.Cuts) (width 2))
)
