<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0.0634" y1="0.1066" x2="38.1382" y2="0.1828" width="0" layer="20"/>
<wire x1="38.1382" y1="0.1828" x2="38.0874" y2="37.9934" width="0" layer="20"/>
<wire x1="38.0874" y1="37.9934" x2="-0.0382" y2="37.9934" width="0" layer="20"/>
<wire x1="-0.0382" y1="37.9934" x2="0.0634" y2="0.1066" width="0" layer="20"/>
<rectangle x1="0" y1="0.127" x2="38.1508" y2="37.973" layer="46"/>
<text>LED ARRAY</text>
</plain>
<libraries>
<library name="con-lstb">
<packages>
<package name="MA08-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="00_fab">
<packages>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SV2" library="con-lstb" package="MA08-1" value=""/>
<element name="SV4" library="con-lstb" package="MA08-1" value=""/>
<element name="SV1" library="con-lstb" package="MA08-1" value=""/>
<element name="BLUELED" library="00_fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="R1" library="00_fab" package="R1206FAB" value="499"/>
<element name="R2" library="00_fab" package="R1206FAB" value="0"/>
<element name="R3" library="00_fab" package="R1206FAB" value="0"/>
<element name="R4" library="00_fab" package="R1206FAB" value="0"/>
<element name="BLUELED1" library="00_fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="BLUELED2" library="00_fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="R6" library="00_fab" package="R1206FAB" value="499"/>
<element name="R7" library="00_fab" package="R1206FAB" value="499"/>
<element name="R8" library="00_fab" package="R1206FAB" value="499"/>
<element name="BLUELED4" library="00_fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="BLUELED5" library="00_fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="BLUELED6" library="00_fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="R9" library="00_fab" package="R1206FAB" value="0"/>
<element name="R10" library="00_fab" package="R1206FAB" value="0"/>
<element name="R11" library="00_fab" package="R1206FAB" value="0"/>
<element name="BLUELED7" library="00_fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="BLUELED8" library="00_fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="BLUELED9" library="00_fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="R12" library="00_fab" package="R1206FAB" value="0"/>
<element name="R13" library="00_fab" package="R1206FAB" value="0"/>
<element name="R14" library="00_fab" package="R1206FAB" value="0"/>
<element name="BLUELED10" library="00_fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="BLUELED11" library="00_fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="BLUELED12" library="00_fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="R15" library="00_fab" package="R1206FAB" value="0"/>
<element name="R16" library="00_fab" package="R1206FAB" value="0"/>
<element name="R17" library="00_fab" package="R1206FAB" value="0"/>
</elements>
<signals>
<signal name="PIN9">
<contactref element="R1" pad="1"/>
<contactref element="SV2" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="SV2" pad="5"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R7" pad="2"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="R8" pad="2"/>
<contactref element="SV1" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="BLUELED" pad="2"/>
<contactref element="BLUELED1" pad="2"/>
<contactref element="BLUELED2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="2"/>
<contactref element="BLUELED" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="2"/>
<contactref element="BLUELED1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R8" pad="1"/>
<contactref element="BLUELED6" pad="2"/>
<contactref element="BLUELED9" pad="2"/>
<contactref element="BLUELED12" pad="2"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R15" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="BLUELED10" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R4" pad="2"/>
<contactref element="BLUELED2" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R7" pad="1"/>
<contactref element="BLUELED5" pad="2"/>
<contactref element="BLUELED8" pad="2"/>
<contactref element="BLUELED11" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R12" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="BLUELED7" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="1"/>
<contactref element="BLUELED4" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="BLUELED7" pad="2"/>
<contactref element="BLUELED10" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R9" pad="1"/>
<contactref element="BLUELED5" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R16" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="BLUELED11" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R10" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="BLUELED6" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="BLUELED12" pad="1"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R13" pad="2"/>
<contactref element="BLUELED8" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="R14" pad="2"/>
<contactref element="BLUELED9" pad="1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R9" pad="2"/>
<contactref element="BLUELED4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
