<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="48.77" y2="0" width="0" layer="20"/>
<wire x1="48.77" y1="0" x2="48.77" y2="31.09" width="0" layer="20"/>
<wire x1="48.77" y1="31.09" x2="0" y2="31.09" width="0" layer="20"/>
<wire x1="0" y1="31.09" x2="0" y2="0" width="0" layer="20"/>
<text>T</text>
<text>R</text>
<text>G</text>
<text>G</text>
<text>Bridge</text>
<text>Node 0</text>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="2X02SMD">
</package>
<package name="C1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="R1206FAB">
</package>
<package name="1X06SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BRIDGE" library="fab" package="SOIC8" value="ATTINY45SI"/>
<element name="BUS" library="fab" package="2X02SMD" value=""/>
<element name="C1" library="fab" package="C1206FAB" value="1uF"/>
<element name="JP1" library="fab" package="2X03SMD" value=""/>
<element name="LED1" library="fab" package="LED1206FAB" value="Green"/>
<element name="R1" library="fab" package="R1206FAB" value="10k"/>
<element name="R2" library="fab" package="R1206FAB" value="1k"/>
<element name="FTDI" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="R3" library="fab" package="R1206FAB" value="499 ohm"/>
<element name="LED2" library="fab" package="LED1206FAB" value="Blue"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="BUS" pad="1"/>
<contactref element="FTDI" pad="1"/>
<contactref element="BRIDGE" pad="4"/>
<contactref element="JP1" pad="1"/>
<contactref element="LED2" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="BRIDGE" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="5"/>
<contactref element="BRIDGE" pad="8"/>
<contactref element="BUS" pad="3"/>
<contactref element="FTDI" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="6"/>
<contactref element="BRIDGE" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="R2" pad="2"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="TX">
<contactref element="BUS" pad="2"/>
<contactref element="FTDI" pad="4"/>
<contactref element="BRIDGE" pad="2"/>
</signal>
<signal name="RX">
<contactref element="BUS" pad="4"/>
<contactref element="FTDI" pad="5"/>
<contactref element="BRIDGE" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="BRIDGE" pad="7"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="2"/>
<contactref element="LED2" pad="1"/>
</signal>
<signal name="MOSI/LED">
<contactref element="BRIDGE" pad="5"/>
<contactref element="JP1" pad="3"/>
<contactref element="LED1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
