#

##

##

    礦ision Build Log
    Project:
    C:\nRF51\5.青云测试代码\第1部分：外设应用篇\实验3：按键扫描副本\user\key.uvproj
    Project File Date:  03/18/2016

    Output:
    Build target 'Target 1'
    compiling key.c...
    linking...
    Program Size: Code=932 RO-data=224 RW-data=4 ZI-data=4196
    ".\key.axf" - 0 Error(s), 0 Warning(s).

... Program Size: Code=932 RO-data=224 RW-data=4 ZI-data=4196 ".\key.axf" - 0 Error(s), 0 Warning(s). ected (256 KB flash, 8 KB RAM). Set JLink Project File to "C:\nRF51\5.青云测试代码\第1部分：外设应用篇\实验3：按键扫描副本\user\JLinkSettings.ini" * JLink Info: Device "NRF51822" selected (256 KB flash, 8 KB RAM). JLink info: ------------ DLL: V4.60a, compiled Jan 16 2013 17:15:30 Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04 Hardware: V7.00 S/N : 20090928 Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull * JLink Info: Found SWD-DP with ID 0x0BB11477 * JLink Info: FPUnit: 4 code (BP) slots and 0 literal slots * JLink Info: Found Cortex-M0 r0p0, Little endian. ROMTableAddr = 0xE00FF003 Target info: ------------ Device: nRF51822_xxAA VTarget = 3.300V State of Pins: TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1 Hardware-Breakpoints: 4 Software-Breakpoints: 8192 Watchpoints: 2 JTAG speed: 2000 kHz Erase Done. Programming Done. Verify OK. Application running ... n running ...