<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="27.92" y2="0" width="0" layer="20"/>
<wire x1="27.92" y1="0" x2="27.92" y2="17.12" width="0" layer="20"/>
<wire x1="27.92" y1="17.12" x2="0" y2="17.12" width="0" layer="20"/>
<wire x1="0" y1="17.12" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="R1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X1-BIGPOGO">
</package>
<package name="1X03-CLEANBIG">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="fab" package="R1206FAB" value="1k ohm"/>
<element name="R2" library="fab" package="R1206FAB" value="1k ohm"/>
<element name="R3" library="fab" package="R1206FAB" value="1k ohm"/>
<element name="U$1" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$2" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$3" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="JP1" library="adafruit" package="1X1-BIGPOGO" value=""/>
<element name="JP2" library="adafruit" package="1X03-CLEANBIG" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$3" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="JP2" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="JP2" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="JP2" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$1" pad="2"/>
<contactref element="JP1" pad="P$1"/>
</signal>
<signal name="GND">
</signal>
<signal name="N$9">
</signal>
</signals>
</board>
</drawing>
</eagle>
