(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 26)
    (no_connects 1)
    (area 151.054999 93.904999 185.495001 127.075001)
    (thickness 1.6)
    (drawings 4)
    (tracks 110)
    (zones 0)
    (modules 10)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4064)
    (user_trace_width 0.2032)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 151.13 127)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x01020_00000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory C:/Users/chewlk/Documents/kicad/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(D1-Pad1)")
  (net 4 /LED)
  (net 5 "Net-(IC1-Pad2)")
  (net 6 "Net-(IC1-Pad3)")
  (net 7 /RST)
  (net 8 /PB)
  (net 9 /MOSI)
  (net 10 /MISO)
  (net 11 /SCK)
  (net 12 "Net-(IC1-Pad10)")
  (net 13 "Net-(IC1-Pad11)")
  (net 14 "Net-(IC1-Pad12)")
  (net 15 "Net-(IC1-Pad13)")
  (net 16 "Net-(J2-Pad2)")
  (net 17 "Net-(J2-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /LED)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /PB)
    (add_net /RST)
    (add_net /SCK)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad6)")
    (add_net VCC)
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 173.99 97.79)
    (attr smd)
    (fp_text reference C1 (at 0.762 -1.778) (layer B.SilkS))
    (fp_text value 1uF (at 1.27 1.778) (layer B.SilkS))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module fab:fab-LED1206FAB (layer F.Cu) (tedit 200000)
    (at 161.29 109.22 90)
    (descr "LED1206 FAB STYLE (SMALLER PADS TO ALLOW TRACE BETWEEN)")
    (tags "LED1206 FAB STYLE (SMALLER PADS TO ALLOW TRACE BETWEEN)")
    (attr smd)
    (fp_text reference D1 (at 0.762 -1.778 90) (layer B.SilkS))
    (fp_text value LED (at 1.27 1.778 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 4 /LED))
  )
  (module fab:fab-SOIC14 (layer F.Cu) (tedit 56DB93CA)
    (at 170.18 106.68 270)
    (descr "SMALL OUTLINE PACKAGE")
    (tags "SMALL OUTLINE PACKAGE")
    (attr smd)
    (fp_text reference IC1 (at -5.1435 -1.143 360) (layer B.SilkS))
    (fp_text value ATTINY44 (at 0 -0.254 270) (layer F.SilkS))
    (pad 1 smd rect (at -3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at 0 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 7 /RST))
    (pad 5 smd rect (at 1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 4 /LED))
    (pad 6 smd rect (at 2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 8 /PB))
    (pad 7 smd rect (at 3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 9 /MOSI))
    (pad 8 smd rect (at 3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 10 /MISO))
    (pad 9 smd rect (at 2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCK))
    (pad 10 smd rect (at 1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at 0 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at -2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at -3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 56DB9325)
    (at 170.18 119.38 270)
    (attr smd)
    (fp_text reference J1 (at 1.27 4.445 270) (layer B.SilkS))
    (fp_text value ISP (at -1.27 -4.445 270) (layer B.SilkS))
    (pad 1 smd rect (at -2.54 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 /MISO))
    (pad 2 smd rect (at 2.91846 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at -2.54 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCK))
    (pad 4 smd rect (at 2.91846 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 /MOSI))
    (pad 5 smd rect (at -2.54 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 /RST))
    (pad 6 smd rect (at 2.91846 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module fab:fab-1X06SMD (layer F.Cu) (tedit 56DB93F9)
    (at 180.34 104.14)
    (attr smd)
    (fp_text reference J2 (at -2.54 0 90) (layer B.SilkS))
    (fp_text value FTDI (at -0.254 8.382) (layer F.SilkS))
    (pad 1 smd rect (at 0 -6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 -3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at 0 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 4 smd rect (at 0 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad13)"))
    (pad 5 smd rect (at 0 3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad12)"))
    (pad 6 smd rect (at 0 6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-Pad6)"))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 167.64 97.79)
    (attr smd)
    (fp_text reference R1 (at 0.762 -1.778) (layer B.SilkS))
    (fp_text value 10k (at 1.27 1.778) (layer B.SilkS))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 7 /RST))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 154.94 107.95)
    (attr smd)
    (fp_text reference R2 (at 0.762 -1.778) (layer B.SilkS))
    (fp_text value 499 (at 1.27 1.778) (layer B.SilkS))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 56DB935A)
    (at 154.94 111.76)
    (attr smd)
    (fp_text reference R3 (at -1.27 1.905) (layer B.SilkS))
    (fp_text value 10k (at 2.032 1.778) (layer B.SilkS))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 8 /PB))
  )
  (module fab:fab-6MM_SWITCH (layer F.Cu) (tedit 56DB9308)
    (at 160.02 119.38 270)
    (descr "OMRON SWITCH")
    (tags "OMRON SWITCH")
    (attr smd)
    (fp_text reference S1 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value PB (at 0 -3.81 270) (layer B.SilkS))
    (fp_text user 1 (at -3.683 -2.286 270) (layer B.SilkS))
    (fp_text user 2 (at 4.191 -2.159 270) (layer B.SilkS))
    (fp_text user 3 (at -3.937 2.159 270) (layer B.SilkS))
    (fp_text user 4 (at 4.191 2.159 270) (layer B.SilkS))
    (pad 1 smd rect (at -3.302 -2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.302 -2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.302 2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 8 /PB))
    (pad 4 smd rect (at 3.302 2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 8 /PB))
  )
  (module fab:fab-EFOBM (layer F.Cu) (tedit 56DB8FDB)
    (at 160.02 102.87 270)
    (attr smd)
    (fp_text reference XTAL1 (at -3.175 -0.127 360) (layer F.SilkS))
    (fp_text value 20MHz (at 2.667 -0.254 360) (layer F.SilkS))
    (pad 1 smd rect (at -1.34874 0) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad2)"))
    (pad 2 smd rect (at 0 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.34874 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad3)"))
  )
  (gr_line (start 151.13 93.98) (end 151.13 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185.42 93.98) (end 151.13 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185.42 127) (end 185.42 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.13 127) (end 185.42 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.511 94.488) (xy 151.511 126.619) (xy 185.039 126.492) (xy 185.166 94.488) (xy 151.511 94.361)
        (xy 151.511 94.488)
      )
    )
  )
)
