(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 20)
    (no_connects 1)
    (area 135.535999 79.655999 177.138801 122.465301)
    (thickness 1.6)
    (drawings 10)
    (tracks 95)
    (zones 0)
    (modules 7)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.35)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 1.7)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ../))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 "Net-(IC1-Pad2)")
  (net 3 "Net-(IC1-Pad3)")
  (net 4 /PB3)
  (net 5 /PA6)
  (net 6 /PA5)
  (net 7 /PA4)
  (net 8 "Net-(IC1-Pad10)")
  (net 9 "Net-(IC1-Pad11)")
  (net 10 "Net-(IC1-Pad12)")
  (net 11 "Net-(IC1-Pad13)")
  (net 12 GND)
  (net 13 "Net-(IC1-Pad5)")
  (net 14 /PA7)
  (net 15 "Net-(M2-Pad1)")
  (net 16 "Net-(M2-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /PA4)
    (add_net /PA5)
    (add_net /PA6)
    (add_net /PA7)
    (add_net /PB3)
    (add_net GND)
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(M2-Pad1)")
    (add_net "Net-(M2-Pad5)")
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 572DC187)
    (at 167.1828 116.6241 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 0 (at 0 2.3 90) (layer F.Fab))
    (pad 2 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-SOIC14 (layer F.Cu) (tedit 200000)
    (at 161.2265 109.093 90)
    (descr "SMALL OUTLINE PACKAGE")
    (tags "SMALL OUTLINE PACKAGE")
    (attr smd)
    (fp_text reference IC1 (at -5.1435 -1.143 180) (layer B.SilkS))
    (fp_text value ATTINY44A-SS (at 1.27 0.0635 90) (layer B.SilkS))
    (pad 1 smd rect (at -3.81 2.6035 90) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -2.54 2.6035 90) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -1.27 2.6035 90) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at 0 2.6035 90) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 4 /PB3))
    (pad 5 smd rect (at 1.27 2.6035 90) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad5)"))
    (pad 6 smd rect (at 2.54 2.6035 90) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 14 /PA7))
    (pad 7 smd rect (at 3.81 2.6035 90) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 5 /PA6))
    (pad 8 smd rect (at 3.81 -2.6035 90) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 6 /PA5))
    (pad 9 smd rect (at 2.54 -2.6035 90) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 7 /PA4))
    (pad 10 smd rect (at 1.27 -2.6035 90) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at 0 -2.6035 90) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -1.27 -2.6035 90) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at -2.54 -2.6035 90) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at -3.81 -2.6035 90) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 161.1884 99.9236 90)
    (attr smd)
    (fp_text reference M1 (at -0.635 -4.445 90) (layer B.SilkS))
    (fp_text value "AVRISP & I2C" (at 0 4.445 90) (layer B.SilkS))
    (pad 1 smd rect (at -2.54 -2.54 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 /PA5))
    (pad 2 smd rect (at 2.91846 -2.54 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.54 0 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 /PA4))
    (pad 4 smd rect (at 2.91846 0 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 /PA6))
    (pad 5 smd rect (at -2.54 2.54 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 /PB3))
    (pad 6 smd rect (at 2.91846 2.54 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 170.3324 99.9236 90)
    (attr smd)
    (fp_text reference M2 (at -0.635 -4.445 90) (layer B.SilkS))
    (fp_text value I2C (at 0 4.445 90) (layer B.SilkS))
    (pad 1 smd rect (at -2.54 -2.54 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(M2-Pad1)"))
    (pad 2 smd rect (at 2.91846 -2.54 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.54 0 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 /PA4))
    (pad 4 smd rect (at 2.91846 0 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 /PA6))
    (pad 5 smd rect (at -2.54 2.54 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(M2-Pad5)"))
    (pad 6 smd rect (at 2.91846 2.54 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
  )
  (module Connect:PINHEAD1-3 (layer F.Cu) (tedit 572DB8F0)
    (at 161.3662 115.8494 180)
    (attr virtual)
    (fp_text reference P1 (at 0.1524 -3.6322 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 14 /PA7))
    (pad 2 thru_hole oval (at 0 0 180) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 12 GND))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 572DAC16)
    (at 169.9768 107.2896)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 10k (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /PB3))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fablab-noninventory:Crystal_XC1109CT-ND (layer F.Cu) (tedit 572DAE58)
    (at 168.91 110.998 90)
    (fp_text reference X1 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value CRYSTAL_SMD (at 0 -3.81 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0 90) (size 0.75 3.8) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 1.27 0 90) (size 0.75 3.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad3)"))
    (pad 3 smd rect (at -1.27 0 90) (size 0.75 3.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad2)"))
  )
  (gr_line (start 155.0416 91.0336) (end 155.0416 91.1225) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.0888 91.0336) (end 155.0416 91.0336) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.0888 122.4153) (end 177.0888 91.0336) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.0416 122.4153) (end 177.0888 122.4153) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.0416 91.1225) (end 155.0416 122.4153) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text servo_44_I2C (at 174.8663 113.792 270) (layer F.Cu))
)
