<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="63.551" y2="0" width="0" layer="20"/>
<wire x1="63.551" y1="0" x2="63.551" y2="46.98" width="0" layer="20"/>
<wire x1="63.551" y1="46.98" x2="0" y2="46.98" width="0" layer="20"/>
<wire x1="0" y1="46.98" x2="0" y2="0" width="0" layer="20"/>
<text>A5</text>
<text>+</text>
<text>A4</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>1</text>
<text>0</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>VCC</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>-</text>
<text>Fab Lab</text>
<text>TECSUP</text>
<text>J1</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>DTR</text>
<text>Tx</text>
<text>Rx</text>
<text>MOSI</text>
<text>MISO</text>
<text>SCK</text>
</plain>
<libraries>
<library name="atmega8">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="ng">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="01_fab">
<packages>
<package name="2X03SMD">
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="01_ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="JACK_2.1MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="atmega8" package="TQFP32-08" value="ATMEGA328P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="ng" package="1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="ng" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="ng" package="1206" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="ng" package="1206" value="LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="ng" package="1206" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="ng" package="1206" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C1206" value=".1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X06" value="FTDI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="01_FAB_Hello" package="1206" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="01_FAB_Hello" package="1206" value="LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="01_fab" package="2X03SMD" value="AVRISPSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="XTAL" library="crystal" package="HC49/S" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C025-024X044" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C025-024X044" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="01_SparkFun" package="SOT223" value="V_REG_MIC2920">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="01_SparkFun" package="1206" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="01_SparkFun" package="1206" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="01_ng" package="1206" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="fab" package="JACK_2.1MM" value="JACK2.1MM"/>
<element name="JP7" library="pinhead" package="1X02" value=""/>
<element name="R5" library="01_ng" package="1206" value="0"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="D2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="JP3" pad="6"/>
<contactref element="D1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="J2" pad="6"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="JP3" pad="5"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP5" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="J3" pad="CONTACT"/>
<contactref element="JP7" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="JP3" pad="4"/>
<contactref element="R4" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="6"/>
<contactref element="J2" pad="2"/>
<contactref element="JP5" pad="4"/>
<contactref element="JP5" pad="3"/>
<contactref element="U2" pad="3"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="29"/>
<contactref element="R1" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="J2" pad="5"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="17"/>
<contactref element="J2" pad="3"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="R2" pad="2"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="DTR">
<contactref element="C1" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="31"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="30"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="32"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="2"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="9"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="10"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="11"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="23"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="24"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="25"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="26"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="27"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="28"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="12"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="13"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="14"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="R4" pad="2"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="MISO">
<contactref element="J2" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="J2" pad="4"/>
<contactref element="U1" pad="15"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="C4" pad="1"/>
<contactref element="XTAL" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$19">
<contactref element="XTAL" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$9">
</signal>
<signal name="VCC/2">
<contactref element="U2" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="J3" pad="PIN"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="N$22">
</signal>
<signal name="N$24">
</signal>
<signal name="N$25">
</signal>
<signal name="N$26">
</signal>
<signal name="N$28">
</signal>
<signal name="N$29">
</signal>
<signal name="N$27">
</signal>
<signal name="N$30">
</signal>
</signals>
</board>
</drawing>
</eagle>
