<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0.0508" y1="-0.1016" x2="27.6608" y2="0" width="0" layer="20"/>
<wire x1="27.6608" y1="0" x2="27.7116" y2="18.5574" width="0" layer="20"/>
<wire x1="27.7116" y1="18.5574" x2="0.0508" y2="18.5574" width="0" layer="20"/>
<wire x1="0.0508" y1="18.5574" x2="0" y2="17.0688" width="0" layer="20"/>
<wire x1="0.0254" y1="17.9324" x2="0" y2="17.4752" width="1.016" layer="20"/>
<wire x1="0" y1="17.4752" x2="0" y2="17.0688" width="1.016" layer="20"/>
<wire x1="0" y1="17.0688" x2="0.0508" y2="-0.1016" width="1.016" layer="20"/>
<wire x1="0.0508" y1="-0.1016" x2="27.686" y2="-0.1016" width="1.016" layer="20"/>
<wire x1="27.686" y1="-0.1016" x2="27.6606" y2="18.6436" width="1.016" layer="20"/>
<wire x1="27.6606" y1="18.6436" x2="0.0254" y2="18.6436" width="1.016" layer="20"/>
<wire x1="0.0254" y1="18.6436" x2="0" y2="17.4752" width="1.016" layer="20"/>
<circle x="24.13" y="16.4338" radius="0.209453125" width="0.4064" layer="20"/>
<circle x="24.1046" y="13.8938" radius="0.209453125" width="0.4064" layer="20"/>
<circle x="24.1046" y="11.3284" radius="0.209453125" width="0.4064" layer="20"/>
<circle x="24.1046" y="8.8138" radius="0.209453125" width="0.4064" layer="20"/>
<circle x="24.1046" y="3.7338" radius="0.209453125" width="0.4064" layer="20"/>
<circle x="24.13" y="6.2738" radius="0.209453125" width="0.4064" layer="20"/>
<circle x="24.1046" y="8.7884" radius="0.209453125" width="0.4064" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="R1206FAB">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="1X06SMD">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1uf"/>
<element name="LED1" library="fab" package="LED1206FAB" value="a     c"/>
<element name="R1" library="fab" package="R1206FAB" value="10k"/>
<element name="U$1" library="fab" package="SOIC8" value="tt45"/>
<element name="U$3" library="fab" package="2X03SMD" value="m2g"/>
<element name="U$4" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="S1" library="fab" package="6MM_SWITCH" value=""/>
<element name="R2" library="fab" package="R1206FAB" value="1k"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="8"/>
<contactref element="U$3" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U$4" pad="3"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="7"/>
<contactref element="U$3" pad="3"/>
<contactref element="U$4" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="6"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$4" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="5"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="XTAL1">
<contactref element="U$1" pad="2"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="XTAL2">
<contactref element="U$1" pad="3"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="U$3" pad="6"/>
<contactref element="U$4" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="S1" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="RST">
<contactref element="U$3" pad="5"/>
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="U$4" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="U$4" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
