<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
<text>FAB2016</text>
<text>V</text>
</plain>
<libraries>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="R1206FAB">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA08-1W">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="avr-7" package="TQFP32-08" value="MEGA48/88/168-AU"/>
<element name="R1" library="fab" package="R1206FAB" value=""/>
<element name="SV1" library="con-lstb" package="MA08-1W" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="SV3" library="con-lstb" package="MA08-1W" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="U$2" library="fab" package="2X03" value="AVRISP"/>
<element name="LED1" library="led" package="CHIPLED_1206" value=""/>
</elements>
<signals>
<signal name="AGND">
<contactref element="IC1" pad="21"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="U$2" pad="2"/>
<contactref element="SV1" pad="8"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="3"/>
<contactref element="U$2" pad="6"/>
<contactref element="SV1" pad="7"/>
</signal>
<signal name="RESET">
<contactref element="U$2" pad="5"/>
<contactref element="IC1" pad="29"/>
</signal>
<signal name="PB0">
<contactref element="SV1" pad="1"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="PB1">
<contactref element="SV1" pad="2"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="PB2">
<contactref element="SV1" pad="3"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="1"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="17"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="4"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="PD0">
<contactref element="IC1" pad="30"/>
<contactref element="SV3" pad="1"/>
</signal>
<signal name="PD1">
<contactref element="IC1" pad="31"/>
<contactref element="SV3" pad="2"/>
</signal>
<signal name="PD2">
<contactref element="IC1" pad="32"/>
<contactref element="SV3" pad="3"/>
</signal>
<signal name="PD3">
<contactref element="IC1" pad="1"/>
<contactref element="SV3" pad="4"/>
</signal>
<signal name="PD4">
<contactref element="IC1" pad="2"/>
<contactref element="SV3" pad="5"/>
</signal>
<signal name="PD5">
<contactref element="IC1" pad="9"/>
<contactref element="SV3" pad="6"/>
</signal>
<signal name="PD6">
<contactref element="IC1" pad="10"/>
<contactref element="SV3" pad="7"/>
</signal>
<signal name="PD7">
<contactref element="IC1" pad="11"/>
<contactref element="SV3" pad="8"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="PC5">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="28"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
