<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="-12.065" y1="-8.89" x2="-33.02" y2="-8.89" width="0.254" layer="20"/>
<wire x1="-33.02" y1="-8.89" x2="-34.925" y2="-6.985" width="0.254" layer="20"/>
<wire x1="-34.925" y1="-6.985" x2="-34.925" y2="14.605" width="0.254" layer="20"/>
<wire x1="-34.925" y1="14.605" x2="-33.02" y2="16.51" width="0.254" layer="20"/>
<wire x1="-12.065" y1="-8.89" x2="-10.16" y2="-6.985" width="0.254" layer="20"/>
<wire x1="-10.16" y1="-6.985" x2="-10.16" y2="14.605" width="0.254" layer="20"/>
<wire x1="-10.16" y1="14.605" x2="-12.065" y2="16.51" width="0.254" layer="20"/>
<wire x1="-12.065" y1="16.51" x2="-33.02" y2="16.51" width="0.254" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="2X02SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="fab" package="C1206" value="CAP-US1206"/>
<element name="R1" library="fab" package="R1206" value=""/>
<element name="R2" library="fab" package="R1206" value=""/>
<element name="R3" library="fab" package="R1206" value=""/>
<element name="U$1" library="fab" package="SOIC8" value="ATTINY45SI"/>
<element name="U$2" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$4" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$3" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="S1" library="fab" package="6MM_SWITCH" value=""/>
<element name="R4" library="fab" package="R1206" value=""/>
</elements>
<signals>
<signal name="RST">
<contactref element="U$1" pad="1"/>
<contactref element="U$2" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="PB3">
<contactref element="U$1" pad="2"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="PB4">
<contactref element="U$1" pad="3"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="U$2" pad="6"/>
<contactref element="U$4" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="8"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$4" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="PB2">
<contactref element="U$1" pad="7"/>
<contactref element="U$4" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="PB0">
<contactref element="U$1" pad="5"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$4" pad="3"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="PB1">
<contactref element="U$1" pad="6"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R4" pad="2"/>
<contactref element="U$3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
